# IRremoteESP8266: Member List

IRLgAc Member List

This is the complete list of members for IRLgAc, including all inherited members.

_ | IRLgAc | private
_irsend | IRLgAc | private
_protocol | IRLgAc | private
_setTemp(const uint8_t value) | IRLgAc | inlineprivate
_temp | IRLgAc | private
begin(void) | IRLgAc |
calcChecksum(const uint32_t state) | IRLgAc | static
calibrate(void) | IRLgAc | inline
checksum(void) | IRLgAc | private
convertFan(const stdAc::fanspeed_t speed) | IRLgAc | static
convertMode(const stdAc::opmode_t mode) | IRLgAc | static
getFan(void) const | IRLgAc |
getMode(void) const | IRLgAc |
getModel(void) const | IRLgAc |
getPower(void) const | IRLgAc |
getRaw(void) | IRLgAc |
getTemp(void) const | IRLgAc |
IRLgAc(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRLgAc | explicit
isValidLgAc(void) const | IRLgAc |
off(void) | IRLgAc |
on(void) | IRLgAc |
send(const uint16_t repeat=kLgDefaultRepeat) | IRLgAc |
setFan(const uint8_t speed) | IRLgAc |
setMode(const uint8_t mode) | IRLgAc |
setModel(const lg_ac_remote_model_t model) | IRLgAc |
setPower(const bool on) | IRLgAc |
setRaw(const uint32_t new_code) | IRLgAc |
setTemp(const uint8_t degrees) | IRLgAc |
stateReset(void) | IRLgAc |
toCommon(void) const | IRLgAc |
toCommonFanSpeed(const uint8_t speed) | IRLgAc | static
toCommonMode(const uint8_t mode) | IRLgAc | static
toString(void) const | IRLgAc |
validChecksum(const uint32_t state) | IRLgAc | static