# IRremoteESP8266: IRPanasonicAc32 Class Reference

IRPanasonicAc32 Class Reference

Class for handling detailed Panasonic 32bit A/C messages. More...

`#include <ir_Panasonic.h>`

Collaboration diagram for IRPanasonicAc32:
[legend]

## Public Member Functions

| IRPanasonicAc32 (const uint16_t pin, const bool inverted=false, const bool use_modulation=true)
| Class constructor. More...
void | stateReset (void)
| Reset the state of the remote to a known good state/sequence. More...
void | send (const uint16_t repeat=kPanasonicAcDefaultRepeat)
| Send the current internal state as IR messages. More...
int8_t | calibrate (void)
| Run the calibration to calculate uSec timing offsets for this platform. More...
void | begin (void)
| Set up hardware to be able to send a message. More...
void | setPowerToggle (const bool on)
| Set the Power Toggle setting of the A/C. More...
bool | getPowerToggle (void) const
| Get the Power Toggle setting of the A/C. More...
void | setTemp (const uint8_t temp)
| Set the desired temperature. More...
uint8_t | getTemp (void) const
| Get the current desired temperature setting. More...
void | setFan (const uint8_t fan)
| Set the speed of the fan. More...
uint8_t | getFan (void) const
| Get the current fan speed setting. More...
void | setMode (const uint8_t mode)
| Set the operating mode of the A/C. More...
uint8_t | getMode (void) const
| Get the operating mode setting of the A/C. More...
void | setRaw (const uint32_t state)
| Set the internal state from a valid code for this protocol. More...
uint32_t | getRaw (void) const
| Get a copy of the internal state/code for this protocol. More...
void | setSwingVertical (const uint8_t pos)
| Control the vertical swing setting. More...
uint8_t | getSwingVertical (void) const
| Get the current vertical swing setting. More...
void | setSwingHorizontal (const bool on)
| Control the horizontal swing setting. More...
bool | getSwingHorizontal (void) const
| Get the current horizontal swing setting. More...
stdAc::state_t | toCommon (const stdAc::state_t *prev=NULL) const
| Convert the current internal state into its stdAc::state_t equivalent. More...
String | toString (void) const
| Convert the current internal state into a human readable string. More...

## Static Public Member Functions

static uint8_t | convertMode (const stdAc::opmode_t mode)
| Convert a stdAc::opmode_t enum into its native mode. More...
static uint8_t | convertFan (const stdAc::fanspeed_t speed)
| Convert a stdAc::fanspeed_t enum into it's native speed. More...
static uint8_t | convertSwingV (const stdAc::swingv_t position)
| Convert a standard A/C vertical swing into its native setting. More...
static stdAc::opmode_t | toCommonMode (const uint8_t mode)
| Convert a native mode into its stdAc equivalent. More...
static stdAc::fanspeed_t | toCommonFanSpeed (const uint8_t speed)
| Convert a native fan speed into its stdAc equivalent. More...
static stdAc::swingv_t | toCommonSwingV (const uint8_t pos)
| Convert a native vertical swing postion to it's common equivalent. More...

## Private Attributes

IRsend | _irsend
| Instance of the IR send class. More...
PanasonicAc32Protocol | _
| The state in code form. More...

## Detailed Description

Class for handling detailed Panasonic 32bit A/C messages.

## Constructor & Destructor Documentation

## IRPanasonicAc32()

IRPanasonicAc32::IRPanasonicAc32 | ( | const uint16_t | pin,
|  | const bool | inverted = `false`,
|  | const bool | use_modulation = `true`
| ) |  |

explicit

Class constructor.

Parameters

  [in] | pin | GPIO to be used when sending.
  [in] | inverted | Is the output signal to be inverted?
  [in] | use_modulation | Is frequency modulation to be used?

## Member Function Documentation

## begin()

void IRPanasonicAc32::begin | ( | void |  | ) |

Set up hardware to be able to send a message.

## calibrate()

int8_t IRPanasonicAc32::calibrate | ( | void |  | ) |

inline

Run the calibration to calculate uSec timing offsets for this platform.

Returns
  The uSec timing offset needed per modulation of the IR Led.

Note
  This will produce a 65ms IR signal pulse at 38kHz. Only ever needs to be run once per object instantiation, if at all.

## convertFan()

uint8_t IRPanasonicAc32::convertFan | ( | const stdAc::fanspeed_t | speed | ) |

static

Convert a stdAc::fanspeed_t enum into it's native speed.

Parameters

  [in] | speed | The enum to be converted.

Returns
  The native equivalent of the enum.

## convertMode()

uint8_t IRPanasonicAc32::convertMode | ( | const stdAc::opmode_t | mode | ) |

static

Convert a stdAc::opmode_t enum into its native mode.

Parameters

  [in] | mode | The enum to be converted.

Returns
  The native equivalent of the enum.

## convertSwingV()

uint8_t IRPanasonicAc32::convertSwingV | ( | const stdAc::swingv_t | position | ) |

static

Convert a standard A/C vertical swing into its native setting.

Parameters

  [in] | position | A stdAc::swingv_t position to convert.

Returns
  The equivalent native horizontal swing position.

## getFan()

uint8_t IRPanasonicAc32::getFan | ( | void |  | ) | const

Get the current fan speed setting.

Returns
  The current fan speed.

## getMode()

uint8_t IRPanasonicAc32::getMode | ( | void |  | ) | const

Get the operating mode setting of the A/C.

Returns
  The current operating mode setting.

## getPowerToggle()

bool IRPanasonicAc32::getPowerToggle | ( | void |  | ) | const

Get the Power Toggle setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## getRaw()

uint32_t IRPanasonicAc32::getRaw | ( | void |  | ) | const

Get a copy of the internal state/code for this protocol.

Returns
  The code for this protocol based on the current internal state.

## getSwingHorizontal()

bool IRPanasonicAc32::getSwingHorizontal | ( | void |  | ) | const

Get the current horizontal swing setting.

Returns
  The current position it is set to.

## getSwingVertical()

uint8_t IRPanasonicAc32::getSwingVertical | ( | void |  | ) | const

Get the current vertical swing setting.

Returns
  The current position it is set to.

## getTemp()

uint8_t IRPanasonicAc32::getTemp | ( | void |  | ) | const

Get the current desired temperature setting.

Returns
  The current setting for temp. in degrees celsius.

## send()

void IRPanasonicAc32::send | ( | const uint16_t | repeat = `kPanasonicAcDefaultRepeat` | ) |

Send the current internal state as IR messages.

Parameters

  [in] | repeat | Nr. of times the message will be repeated.

## setFan()

void IRPanasonicAc32::setFan | ( | const uint8_t | speed | ) |

Set the speed of the fan.

Parameters

  [in] | speed | The desired setting.

## setMode()

void IRPanasonicAc32::setMode | ( | const uint8_t | mode | ) |

Set the operating mode of the A/C.

Parameters

  [in] | mode | The desired operating mode.

Note
  If we get an unexpected mode, default to AUTO.

## setPowerToggle()

void IRPanasonicAc32::setPowerToggle | ( | const bool | on | ) |

Set the Power Toggle setting of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## setRaw()

void IRPanasonicAc32::setRaw | ( | const uint32_t | state | ) |

Set the internal state from a valid code for this protocol.

Parameters

  [in] | state | A valid code for this protocol.

## setSwingHorizontal()

void IRPanasonicAc32::setSwingHorizontal | ( | const bool | on | ) |

Control the horizontal swing setting.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## setSwingVertical()

void IRPanasonicAc32::setSwingVertical | ( | const uint8_t | pos | ) |

Control the vertical swing setting.

Parameters

  [in] | pos | The position to set the vertical swing to.

## setTemp()

void IRPanasonicAc32::setTemp | ( | const uint8_t | degrees | ) |

Set the desired temperature.

Parameters

  [in] | degrees | The temperature in degrees celsius.

## stateReset()

void IRPanasonicAc32::stateReset | ( | void |  | ) |

Reset the state of the remote to a known good state/sequence.

## toCommon()

stdAc::state_t IRPanasonicAc32::toCommon | ( | const stdAc::state_t * | prev = `NULL` | ) | const

Convert the current internal state into its stdAc::state_t equivalent.

Parameters

  [in] | prev | Ptr to the previous state if required.

Returns
  The stdAc equivalent of the native settings.

## toCommonFanSpeed()

stdAc::fanspeed_t IRPanasonicAc32::toCommonFanSpeed | ( | const uint8_t | spd | ) |

static

Convert a native fan speed into its stdAc equivalent.

Parameters

  [in] | spd | The native setting to be converted.

Returns
  The stdAc equivalent of the native setting.

## toCommonMode()

stdAc::opmode_t IRPanasonicAc32::toCommonMode | ( | const uint8_t | mode | ) |

static

Convert a native mode into its stdAc equivalent.

Parameters

  [in] | mode | The native setting to be converted.

Returns
  The stdAc equivalent of the native setting.

## toCommonSwingV()

stdAc::swingv_t IRPanasonicAc32::toCommonSwingV | ( | const uint8_t | pos | ) |

static

Convert a native vertical swing postion to it's common equivalent.

Parameters

  [in] | pos | A native position to convert.

Returns
  The common vertical swing position.

## toString()

String IRPanasonicAc32::toString | ( | void |  | ) | const

Convert the current internal state into a human readable string.

Returns
  A human readable string.

## Member Data Documentation

## _

PanasonicAc32Protocol IRPanasonicAc32::_

private

The state in code form.

## _irsend

IRsend IRPanasonicAc32::_irsend

private

Instance of the IR send class.

The documentation for this class was generated from the following files:

- src/ir_Panasonic.h
- src/ir_Panasonic.cpp