# IRremoteESP8266: ArgoProtocol Union Reference

ArgoProtocol Union Reference

Native representation of a Argo A/C message. More...

`#include <ir_Argo.h>`

## Public Attributes

uint8_t | raw [kArgoStateLength]
| The state in native IR code form. More...
struct {
uint64_t __pad0__:8
uint64_t __pad1__:8
uint64_t __pad2__:3
uint64_t Mode:3
uint64_t Temp:5
uint64_t Fan:2
uint64_t RoomTemp:5
uint64_t Flap:3
uint64_t __pad3__:3
uint64_t __pad4__:8
uint64_t __pad5__:8
uint64_t __pad6__:3
uint64_t __pad7__:5
uint32_t __pad8__:6
uint32_t __pad9__:1
uint32_t __pad10__:1
uint32_t __pad11__:1
uint32_t __pad12__:1
uint32_t Night:1
uint32_t Max:1
uint32_t __pad13__:1
uint32_t Power:1
uint32_t __pad14__:1
uint32_t iFeel:1
uint32_t __pad15__:2
uint32_t Sum:8
uint32_t __pad16__:6
}; |

## Detailed Description

Native representation of a Argo A/C message.

## Member Data Documentation

## @5

struct { ... }

## __pad0__

uint64_t ArgoProtocol::__pad0__

## __pad10__

uint32_t ArgoProtocol::__pad10__

## __pad11__

uint32_t ArgoProtocol::__pad11__

## __pad12__

uint32_t ArgoProtocol::__pad12__

## __pad13__

uint32_t ArgoProtocol::__pad13__

## __pad14__

uint32_t ArgoProtocol::__pad14__

## __pad15__

uint32_t ArgoProtocol::__pad15__

## __pad16__

uint32_t ArgoProtocol::__pad16__

## __pad1__

uint64_t ArgoProtocol::__pad1__

## __pad2__

uint64_t ArgoProtocol::__pad2__

## __pad3__

uint64_t ArgoProtocol::__pad3__

## __pad4__

uint64_t ArgoProtocol::__pad4__

## __pad5__

uint64_t ArgoProtocol::__pad5__

## __pad6__

uint64_t ArgoProtocol::__pad6__

## __pad7__

uint64_t ArgoProtocol::__pad7__

## __pad8__

uint32_t ArgoProtocol::__pad8__

## __pad9__

uint32_t ArgoProtocol::__pad9__

## Fan

uint64_t ArgoProtocol::Fan

## Flap

uint64_t ArgoProtocol::Flap

## iFeel

uint32_t ArgoProtocol::iFeel

## Max

uint32_t ArgoProtocol::Max

## Mode

uint64_t ArgoProtocol::Mode

## Night

uint32_t ArgoProtocol::Night

## Power

uint32_t ArgoProtocol::Power

## raw

uint8_t ArgoProtocol::raw[kArgoStateLength]

The state in native IR code form.

## RoomTemp

uint64_t ArgoProtocol::RoomTemp

## Sum

uint32_t ArgoProtocol::Sum

## Temp

uint64_t ArgoProtocol::Temp

The documentation for this union was generated from the following file:

- src/ir_Argo.h