# IRremoteESP8266: IRAmcorAc Class Reference

IRAmcorAc Class Reference

Class for handling detailed Amcor A/C messages. More...

`#include <ir_Amcor.h>`

Collaboration diagram for IRAmcorAc:
[legend]

## Public Member Functions

| IRAmcorAc (const uint16_t pin, const bool inverted=false, const bool use_modulation=true)
| Class constructor. More...
void | stateReset ()
| Reset the internals of the object to a known good state. More...
void | send (const uint16_t repeat=kAmcorDefaultRepeat)
| Send the current internal state as an IR message. More...
int8_t | calibrate (void)
| Run the calibration to calculate uSec timing offsets for this platform. More...
void | begin ()
| Set up hardware to be able to send a message. More...
void | setPower (const bool state)
| Set the internal state to have the desired power. More...
bool | getPower (void) const
| Get the power setting from the internal state. More...
void | on (void)
| Set the internal state to have the power on. More...
void | off (void)
| Set the internal state to have the power off. More...
void | setTemp (const uint8_t temp)
| Set the temperature. More...
uint8_t | getTemp (void) const
| Get the current temperature setting. More...
void | setMax (const bool on)
| Control the current Maximum Cooling or Heating setting. (i.e. Turbo) More...
bool | getMax (void) const
| Is the Maximum Cooling or Heating setting (i.e. Turbo) setting on? More...
void | setFan (const uint8_t speed)
| Set the speed of the fan. More...
uint8_t | getFan (void) const
| Get the current fan speed setting. More...
void | setMode (const uint8_t mode)
| Set the desired operation mode. More...
uint8_t | getMode (void) const
| Get the current operation mode setting. More...
uint8_t * | getRaw (void)
| Get the raw state of the object, suitable to be sent with the appropriate IRsend object method. More...
void | setRaw (const uint8_t state[])
| Set the raw state of the object. More...
stdAc::state_t | toCommon (void) const
| Convert the current internal state into its stdAc::state_t equivalent. More...
String | toString (void) const
| Convert the current internal state into a human readable string. More...

## Static Public Member Functions

static uint8_t | calcChecksum (const uint8_t state[], const uint16_t length=kAmcorStateLength)
| Calculate the checksum for the supplied state. More...
static bool | validChecksum (const uint8_t state[], const uint16_t length=kAmcorStateLength)
| Verify the checksum is valid for a given state. More...
static uint8_t | convertMode (const stdAc::opmode_t mode)
| Convert a stdAc::opmode_t enum into its native mode. More...
static uint8_t | convertFan (const stdAc::fanspeed_t speed)
| Convert a stdAc::fanspeed_t enum into it's native speed. More...
static stdAc::opmode_t | toCommonMode (const uint8_t mode)
| Convert a native mode into its stdAc equivalent. More...
static stdAc::fanspeed_t | toCommonFanSpeed (const uint8_t speed)
| Convert a native fan speed into its stdAc equivalent. More...

## Private Member Functions

void | checksum (void)
| Update the checksum value for the internal state. More...

## Private Attributes

IRsend | _irsend
AmcorProtocol | _

## Detailed Description

Class for handling detailed Amcor A/C messages.

## Constructor & Destructor Documentation

## IRAmcorAc()

IRAmcorAc::IRAmcorAc | ( | const uint16_t | pin,
|  | const bool | inverted = `false`,
|  | const bool | use_modulation = `true`
| ) |  |

explicit

Class constructor.

Parameters

  [in] | pin | GPIO to be used when sending.
  [in] | inverted | Is the output signal to be inverted?
  [in] | use_modulation | Is frequency modulation to be used?

## Member Function Documentation

## begin()

void IRAmcorAc::begin | ( |  | ) |

Set up hardware to be able to send a message.

## calcChecksum()

uint8_t IRAmcorAc::calcChecksum | ( | const uint8_t | state[],
|  | const uint16_t | length = `kAmcorStateLength`
| ) |  |

static

Calculate the checksum for the supplied state.

Parameters

  [in] | state | The source state to generate the checksum from.
  [in] | length | Length of the supplied state to checksum.

Returns
  The checksum value.

## calibrate()

int8_t IRAmcorAc::calibrate | ( | void |  | ) |

inline

Run the calibration to calculate uSec timing offsets for this platform.

Returns
  The uSec timing offset needed per modulation of the IR Led.

Note
  This will produce a 65ms IR signal pulse at 38kHz. Only ever needs to be run once per object instantiation, if at all.

## checksum()

void IRAmcorAc::checksum | ( | void |  | ) |

private

Update the checksum value for the internal state.

## convertFan()

uint8_t IRAmcorAc::convertFan | ( | const stdAc::fanspeed_t | speed | ) |

static

Convert a stdAc::fanspeed_t enum into it's native speed.

Parameters

  [in] | speed | The enum to be converted.

Returns
  The native equivalent of the enum.

## convertMode()

uint8_t IRAmcorAc::convertMode | ( | const stdAc::opmode_t | mode | ) |

static

Convert a stdAc::opmode_t enum into its native mode.

Parameters

  [in] | mode | The enum to be converted.

Returns
  The native equivalent of the enum.

## getFan()

uint8_t IRAmcorAc::getFan | ( | void |  | ) | const

Get the current fan speed setting.

Returns
  The current fan speed.

## getMax()

bool IRAmcorAc::getMax | ( | void |  | ) | const

Is the Maximum Cooling or Heating setting (i.e. Turbo) setting on?

Returns
  The current value.

## getMode()

uint8_t IRAmcorAc::getMode | ( | void |  | ) | const

Get the current operation mode setting.

Returns
  The current operation mode.

## getPower()

bool IRAmcorAc::getPower | ( | void |  | ) | const

Get the power setting from the internal state.

Returns
  A boolean indicating the power setting.

## getRaw()

uint8_t * IRAmcorAc::getRaw | ( | void |  | ) |

Get the raw state of the object, suitable to be sent with the appropriate IRsend object method.

Returns
  A PTR to the internal state.

## getTemp()

uint8_t IRAmcorAc::getTemp | ( | void |  | ) | const

Get the current temperature setting.

Returns
  Get current setting for temp. in degrees celsius.

## off()

void IRAmcorAc::off | ( | void |  | ) |

Set the internal state to have the power off.

## on()

void IRAmcorAc::on | ( | void |  | ) |

Set the internal state to have the power on.

## send()

void IRAmcorAc::send | ( | const uint16_t | repeat = `kAmcorDefaultRepeat` | ) |

Send the current internal state as an IR message.

Parameters

  [in] | repeat | Nr. of times the message will be repeated.

## setFan()

void IRAmcorAc::setFan | ( | const uint8_t | speed | ) |

Set the speed of the fan.

Parameters

  [in] | speed | The desired setting.

## setMax()

void IRAmcorAc::setMax | ( | const bool | on | ) |

Control the current Maximum Cooling or Heating setting. (i.e. Turbo)

Note
  Only allowed in Cool or Heat mode.

Parameters

  [in] | on | The desired setting.

## setMode()

void IRAmcorAc::setMode | ( | const uint8_t | mode | ) |

Set the desired operation mode.

Parameters

  [in] | mode | The desired operation mode.

## setPower()

void IRAmcorAc::setPower | ( | const bool | on | ) |

Set the internal state to have the desired power.

Parameters

  [in] | on | The desired power state.

## setRaw()

void IRAmcorAc::setRaw | ( | const uint8_t | state[] | ) |

Set the raw state of the object.

Parameters

  [in] | state | The raw state from the native IR message.

## setTemp()

void IRAmcorAc::setTemp | ( | const uint8_t | degrees | ) |

Set the temperature.

Parameters

  [in] | degrees | The temperature in degrees celsius.

## stateReset()

void IRAmcorAc::stateReset | ( |  | ) |

Reset the internals of the object to a known good state.

## toCommon()

stdAc::state_t IRAmcorAc::toCommon | ( | void |  | ) | const

Convert the current internal state into its stdAc::state_t equivalent.

Returns
  The stdAc equivalent of the native settings.

## toCommonFanSpeed()

stdAc::fanspeed_t IRAmcorAc::toCommonFanSpeed | ( | const uint8_t | speed | ) |

static

Convert a native fan speed into its stdAc equivalent.

Parameters

  [in] | speed | The native setting to be converted.

Returns
  The stdAc equivalent of the native setting.

## toCommonMode()

stdAc::opmode_t IRAmcorAc::toCommonMode | ( | const uint8_t | mode | ) |

static

Convert a native mode into its stdAc equivalent.

Parameters

  [in] | mode | The native setting to be converted.

Returns
  The stdAc equivalent of the native setting.

## toString()

String IRAmcorAc::toString | ( | void |  | ) | const

Convert the current internal state into a human readable string.

Returns
  A human readable string.

## validChecksum()

bool IRAmcorAc::validChecksum | ( | const uint8_t | state[],
|  | const uint16_t | length = `kAmcorStateLength`
| ) |  |

static

Verify the checksum is valid for a given state.

Parameters

  [in] | state | The array to verify the checksum of.
  [in] | length | The size of the state.

Returns
  A boolean indicating if it's checksum is valid.

## Member Data Documentation

## _

AmcorProtocol IRAmcorAc::_

private

## _irsend

IRsend IRAmcorAc::_irsend

private

The documentation for this class was generated from the following files:

- src/ir_Amcor.h
- src/ir_Amcor.cpp