# IRremoteESP8266: Member List

IRHaierACYRW02 Member List

This is the complete list of members for IRHaierACYRW02, including all inherited members.

_ | IRHaierACYRW02 | private
_irsend | IRHaierACYRW02 | private
begin(void) | IRHaierACYRW02 |
calibrate(void) | IRHaierACYRW02 | inline
checksum(void) | IRHaierACYRW02 | private
convertFan(const stdAc::fanspeed_t speed) | IRHaierACYRW02 | static
convertMode(const stdAc::opmode_t mode) | IRHaierACYRW02 | static
convertSwingV(const stdAc::swingv_t position) | IRHaierACYRW02 | static
getButton(void) const | IRHaierACYRW02 |
getFan(void) const | IRHaierACYRW02 |
getHealth(void) const | IRHaierACYRW02 |
getMode(void) const | IRHaierACYRW02 |
getPower(void) const | IRHaierACYRW02 |
getRaw(void) | IRHaierACYRW02 |
getSleep(void) const | IRHaierACYRW02 |
getSwing(void) const | IRHaierACYRW02 |
getTemp(void) const | IRHaierACYRW02 |
getTurbo(void) const | IRHaierACYRW02 |
IRHaierACYRW02(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRHaierACYRW02 | explicit
off(void) | IRHaierACYRW02 |
on(void) | IRHaierACYRW02 |
send(const uint16_t repeat=kHaierAcYrw02DefaultRepeat) | IRHaierACYRW02 |
setButton(const uint8_t button) | IRHaierACYRW02 |
setFan(const uint8_t speed) | IRHaierACYRW02 |
setHealth(const bool on) | IRHaierACYRW02 |
setMode(const uint8_t mode) | IRHaierACYRW02 |
setPower(const bool on) | IRHaierACYRW02 |
setRaw(const uint8_t new_code[]) | IRHaierACYRW02 |
setSleep(const bool on) | IRHaierACYRW02 |
setSwing(const uint8_t pos) | IRHaierACYRW02 |
setTemp(const uint8_t temp) | IRHaierACYRW02 |
setTurbo(const uint8_t speed) | IRHaierACYRW02 |
stateReset(void) | IRHaierACYRW02 | private
toCommon(void) const | IRHaierACYRW02 |
toCommonFanSpeed(const uint8_t speed) | IRHaierACYRW02 | static
toCommonMode(const uint8_t mode) | IRHaierACYRW02 | static
toCommonSwingV(const uint8_t pos) | IRHaierACYRW02 | static
toString(void) const | IRHaierACYRW02 |
validChecksum(uint8_t state[], const uint16_t length=kHaierACYRW02StateLength) | IRHaierACYRW02 | static