# IRremoteESP8266: Member List

IRGoodweatherAc Member List

This is the complete list of members for IRGoodweatherAc, including all inherited members.

_ | IRGoodweatherAc | private
_irsend | IRGoodweatherAc | private
begin(void) | IRGoodweatherAc |
calibrate(void) | IRGoodweatherAc | inline
convertFan(const stdAc::fanspeed_t speed) | IRGoodweatherAc | static
convertMode(const stdAc::opmode_t mode) | IRGoodweatherAc | static
convertSwingV(const stdAc::swingv_t swingv) | IRGoodweatherAc | static
getCommand(void) const | IRGoodweatherAc |
getFan(void) const | IRGoodweatherAc |
getLight(void) const | IRGoodweatherAc |
getMode(void) const | IRGoodweatherAc |
getPower(void) const | IRGoodweatherAc |
getRaw(void) | IRGoodweatherAc |
getSleep(void) const | IRGoodweatherAc |
getSwing(void) const | IRGoodweatherAc |
getTemp(void) const | IRGoodweatherAc |
getTurbo(void) const | IRGoodweatherAc |
IRGoodweatherAc(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRGoodweatherAc | explicit
off(void) | IRGoodweatherAc |
on(void) | IRGoodweatherAc |
send(const uint16_t repeat=kGoodweatherMinRepeat) | IRGoodweatherAc |
setCommand(const uint8_t cmd) | IRGoodweatherAc |
setFan(const uint8_t speed) | IRGoodweatherAc |
setLight(const bool toggle) | IRGoodweatherAc |
setMode(const uint8_t mode) | IRGoodweatherAc |
setPower(const bool on) | IRGoodweatherAc |
setRaw(const uint64_t state) | IRGoodweatherAc |
setSleep(const bool toggle) | IRGoodweatherAc |
setSwing(const uint8_t speed) | IRGoodweatherAc |
setTemp(const uint8_t temp) | IRGoodweatherAc |
setTurbo(const bool toggle) | IRGoodweatherAc |
stateReset(void) | IRGoodweatherAc |
toCommon(void) const | IRGoodweatherAc |
toCommonFanSpeed(const uint8_t speed) | IRGoodweatherAc | static
toCommonMode(const uint8_t mode) | IRGoodweatherAc | static
toString(void) const | IRGoodweatherAc |