# IRremoteESP8266: Member List

IRHitachiAc Member List

This is the complete list of members for IRHitachiAc, including all inherited members.

_ | IRHitachiAc | private
_irsend | IRHitachiAc | private
_previoustemp | IRHitachiAc | private
begin(void) | IRHitachiAc |
calcChecksum(const uint8_t state[], const uint16_t length=kHitachiAcStateLength) | IRHitachiAc | static
calibrate(void) | IRHitachiAc | inline
checksum(const uint16_t length=kHitachiAcStateLength) | IRHitachiAc | private
convertFan(const stdAc::fanspeed_t speed) | IRHitachiAc | static
convertMode(const stdAc::opmode_t mode) | IRHitachiAc | static
getFan(void) const | IRHitachiAc |
getMode(void) const | IRHitachiAc |
getPower(void) const | IRHitachiAc |
getRaw(void) | IRHitachiAc |
getSwingHorizontal(void) const | IRHitachiAc |
getSwingVertical(void) const | IRHitachiAc |
getTemp(void) const | IRHitachiAc |
IRHitachiAc(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRHitachiAc | explicit
off(void) | IRHitachiAc |
on(void) | IRHitachiAc |
send(const uint16_t repeat=kHitachiAcDefaultRepeat) | IRHitachiAc |
setFan(const uint8_t speed) | IRHitachiAc |
setMode(const uint8_t mode) | IRHitachiAc |
setPower(const bool on) | IRHitachiAc |
setRaw(const uint8_t new_code[], const uint16_t length=kHitachiAcStateLength) | IRHitachiAc |
setSwingHorizontal(const bool on) | IRHitachiAc |
setSwingVertical(const bool on) | IRHitachiAc |
setTemp(const uint8_t temp) | IRHitachiAc |
stateReset(void) | IRHitachiAc |
toCommon(void) const | IRHitachiAc |
toCommonFanSpeed(const uint8_t speed) | IRHitachiAc | static
toCommonMode(const uint8_t mode) | IRHitachiAc | static
toString(void) const | IRHitachiAc |
validChecksum(const uint8_t state[], const uint16_t length=kHitachiAcStateLength) | IRHitachiAc | static