# IRremoteESP8266: IRNeoclimaAc Class Reference

IRNeoclimaAc Class Reference

Class for handling detailed Neoclima A/C messages. More...

`#include <ir_Neoclima.h>`

Collaboration diagram for IRNeoclimaAc:
[legend]

## Public Member Functions

| IRNeoclimaAc (const uint16_t pin, const bool inverted=false, const bool use_modulation=true)
| Class constructor. More...
void | stateReset (void)
| Reset the state of the remote to a known good state/sequence. More...
void | send (const uint16_t repeat=kNeoclimaMinRepeat)
| Send the current internal state as an IR message. More...
int8_t | calibrate (void)
| Run the calibration to calculate uSec timing offsets for this platform. More...
void | begin (void)
| Set up hardware to be able to send a message. More...
void | setButton (const uint8_t button)
| Set the Button/Command pressed setting of the A/C. More...
uint8_t | getButton (void) const
| Get the Button/Command setting of the A/C. More...
void | on (void)
| Set the requested power state of the A/C to on. More...
void | off (void)
| Set the requested power state of the A/C to off. More...
void | setPower (const bool on)
| Change the power setting. More...
bool | getPower (void) const
| Get the value of the current power setting. More...
void | setMode (const uint8_t mode)
| Set the operating mode of the A/C. More...
uint8_t | getMode (void) const
| Get the operating mode setting of the A/C. More...
void | setTemp (const uint8_t temp, const bool celsius=true)
| Set the temperature. More...
uint8_t | getTemp (void) const
| Get the current temperature setting. More...
void | setFan (const uint8_t speed)
| Set the speed of the fan. More...
uint8_t | getFan (void) const
| Get the current fan speed setting. More...
void | setSwingV (const bool on)
| Set the vertical swing setting of the A/C. More...
bool | getSwingV (void) const
| Get the vertical swing setting of the A/C. More...
void | setSwingH (const bool on)
| Set the horizontal swing setting of the A/C. More...
bool | getSwingH (void) const
| Get the horizontal swing (Air Flow) setting of the A/C. More...
void | setSleep (const bool on)
| Set the Sleep setting of the A/C. More...
bool | getSleep (void) const
| Get the Sleep setting of the A/C. More...
void | setTurbo (const bool on)
| Set the Turbo setting of the A/C. More...
bool | getTurbo (void) const
| Get the Turbo setting of the A/C. More...
void | setEcono (const bool on)
| Set the Economy (Energy Saver) setting of the A/C. More...
bool | getEcono (void) const
| Get the Economy (Energy Saver) setting of the A/C. More...
void | setFresh (const bool on)
| Set the Fresh (air) setting of the A/C. More...
bool | getFresh (void) const
| Get the Fresh (air) setting of the A/C. More...
void | setHold (const bool on)
| Set the Hold setting of the A/C. More...
bool | getHold (void) const
| Get the Hold setting of the A/C. More...
void | setIon (const bool on)
| Set the Ion (filter) setting of the A/C. More...
bool | getIon (void) const
| Get the Ion (filter) setting of the A/C. More...
void | setLight (const bool on)
| Set the Light(LED display) setting of the A/C. More...
bool | getLight (void) const
| Get the Light (LED display) setting of the A/C. More...
void | set8CHeat (const bool on)
| Set the 8°C Heat setting of the A/C. More...
bool | get8CHeat (void) const
| Get the 8°C Heat setting of the A/C. More...
void | setEye (const bool on)
| Set the Eye (Sensor) setting of the A/C. More...
bool | getEye (void) const
| Get the Eye (Sensor) setting of the A/C. More...
bool | getTempUnits (void) const
| Is the A/C unit using Fahrenheit or Celsius for temperature units. More...
bool | getFollow (void) const
| Get the Follow Me setting of the A/C. More...
uint8_t * | getRaw (void)
| Get a PTR to the internal state/code for this protocol. More...
void | setRaw (const uint8_t new_code[], const uint16_t length=kNeoclimaStateLength)
| Set the internal state from a valid code for this protocol. More...
String | toString (void) const
| Convert the current internal state into a human readable string. More...
stdAc::state_t | toCommon (void) const
| Convert the current internal state into its stdAc::state_t equivalent. More...

## Static Public Member Functions

static bool | validChecksum (const uint8_t state[], const uint16_t length=kNeoclimaStateLength)
| Verify the checksum is valid for a given state. More...
static uint8_t | calcChecksum (const uint8_t state[], const uint16_t length=kNeoclimaStateLength)
| Calculate the checksum for a given state. More...
static uint8_t | convertMode (const stdAc::opmode_t mode)
| Convert a stdAc::opmode_t enum into its native mode. More...
static uint8_t | convertFan (const stdAc::fanspeed_t speed)
| Convert a stdAc::fanspeed_t enum into it's native speed. More...
static stdAc::opmode_t | toCommonMode (const uint8_t mode)
| Convert a native mode into its stdAc equivalent. More...
static stdAc::fanspeed_t | toCommonFanSpeed (const uint8_t speed)
| Convert a native fan speed into its stdAc equivalent. More...

## Private Member Functions

void | checksum (const uint16_t length=kNeoclimaStateLength)
| Calculate & update the checksum for the internal state. More...

## Private Attributes

IRsend | _irsend
| Instance of the IR send class. More...
NeoclimaProtocol | _

## Detailed Description

Class for handling detailed Neoclima A/C messages.

## Constructor & Destructor Documentation

## IRNeoclimaAc()

IRNeoclimaAc::IRNeoclimaAc | ( | const uint16_t | pin,
|  | const bool | inverted = `false`,
|  | const bool | use_modulation = `true`
| ) |  |

explicit

Class constructor.

Parameters

  [in] | pin | GPIO to be used when sending.
  [in] | inverted | Is the output signal to be inverted?
  [in] | use_modulation | Is frequency modulation to be used?

## Member Function Documentation

## begin()

void IRNeoclimaAc::begin | ( | void |  | ) |

Set up hardware to be able to send a message.

## calcChecksum()

uint8_t IRNeoclimaAc::calcChecksum | ( | const uint8_t | state[],
|  | const uint16_t | length = `kNeoclimaStateLength`
| ) |  |

static

Calculate the checksum for a given state.

Parameters

  [in] | state | The array to calc the checksum of.
  [in] | length | The length/size of the array.

Returns
  The calculated checksum value.

## calibrate()

int8_t IRNeoclimaAc::calibrate | ( | void |  | ) |

inline

Run the calibration to calculate uSec timing offsets for this platform.

Returns
  The uSec timing offset needed per modulation of the IR Led.

Note
  This will produce a 65ms IR signal pulse at 38kHz. Only ever needs to be run once per object instantiation, if at all.

## checksum()

void IRNeoclimaAc::checksum | ( | const uint16_t | length = `kNeoclimaStateLength` | ) |

private

Calculate & update the checksum for the internal state.

Parameters

  [in] | length | The length/size of the internal state.

## convertFan()

uint8_t IRNeoclimaAc::convertFan | ( | const stdAc::fanspeed_t | speed | ) |

static

Convert a stdAc::fanspeed_t enum into it's native speed.

Parameters

  [in] | speed | The enum to be converted.

Returns
  The native equivalent of the enum.

## convertMode()

uint8_t IRNeoclimaAc::convertMode | ( | const stdAc::opmode_t | mode | ) |

static

Convert a stdAc::opmode_t enum into its native mode.

Parameters

  [in] | mode | The enum to be converted.

Returns
  The native equivalent of the enum.

## get8CHeat()

bool IRNeoclimaAc::get8CHeat | ( | void |  | ) | const

Get the 8°C Heat setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## getButton()

uint8_t IRNeoclimaAc::getButton | ( | void |  | ) | const

Get the Button/Command setting of the A/C.

Returns
  The value of the button/command that was pressed.

## getEcono()

bool IRNeoclimaAc::getEcono | ( | void |  | ) | const

Get the Economy (Energy Saver) setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## getEye()

bool IRNeoclimaAc::getEye | ( | void |  | ) | const

Get the Eye (Sensor) setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## getFan()

uint8_t IRNeoclimaAc::getFan | ( | void |  | ) | const

Get the current fan speed setting.

Returns
  The current fan speed/mode.

## getFollow()

bool IRNeoclimaAc::getFollow | ( | void |  | ) | const

Get the Follow Me setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## getFresh()

bool IRNeoclimaAc::getFresh | ( | void |  | ) | const

Get the Fresh (air) setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## getHold()

bool IRNeoclimaAc::getHold | ( | void |  | ) | const

Get the Hold setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## getIon()

bool IRNeoclimaAc::getIon | ( | void |  | ) | const

Get the Ion (filter) setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## getLight()

bool IRNeoclimaAc::getLight | ( | void |  | ) | const

Get the Light (LED display) setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## getMode()

uint8_t IRNeoclimaAc::getMode | ( | void |  | ) | const

Get the operating mode setting of the A/C.

Returns
  The current operating mode setting.

## getPower()

bool IRNeoclimaAc::getPower | ( | void |  | ) | const

Get the value of the current power setting.

Returns
  true, the setting is on. false, the setting is off.

## getRaw()

uint8_t * IRNeoclimaAc::getRaw | ( | void |  | ) |

Get a PTR to the internal state/code for this protocol.

Returns
  PTR to a code for this protocol based on the current internal state.

## getSleep()

bool IRNeoclimaAc::getSleep | ( | void |  | ) | const

Get the Sleep setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## getSwingH()

bool IRNeoclimaAc::getSwingH | ( | void |  | ) | const

Get the horizontal swing (Air Flow) setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## getSwingV()

bool IRNeoclimaAc::getSwingV | ( | void |  | ) | const

Get the vertical swing setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## getTemp()

uint8_t IRNeoclimaAc::getTemp | ( | void |  | ) | const

Get the current temperature setting.

Returns
  The current setting for temp. in degrees.

Note
  The units of the temperature (F/C) is determined by `getTempUnits()`.

## getTempUnits()

bool IRNeoclimaAc::getTempUnits | ( | void |  | ) | const

Is the A/C unit using Fahrenheit or Celsius for temperature units.

Returns
  false, Fahrenheit. true, Celsius.

## getTurbo()

bool IRNeoclimaAc::getTurbo | ( | void |  | ) | const

Get the Turbo setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## off()

void IRNeoclimaAc::off | ( | void |  | ) |

Set the requested power state of the A/C to off.

## on()

void IRNeoclimaAc::on | ( | void |  | ) |

Set the requested power state of the A/C to on.

## send()

void IRNeoclimaAc::send | ( | const uint16_t | repeat = `kNeoclimaMinRepeat` | ) |

Send the current internal state as an IR message.

Parameters

  [in] | repeat | Nr. of times the message will be repeated.

## set8CHeat()

void IRNeoclimaAc::set8CHeat | ( | const bool | on | ) |

Set the 8°C Heat setting of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

Note
  This feature maintains the room temperature steadily at 8°C and prevents the room from freezing by activating the heating operation automatically when nobody is at home over a longer period during severe winter.

## setButton()

void IRNeoclimaAc::setButton | ( | const uint8_t | button | ) |

Set the Button/Command pressed setting of the A/C.

Parameters

  [in] | button | The value of the button/command that was pressed.

## setEcono()

void IRNeoclimaAc::setEcono | ( | const bool | on | ) |

Set the Economy (Energy Saver) setting of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## setEye()

void IRNeoclimaAc::setEye | ( | const bool | on | ) |

Set the Eye (Sensor) setting of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## setFan()

void IRNeoclimaAc::setFan | ( | const uint8_t | speed | ) |

Set the speed of the fan.

Parameters

  [in] | speed | The desired setting. 0-3, 0 is auto, 1-3 is the speed

## setFresh()

void IRNeoclimaAc::setFresh | ( | const bool | on | ) |

Set the Fresh (air) setting of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## setHold()

void IRNeoclimaAc::setHold | ( | const bool | on | ) |

Set the Hold setting of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## setIon()

void IRNeoclimaAc::setIon | ( | const bool | on | ) |

Set the Ion (filter) setting of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## setLight()

void IRNeoclimaAc::setLight | ( | const bool | on | ) |

Set the Light(LED display) setting of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## setMode()

void IRNeoclimaAc::setMode | ( | const uint8_t | mode | ) |

Set the operating mode of the A/C.

Parameters

  [in] | mode | The desired operating mode.

## setPower()

void IRNeoclimaAc::setPower | ( | const bool | on | ) |

Change the power setting.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## setRaw()

void IRNeoclimaAc::setRaw | ( | const uint8_t | new_code[],
|  | const uint16_t | length = `kNeoclimaStateLength`
| ) |  |

Set the internal state from a valid code for this protocol.

Parameters

  [in] | new_code | A valid code for this protocol.
  [in] | length | The length/size of the new_code array.

## setSleep()

void IRNeoclimaAc::setSleep | ( | const bool | on | ) |

Set the Sleep setting of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## setSwingH()

void IRNeoclimaAc::setSwingH | ( | const bool | on | ) |

Set the horizontal swing setting of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## setSwingV()

void IRNeoclimaAc::setSwingV | ( | const bool | on | ) |

Set the vertical swing setting of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## setTemp()

void IRNeoclimaAc::setTemp | ( | const uint8_t | temp,
|  | const bool | celsius = `true`
| ) |  |

Set the temperature.

Parameters

  [in] | temp | The temperature in degrees celsius.
  [in] | celsius | Use Fahrenheit (false) or Celsius (true).

## setTurbo()

void IRNeoclimaAc::setTurbo | ( | const bool | on | ) |

Set the Turbo setting of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## stateReset()

void IRNeoclimaAc::stateReset | ( | void |  | ) |

Reset the state of the remote to a known good state/sequence.

## toCommon()

stdAc::state_t IRNeoclimaAc::toCommon | ( | void |  | ) | const

Convert the current internal state into its stdAc::state_t equivalent.

Returns
  The stdAc equivalent of the native settings.

## toCommonFanSpeed()

stdAc::fanspeed_t IRNeoclimaAc::toCommonFanSpeed | ( | const uint8_t | speed | ) |

static

Convert a native fan speed into its stdAc equivalent.

Parameters

  [in] | speed | The native setting to be converted.

Returns
  The stdAc equivalent of the native setting.

## toCommonMode()

stdAc::opmode_t IRNeoclimaAc::toCommonMode | ( | const uint8_t | mode | ) |

static

Convert a native mode into its stdAc equivalent.

Parameters

  [in] | mode | The native setting to be converted.

Returns
  The stdAc equivalent of the native setting.

## toString()

String IRNeoclimaAc::toString | ( | void |  | ) | const

Convert the current internal state into a human readable string.

Returns
  A human readable string.

## validChecksum()

bool IRNeoclimaAc::validChecksum | ( | const uint8_t | state[],
|  | const uint16_t | length = `kNeoclimaStateLength`
| ) |  |

static

Verify the checksum is valid for a given state.

Parameters

  [in] | state | The array to verify the checksum of.
  [in] | length | The length/size of the array.

Returns
  true, if the state has a valid checksum. Otherwise, false.

## Member Data Documentation

## _

NeoclimaProtocol IRNeoclimaAc::_

private

## _irsend

IRsend IRNeoclimaAc::_irsend

private

Instance of the IR send class.

The documentation for this class was generated from the following files:

- src/ir_Neoclima.h
- src/ir_Neoclima.cpp