# IRremoteESP8266: src/ir_Argo.h Source File

ir_Argo.h
Go to the documentation of this file.
// Copyright 2017 Schmolders
// Supports:
// Brand: Argo, Model: Ulisse 13 DCI Mobile Split A/C
#ifndef IR_ARGO_H_
#define IR_ARGO_H_
#ifndef UNIT_TEST
#include <Arduino.h>
#endif
#include "IRremoteESP8266.h"
#include "IRsend.h"
#ifdef UNIT_TEST
#include "IRsend_test.h"
#endif
// ARGO Ulisse DCI
union ArgoProtocol {
uint8_t raw[kArgoStateLength];
struct {
// Byte 0
uint64_t :8; // Typically 0b00110101
// Byte 1
uint64_t :8; // Typically 0b10101111
// Byte 2~4
uint64_t :3;
uint64_t Mode :3;
uint64_t Temp :5; // straddle byte 2 and 3
uint64_t Fan :2;
uint64_t RoomTemp :5; // straddle byte 3 and 4
uint64_t Flap :3; // SwingV
uint64_t :3; // OnTimer, maybe hours
// Byte 5
uint64_t :8; // OnTimer, maybe minutes
// Byte 6
uint64_t :8; // OffTimer, maybe minutes
// Byte 7
uint64_t :3; // OffTimer, maybe hours
uint64_t :5; // Time
// Byte 8
uint32_t :6; // Time
uint32_t :1; // Timer On/Off
uint32_t :1; // Timer Program
// Byte 9
uint32_t :1; // Timer Program
uint32_t :1; // Timer 1h
uint32_t Night :1;
uint32_t Max :1;
uint32_t :1; // Filter
uint32_t Power :1;
uint32_t :1; // const 0
uint32_t iFeel :1;
// Byte 10~11
uint32_t :2; // const 01
uint32_t Sum :8; // straddle byte 10 and 11
uint32_t :6;
};
};
// Constants. Store MSB left.
const uint8_t kArgoHeatBit = 0b00100000;
// Mode 0b00111000
const uint8_t kArgoCool = 0b000;
const uint8_t kArgoDry = 0b001;
const uint8_t kArgoAuto = 0b010;
const uint8_t kArgoOff = 0b011;
const uint8_t kArgoHeat = 0b100;
const uint8_t kArgoHeatAuto = 0b101;
// ?no idea what mode that is
const uint8_t kArgoHeatBlink = 0b110;
// Fan 0b00011000
const uint8_t kArgoFanAuto = 0; // 0b00
const uint8_t kArgoFan1 = 1; // 0b01
const uint8_t kArgoFan2 = 2; // 0b10
const uint8_t kArgoFan3 = 3; // 0b11
// Temp
const uint8_t kArgoTempDelta = 4;
const uint8_t kArgoMaxRoomTemp = 35; // Celsius
const uint8_t kArgoMinTemp = 10; // Celsius delta +4
const uint8_t kArgoMaxTemp = 32; // Celsius
// Flap/SwingV
const uint8_t kArgoFlapAuto = 0;
const uint8_t kArgoFlap1 = 1;
const uint8_t kArgoFlap2 = 2;
const uint8_t kArgoFlap3 = 3;
const uint8_t kArgoFlap4 = 4;
const uint8_t kArgoFlap5 = 5;
const uint8_t kArgoFlap6 = 6;
const uint8_t kArgoFlapFull = 7;
// Legacy defines. (Deprecated)
#define ARGO_COOL_ON kArgoCoolOn
#define ARGO_COOL_OFF kArgoCoolOff
#define ARGO_COOL_AUTO kArgoCoolAuto
#define ARGO_COOL_HUM kArgoCoolHum
#define ARGO_HEAT_ON kArgoHeatOn
#define ARGO_HEAT_AUTO kArgoHeatAuto
#define ARGO_HEAT_BLINK kArgoHeatBlink
#define ARGO_MIN_TEMP kArgoMinTemp
#define ARGO_MAX_TEMP kArgoMaxTemp
#define ARGO_FAN_AUTO kArgoFanAuto
#define ARGO_FAN_3 kArgoFan3
#define ARGO_FAN_2 kArgoFan2
#define ARGO_FAN_1 kArgoFan1
#define ARGO_FLAP_AUTO kArgoFlapAuto
#define ARGO_FLAP_1 kArgoFlap1
#define ARGO_FLAP_2 kArgoFlap2
#define ARGO_FLAP_3 kArgoFlap3
#define ARGO_FLAP_4 kArgoFlap4
#define ARGO_FLAP_5 kArgoFlap5
#define ARGO_FLAP_6 kArgoFlap6
#define ARGO_FLAP_FULL kArgoFlapFull
class IRArgoAC {
public:
explicit IRArgoAC(const uint16_t pin, const bool inverted = false,
const bool use_modulation = true);
#if SEND_ARGO
void send(const uint16_t repeat = kArgoDefaultRepeat);
int8_t calibrate(void) { return _irsend.calibrate(); }
#endif // SEND_ARGO
void begin(void);
void on(void);
void off(void);
void setPower(const bool on);
bool getPower(void) const;
void setTemp(const uint8_t degrees);
uint8_t getTemp(void) const;
void setFan(const uint8_t fan);
uint8_t getFan(void) const;
void setFlap(const uint8_t flap);
uint8_t getFlap(void) const;
void setMode(const uint8_t mode);
uint8_t getMode(void) const;
void setMax(const bool on);
bool getMax(void) const;
void setNight(const bool on);
bool getNight(void) const;
void setiFeel(const bool on);
bool getiFeel(void) const;
void setTime(void);
void setRoomTemp(const uint8_t degrees);
uint8_t getRoomTemp(void) const;
uint8_t* getRaw(void);
void setRaw(const uint8_t state[]);
static uint8_t calcChecksum(const uint8_t state[],
const uint16_t length = kArgoStateLength);
static bool validChecksum(const uint8_t state[],
const uint16_t length = kArgoStateLength);
static uint8_t convertMode(const stdAc::opmode_t mode);
static uint8_t convertFan(const stdAc::fanspeed_t speed);
static uint8_t convertSwingV(const stdAc::swingv_t position);
static stdAc::opmode_t toCommonMode(const uint8_t mode);
static stdAc::fanspeed_t toCommonFanSpeed(const uint8_t speed);
stdAc::state_t toCommon(void) const;
String toString(void) const;
#ifndef UNIT_TEST
private:
IRsend _irsend;
#else
IRsendTest _irsend;
#endif
// # of bytes per command
ArgoProtocol _;
void stateReset(void);
void checksum(void);
// Attributes
uint8_t flap_mode;
uint8_t heat_mode;
uint8_t cool_mode;
};
#endif // IR_ARGO_H_
IRArgoAC::setTime
void setTime(void)
Set the time for the A/C.
Definition: ir_Argo.cpp:244
IRArgoAC::calcChecksum
static uint8_t calcChecksum(const uint8_t state[], const uint16_t length=kArgoStateLength)
Verify the checksum is valid for a given state.
Definition: ir_Argo.cpp:72
ArgoProtocol::Sum
uint32_t Sum
Definition: ir_Argo.h:61
IRArgoAC::flap_mode
uint8_t flap_mode
Definition: ir_Argo.h:200
IRArgoAC::setFan
void setFan(const uint8_t fan)
Set the speed of the fan.
Definition: ir_Argo.cpp:176
IRArgoAC::_irsend
IRsend _irsend
instance of the IR send class
Definition: ir_Argo.h:188
kArgoHeatBlink
const uint8_t kArgoHeatBlink
Definition: ir_Argo.h:78
stdAc::swingv_t
swingv_t
Common A/C settings for Vertical Swing.
Definition: IRsend.h:70
IRArgoAC::getFan
uint8_t getFan(void) const
Get the current fan speed setting.
Definition: ir_Argo.cpp:182
kArgoMaxTemp
const uint8_t kArgoMaxTemp
Definition: ir_Argo.h:90
kArgoDefaultRepeat
const uint16_t kArgoDefaultRepeat
Definition: IRremoteESP8266.h:888
IRArgoAC::setTemp
void setTemp(const uint8_t degrees)
Set the temperature.
Definition: ir_Argo.cpp:159
IRArgoAC::setFlap
void setFlap(const uint8_t flap)
Set the flap position. i.e. Swing.
Definition: ir_Argo.cpp:189
IRArgoAC::toString
String toString(void) const
Convert the current internal state into a human readable string.
Definition: ir_Argo.cpp:372
IRArgoAC::convertMode
static uint8_t convertMode(const stdAc::opmode_t mode)
Convert a stdAc::opmode_t enum into its native mode.
Definition: ir_Argo.cpp:265
IRArgoAC::getRoomTemp
uint8_t getRoomTemp(void) const
Get the currently stored value for the room temperature setting.
Definition: ir_Argo.cpp:258
stdAc::fanspeed_t
fanspeed_t
Common A/C settings for Fan Speeds.
Definition: IRsend.h:58
kArgoFlap2
const uint8_t kArgoFlap2
Definition: ir_Argo.h:95
IRArgoAC::getFlap
uint8_t getFlap(void) const
Get the flap position. i.e. Swing.
Definition: ir_Argo.cpp:197
IRArgoAC::stateReset
void stateReset(void)
Reset the internals of the object to a known good state.
Definition: ir_Argo.cpp:98
ArgoProtocol::Night
uint32_t Night
Definition: ir_Argo.h:53
kArgoFlap4
const uint8_t kArgoFlap4
Definition: ir_Argo.h:97
kArgoHeatBit
const uint8_t kArgoHeatBit
Definition: ir_Argo.h:68
IRArgoAC::calibrate
int8_t calibrate(void)
Run the calibration to calculate uSec timing offsets for this platform.
Definition: ir_Argo.h:138
IRsend.h
IRArgoAC::getPower
bool getPower(void) const
Get the power setting from the internal state.
Definition: ir_Argo.cpp:144
kArgoFlap3
const uint8_t kArgoFlap3
Definition: ir_Argo.h:96
IRsend
Class for sending all basic IR protocols.
Definition: IRsend.h:182
IRArgoAC::validChecksum
static bool validChecksum(const uint8_t state[], const uint16_t length=kArgoStateLength)
Verify the checksum is valid for a given state.
Definition: ir_Argo.cpp:83
IRsend::calibrate
int8_t calibrate(uint16_t hz=38000U)
Calculate & set any offsets to account for execution times during sending.
Definition: IRsend.cpp:207
kArgoStateLength
const uint16_t kArgoStateLength
Definition: IRremoteESP8266.h:886
String
std::string String
Definition: IRremoteESP8266.h:1178
kArgoFan1
const uint8_t kArgoFan1
Definition: ir_Argo.h:82
IRArgoAC::toCommonMode
static stdAc::opmode_t toCommonMode(const uint8_t mode)
Convert a native mode into its stdAc equivalent.
Definition: ir_Argo.cpp:322
kArgoOff
const uint8_t kArgoOff
Definition: ir_Argo.h:74
ArgoProtocol::Flap
uint64_t Flap
Definition: ir_Argo.h:37
IRArgoAC::getiFeel
bool getiFeel(void) const
Get the status of iFeel mode.
Definition: ir_Argo.cpp:240
IRArgoAC::convertSwingV
static uint8_t convertSwingV(const stdAc::swingv_t position)
Convert a stdAc::swingv_t enum into it's native setting.
Definition: ir_Argo.cpp:302
kArgoFlapFull
const uint8_t kArgoFlapFull
Definition: ir_Argo.h:100
ArgoProtocol::Mode
uint64_t Mode
Definition: ir_Argo.h:33
IRremoteESP8266.h
IRArgoAC::getTemp
uint8_t getTemp(void) const
Get the current temperature setting.
Definition: ir_Argo.cpp:170
kArgoDry
const uint8_t kArgoDry
Definition: ir_Argo.h:72
IRArgoAC::toCommon
stdAc::state_t toCommon(void) const
Convert the current internal state into its stdAc::state_t equivalent.
Definition: ir_Argo.cpp:346
kArgoAuto
const uint8_t kArgoAuto
Definition: ir_Argo.h:73
IRArgoAC::setRoomTemp
void setRoomTemp(const uint8_t degrees)
Set the value for the current room temperature.
Definition: ir_Argo.cpp:250
IRArgoAC::convertFan
static uint8_t convertFan(const stdAc::fanspeed_t speed)
Convert a stdAc::fanspeed_t enum into it's native speed.
Definition: ir_Argo.cpp:284
IRArgoAC::off
void off(void)
Set the internal state to have the power off.
Definition: ir_Argo.cpp:134
ArgoProtocol::Temp
uint64_t Temp
Definition: ir_Argo.h:34
ArgoProtocol::Power
uint32_t Power
Definition: ir_Argo.h:56
IRArgoAC::setPower
void setPower(const bool on)
Set the internal state to have the desired power.
Definition: ir_Argo.cpp:138
kArgoFlap1
const uint8_t kArgoFlap1
Definition: ir_Argo.h:94
ArgoProtocol::raw
uint8_t raw[kArgoStateLength]
The state in native IR code form.
Definition: ir_Argo.h:25
IRArgoAC::getRaw
uint8_t * getRaw(void)
Get the raw state of the object, suitable to be sent with the appropriate IRsend object method.
Definition: ir_Argo.cpp:119
ArgoProtocol::Fan
uint64_t Fan
Definition: ir_Argo.h:35
IRArgoAC::heat_mode
uint8_t heat_mode
Definition: ir_Argo.h:201
ArgoProtocol::Max
uint32_t Max
Definition: ir_Argo.h:54
ArgoProtocol::RoomTemp
uint64_t RoomTemp
Definition: ir_Argo.h:36
kArgoMinTemp
const uint8_t kArgoMinTemp
Definition: ir_Argo.h:89
IRArgoAC::on
void on(void)
Set the internal state to have the power on.
Definition: ir_Argo.cpp:131
IRArgoAC::setNight
void setNight(const bool on)
Turn on/off the Night mode. i.e. Sleep.
Definition: ir_Argo.cpp:224
kArgoFan2
const uint8_t kArgoFan2
Definition: ir_Argo.h:83
kArgoCool
const uint8_t kArgoCool
Definition: ir_Argo.h:71
IRArgoAC::send
void send(const uint16_t repeat=kArgoDefaultRepeat)
Send the current internal state as an IR message.
Definition: ir_Argo.cpp:63
IRArgoAC::_
ArgoProtocol _
Definition: ir_Argo.h:195
kArgoHeatAuto
const uint8_t kArgoHeatAuto
Definition: ir_Argo.h:76
ArgoProtocol
Native representation of a Argo A/C message.
Definition: ir_Argo.h:24
IRArgoAC::toCommonFanSpeed
static stdAc::fanspeed_t toCommonFanSpeed(const uint8_t speed)
Convert a native fan speed into its stdAc equivalent.
Definition: ir_Argo.cpp:335
kArgoHeat
const uint8_t kArgoHeat
Definition: ir_Argo.h:75
IRArgoAC::setRaw
void setRaw(const uint8_t state[])
Set the raw state of the object.
Definition: ir_Argo.cpp:126
IRArgoAC::getMode
uint8_t getMode(void) const
Get the current operation mode setting.
Definition: ir_Argo.cpp:201
kArgoFlap5
const uint8_t kArgoFlap5
Definition: ir_Argo.h:98
IRArgoAC::IRArgoAC
IRArgoAC(const uint16_t pin, const bool inverted=false, const bool use_modulation=true)
Class constructor.
Definition: ir_Argo.cpp:53
kArgoTempDelta
const uint8_t kArgoTempDelta
Definition: ir_Argo.h:87
IRArgoAC::checksum
void checksum(void)
Update the checksum for the internal state.
Definition: ir_Argo.cpp:89
kArgoFlap6
const uint8_t kArgoFlap6
Definition: ir_Argo.h:99
IRArgoAC::cool_mode
uint8_t cool_mode
Definition: ir_Argo.h:202
IRArgoAC::getMax
bool getMax(void) const
Is the Max (i.e. Turbo) setting on?
Definition: ir_Argo.cpp:154
IRArgoAC::getNight
bool getNight(void) const
Get the status of Night mode. i.e. Sleep.
Definition: ir_Argo.cpp:230
IRArgoAC::setiFeel
void setiFeel(const bool on)
Turn on/off the iFeel mode.
Definition: ir_Argo.cpp:234
ArgoProtocol::iFeel
uint32_t iFeel
Definition: ir_Argo.h:58
IRArgoAC::setMax
void setMax(const bool on)
Control the current Max setting. (i.e. Turbo)
Definition: ir_Argo.cpp:148
kArgoFlapAuto
const uint8_t kArgoFlapAuto
Definition: ir_Argo.h:93
stdAc::state_t
Structure to hold a common A/C state.
Definition: IRsend.h:97
kArgoFan3
const uint8_t kArgoFan3
Definition: ir_Argo.h:84
IRArgoAC
Class for handling detailed Argo A/C messages.
Definition: ir_Argo.h:127
kArgoFanAuto
const uint8_t kArgoFanAuto
Definition: ir_Argo.h:81
IRArgoAC::begin
void begin(void)
Set up hardware to be able to send a message.
Definition: ir_Argo.cpp:58
IRArgoAC::setMode
void setMode(const uint8_t mode)
Set the desired operation mode.
Definition: ir_Argo.cpp:207
kArgoMaxRoomTemp
const uint8_t kArgoMaxRoomTemp
Definition: ir_Argo.h:88
stdAc::opmode_t
opmode_t
Common A/C settings for A/C operating modes.
Definition: IRsend.h:46