# IRremoteESP8266: Member List

IRHitachiAc1 Member List

This is the complete list of members for IRHitachiAc1, including all inherited members.

_ | IRHitachiAc1 | private
_irsend | IRHitachiAc1 | private
begin(void) | IRHitachiAc1 |
calcChecksum(const uint8_t state[], const uint16_t length=kHitachiAc1StateLength) | IRHitachiAc1 | static
calibrate(void) | IRHitachiAc1 | inline
checksum(const uint16_t length=kHitachiAc1StateLength) | IRHitachiAc1 | private
convertFan(const stdAc::fanspeed_t speed) | IRHitachiAc1 | static
convertMode(const stdAc::opmode_t mode) | IRHitachiAc1 | static
getFan(void) const | IRHitachiAc1 |
getMode(void) const | IRHitachiAc1 |
getModel(void) const | IRHitachiAc1 |
getOffTimer(void) const | IRHitachiAc1 |
getOnTimer(void) const | IRHitachiAc1 |
getPower(void) const | IRHitachiAc1 |
getPowerToggle(void) const | IRHitachiAc1 |
getRaw(void) | IRHitachiAc1 |
getSleep(void) const | IRHitachiAc1 |
getSwingH(void) const | IRHitachiAc1 |
getSwingToggle(void) const | IRHitachiAc1 |
getSwingV(void) const | IRHitachiAc1 |
getTemp(void) const | IRHitachiAc1 |
IRHitachiAc1(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRHitachiAc1 | explicit
off(void) | IRHitachiAc1 |
on(void) | IRHitachiAc1 |
send(const uint16_t repeat=kHitachiAcDefaultRepeat) | IRHitachiAc1 |
setFan(const uint8_t speed, const bool force=false) | IRHitachiAc1 |
setMode(const uint8_t mode) | IRHitachiAc1 |
setModel(const hitachi_ac1_remote_model_t model) | IRHitachiAc1 |
setOffTimer(const uint16_t mins) | IRHitachiAc1 |
setOnTimer(const uint16_t mins) | IRHitachiAc1 |
setPower(const bool on) | IRHitachiAc1 |
setPowerToggle(const bool on) | IRHitachiAc1 |
setRaw(const uint8_t new_code[], const uint16_t length=kHitachiAc1StateLength) | IRHitachiAc1 |
setSleep(const uint8_t mode) | IRHitachiAc1 |
setSwingH(const bool on) | IRHitachiAc1 |
setSwingToggle(const bool toggle) | IRHitachiAc1 |
setSwingV(const bool on) | IRHitachiAc1 |
setTemp(const uint8_t temp) | IRHitachiAc1 |
stateReset(void) | IRHitachiAc1 |
toCommon(void) const | IRHitachiAc1 |
toCommonFanSpeed(const uint8_t speed) | IRHitachiAc1 | static
toCommonMode(const uint8_t mode) | IRHitachiAc1 | static
toString(void) const | IRHitachiAc1 |
validChecksum(const uint8_t state[], const uint16_t length=kHitachiAc1StateLength) | IRHitachiAc1 | static