# IRremoteESP8266: HitachiProtocol Union Reference

HitachiProtocol Union Reference

Native representation of a Hitachi 224-bit A/C message. More...

`#include <ir_Hitachi.h>`

## Public Attributes

uint8_t | raw [kHitachiAcStateLength]
| The state in native code. More...
struct {
uint8_t pad0 [10]
uint8_t Mode:8
uint8_t Temp:8
uint8_t __pad0__:8
uint8_t Fan:8
uint8_t __pad1__:7
uint8_t SwingV:1
uint8_t __pad2__:7
uint8_t SwingH:1
uint8_t __pad3__:8
uint8_t Power:1
uint8_t __pad4__:7
uint8_t pad1 [9]
uint8_t Sum:8
}; |

## Detailed Description

Native representation of a Hitachi 224-bit A/C message.

## Member Data Documentation

## @43

struct { ... }

## __pad0__

uint8_t HitachiProtocol::__pad0__

## __pad1__

uint8_t HitachiProtocol::__pad1__

## __pad2__

uint8_t HitachiProtocol::__pad2__

## __pad3__

uint8_t HitachiProtocol::__pad3__

## __pad4__

uint8_t HitachiProtocol::__pad4__

## Fan

uint8_t HitachiProtocol::Fan

## Mode

uint8_t HitachiProtocol::Mode

## pad0

uint8_t HitachiProtocol::pad0[10]

## pad1

uint8_t HitachiProtocol::pad1[9]

## Power

uint8_t HitachiProtocol::Power

## raw

uint8_t HitachiProtocol::raw[kHitachiAcStateLength]

The state in native code.

## Sum

uint8_t HitachiProtocol::Sum

## SwingH

uint8_t HitachiProtocol::SwingH

## SwingV

uint8_t HitachiProtocol::SwingV

## Temp

uint8_t HitachiProtocol::Temp

The documentation for this union was generated from the following file:

- src/ir_Hitachi.h