# IRremoteESP8266: Mitsubishi112Protocol Union Reference

Mitsubishi112Protocol Union Reference

Native representation of a Mitsubishi 112-bit A/C message. More...

`#include <ir_Mitsubishi.h>`

## Public Attributes

uint8_t | raw [kMitsubishi112StateLength]
| The state in code form. More...
struct {
uint8_t pad0 [5]
uint8_t __pad0__:2
uint8_t Power:1
uint8_t __pad1__:5
uint8_t Mode:3
uint8_t __pad2__:5
uint8_t Temp:4
uint8_t __pad3__:4
uint8_t Fan:3
uint8_t SwingV:3
uint8_t __pad4__:2
uint8_t pad1 [3]
uint8_t __pad5__:2
uint8_t SwingH:4
uint8_t __pad6__:2
uint8_t Sum:8
}; |

## Detailed Description

Native representation of a Mitsubishi 112-bit A/C message.

## Member Data Documentation

## @60

struct { ... }

## __pad0__

uint8_t Mitsubishi112Protocol::__pad0__

## __pad1__

uint8_t Mitsubishi112Protocol::__pad1__

## __pad2__

uint8_t Mitsubishi112Protocol::__pad2__

## __pad3__

uint8_t Mitsubishi112Protocol::__pad3__

## __pad4__

uint8_t Mitsubishi112Protocol::__pad4__

## __pad5__

uint8_t Mitsubishi112Protocol::__pad5__

## __pad6__

uint8_t Mitsubishi112Protocol::__pad6__

## Fan

uint8_t Mitsubishi112Protocol::Fan

## Mode

uint8_t Mitsubishi112Protocol::Mode

## pad0

uint8_t Mitsubishi112Protocol::pad0[5]

## pad1

uint8_t Mitsubishi112Protocol::pad1[3]

## Power

uint8_t Mitsubishi112Protocol::Power

## raw

uint8_t Mitsubishi112Protocol::raw[kMitsubishi112StateLength]

The state in code form.

## Sum

uint8_t Mitsubishi112Protocol::Sum

## SwingH

uint8_t Mitsubishi112Protocol::SwingH

## SwingV

uint8_t Mitsubishi112Protocol::SwingV

## Temp

uint8_t Mitsubishi112Protocol::Temp

The documentation for this union was generated from the following file:

- src/ir_Mitsubishi.h