# IRremoteESP8266: AmcorProtocol Union Reference

AmcorProtocol Union Reference

Native representation of a Amcor A/C message. More...

`#include <ir_Amcor.h>`

## Public Attributes

uint8_t | raw [kAmcorStateLength]
struct {
uint8_t __pad0__:8
uint8_t Mode:3
uint8_t __pad1__:1
uint8_t Fan:3
uint8_t __pad2__:1
uint8_t __pad3__:1
uint8_t Temp:6
uint8_t __pad4__:1
uint8_t __pad5__:8
uint8_t __pad6__:8
uint8_t __pad7__:4
uint8_t Power:4
uint8_t Max:2
uint8_t __pad8__:4
uint8_t Vent:2
uint8_t Sum:8
}; |

## Detailed Description

Native representation of a Amcor A/C message.

## Member Data Documentation

## @3

struct { ... }

## __pad0__

uint8_t AmcorProtocol::__pad0__

## __pad1__

uint8_t AmcorProtocol::__pad1__

## __pad2__

uint8_t AmcorProtocol::__pad2__

## __pad3__

uint8_t AmcorProtocol::__pad3__

## __pad4__

uint8_t AmcorProtocol::__pad4__

## __pad5__

uint8_t AmcorProtocol::__pad5__

## __pad6__

uint8_t AmcorProtocol::__pad6__

## __pad7__

uint8_t AmcorProtocol::__pad7__

## __pad8__

uint8_t AmcorProtocol::__pad8__

## Fan

uint8_t AmcorProtocol::Fan

## Max

uint8_t AmcorProtocol::Max

## Mode

uint8_t AmcorProtocol::Mode

## Power

uint8_t AmcorProtocol::Power

## raw

uint8_t AmcorProtocol::raw[kAmcorStateLength]

## Sum

uint8_t AmcorProtocol::Sum

## Temp

uint8_t AmcorProtocol::Temp

## Vent

uint8_t AmcorProtocol::Vent

The documentation for this union was generated from the following file:

- src/ir_Amcor.h