# IRremoteESP8266: Hitachi1Protocol Union Reference

Hitachi1Protocol Union Reference

Native representation of a Hitachi 104-bit A/C message. More...

`#include <ir_Hitachi.h>`

## Public Attributes

uint8_t | raw [kHitachiAc1StateLength]
| The state in native code. More...
struct {
uint8_t pad [3]
uint8_t __pad0__:6
uint8_t Model:2
uint8_t __pad1__:8
uint8_t Fan:4
uint8_t Mode:4
uint8_t __pad2__:2
uint8_t Temp:5
uint8_t __pad3__:1
uint8_t OffTimerLow:8
uint8_t OffTimerHigh:8
uint8_t OnTimerLow:8
uint8_t OnTimerHigh:8
uint8_t SwingToggle:1
uint8_t Sleep:3
uint8_t PowerToggle:1
uint8_t Power:1
uint8_t SwingV:1
uint8_t SwingH:1
uint8_t Sum:8
}; |

## Detailed Description

Native representation of a Hitachi 104-bit A/C message.

## Member Data Documentation

## @47

struct { ... }

## __pad0__

uint8_t Hitachi1Protocol::__pad0__

## __pad1__

uint8_t Hitachi1Protocol::__pad1__

## __pad2__

uint8_t Hitachi1Protocol::__pad2__

## __pad3__

uint8_t Hitachi1Protocol::__pad3__

## Fan

uint8_t Hitachi1Protocol::Fan

## Mode

uint8_t Hitachi1Protocol::Mode

## Model

uint8_t Hitachi1Protocol::Model

## OffTimerHigh

uint8_t Hitachi1Protocol::OffTimerHigh

## OffTimerLow

uint8_t Hitachi1Protocol::OffTimerLow

## OnTimerHigh

uint8_t Hitachi1Protocol::OnTimerHigh

## OnTimerLow

uint8_t Hitachi1Protocol::OnTimerLow

## pad

uint8_t Hitachi1Protocol::pad[3]

## Power

uint8_t Hitachi1Protocol::Power

## PowerToggle

uint8_t Hitachi1Protocol::PowerToggle

## raw

uint8_t Hitachi1Protocol::raw[kHitachiAc1StateLength]

The state in native code.

## Sleep

uint8_t Hitachi1Protocol::Sleep

## Sum

uint8_t Hitachi1Protocol::Sum

## SwingH

uint8_t Hitachi1Protocol::SwingH

## SwingToggle

uint8_t Hitachi1Protocol::SwingToggle

## SwingV

uint8_t Hitachi1Protocol::SwingV

## Temp

uint8_t Hitachi1Protocol::Temp

The documentation for this union was generated from the following file:

- src/ir_Hitachi.h