# IRremoteESP8266: CarrierProtocol Union Reference

CarrierProtocol Union Reference

Native representation of a Carrier A/C message. More...

`#include <ir_Carrier.h>`

## Public Attributes

uint64_t | raw
| The state of the IR remote. More...
struct {
uint8_t __pad0__:8
uint8_t __pad1__:8
uint8_t Sum:4
uint8_t Mode:2
uint8_t Fan:2
uint8_t Temp:4
uint8_t __pad2__:1
uint8_t SwingV:1
uint8_t __pad3__:2
uint8_t __pad4__:4
uint8_t Power:1
uint8_t OffTimerEnable:1
uint8_t OnTimerEnable:1
uint8_t Sleep:1
uint8_t __pad5__:8
uint8_t __pad6__:4
uint8_t OnTimer:4
uint8_t __pad7__:4
uint8_t OffTimer:4
}; |

## Detailed Description

Native representation of a Carrier A/C message.

## Member Data Documentation

## @7

struct { ... }

## __pad0__

uint8_t CarrierProtocol::__pad0__

## __pad1__

uint8_t CarrierProtocol::__pad1__

## __pad2__

uint8_t CarrierProtocol::__pad2__

## __pad3__

uint8_t CarrierProtocol::__pad3__

## __pad4__

uint8_t CarrierProtocol::__pad4__

## __pad5__

uint8_t CarrierProtocol::__pad5__

## __pad6__

uint8_t CarrierProtocol::__pad6__

## __pad7__

uint8_t CarrierProtocol::__pad7__

## Fan

uint8_t CarrierProtocol::Fan

## Mode

uint8_t CarrierProtocol::Mode

## OffTimer

uint8_t CarrierProtocol::OffTimer

## OffTimerEnable

uint8_t CarrierProtocol::OffTimerEnable

## OnTimer

uint8_t CarrierProtocol::OnTimer

## OnTimerEnable

uint8_t CarrierProtocol::OnTimerEnable

## Power

uint8_t CarrierProtocol::Power

## raw

uint64_t CarrierProtocol::raw

The state of the IR remote.

## Sleep

uint8_t CarrierProtocol::Sleep

## Sum

uint8_t CarrierProtocol::Sum

## SwingV

uint8_t CarrierProtocol::SwingV

## Temp

uint8_t CarrierProtocol::Temp

The documentation for this union was generated from the following file:

- src/ir_Carrier.h