# IRremoteESP8266: Deprecated List

Deprecated List

Member IRsend::sendPanasonic (const uint16_t address, const uint32_t data, const uint16_t nbits=kPanasonicBits, const uint16_t repeat=kNoRepeat)
  This is only for legacy use only, please use `sendPanasonic64()` instead.
Member IRsend::sendSharp (const uint16_t address, const uint16_t command, const uint16_t nbits=kSharpBits, const uint16_t repeat=kNoRepeat)
  Only use this if you are using legacy from the original Arduino-IRremote library. 99% of the time, you will want to use `sendSharpRaw()` instead
Member resultToTimingInfo (const decode_results *const results)
  This is only for those that want this legacy format.