# IRremoteESP8266: Member List

IRTranscoldAc Member List

This is the complete list of members for IRTranscoldAc, including all inherited members.

_irsend | IRTranscoldAc | private
begin() | IRTranscoldAc |
calibrate(void) | IRTranscoldAc | inline
convertFan(const stdAc::fanspeed_t speed) | IRTranscoldAc |
convertMode(const stdAc::opmode_t mode) | IRTranscoldAc |
getFan() | IRTranscoldAc |
getMode() | IRTranscoldAc |
getNormalState(void) | IRTranscoldAc | private
getPower() | IRTranscoldAc |
getRaw() | IRTranscoldAc |
getSwing() | IRTranscoldAc |
getTemp() | IRTranscoldAc |
getTempRaw() | IRTranscoldAc | private
handleSpecialState(const uint32_t data) | IRTranscoldAc | private
IRTranscoldAc(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRTranscoldAc | explicit
isSpecialState(void) | IRTranscoldAc | private
off() | IRTranscoldAc |
on() | IRTranscoldAc |
powerFlag | IRTranscoldAc | private
recoverSavedState(void) | IRTranscoldAc | private
remote_state | IRTranscoldAc | private
saved_state | IRTranscoldAc | private
send(const uint16_t repeat=kTranscoldDefaultRepeat) | IRTranscoldAc |
setFan(const uint8_t speed, const bool modecheck=true) | IRTranscoldAc |
setMode(const uint8_t mode) | IRTranscoldAc |
setPower(const bool state) | IRTranscoldAc |
setRaw(const uint32_t new_code) | IRTranscoldAc |
setSwing() | IRTranscoldAc |
setTemp(const uint8_t temp) | IRTranscoldAc |
setTempRaw(const uint8_t code) | IRTranscoldAc | private
stateReset() | IRTranscoldAc |
swingFlag | IRTranscoldAc | private
swingHFlag | IRTranscoldAc | private
swingVFlag | IRTranscoldAc | private
toCommon(const stdAc::state_t *prev=NULL) | IRTranscoldAc |
toCommonFanSpeed(const uint8_t speed) | IRTranscoldAc | static
toCommonMode(const uint8_t mode) | IRTranscoldAc | static
toString() | IRTranscoldAc |
updateSavedState(void) | IRTranscoldAc | private