# IRremoteESP8266: IRac Class Reference

IRac Class Reference

A universal/common/generic interface for controling supported A/Cs. More...

`#include <IRac.h>`

Collaboration diagram for IRac:
[legend]

## Public Member Functions

| IRac (const uint16_t pin, const bool inverted=false, const bool use_modulation=true)
| Class constructor. More...
void | markAsSent (void)
| Update the previous state to the current one. More...
bool | sendAc (void)
| Send an A/C message based soley on our internal state. More...
bool | sendAc (const stdAc::state_t desired, const stdAc::state_t *prev=NULL)
| Send A/C message for a given device using state_t structures. More...

bool

sendAc (const decode_type_t vendor, const int16_t model, const bool power, const stdAc::opmode_t mode, const float degrees, const bool celsius, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet, const bool turbo, const bool econo, const bool light, const bool filter, const bool clean, const bool beep, const int16_t sleep=-1, const int16_t clock=-1)

| Send A/C message for a given device using common A/C settings. More...
stdAc::state_t | getState (void)
| Get the current internal A/C climate state. More...
stdAc::state_t | getStatePrev (void)
| Get the previous internal A/C climate state that should have already been sent to the device. i.e. What the A/C unit should already be set to. More...
bool | hasStateChanged (void)
| Check if the internal state has changed from what was previously sent. More...

## Static Public Member Functions

static bool | isProtocolSupported (const decode_type_t protocol)
| Is the given protocol supported by the IRac class? More...

static void

initState (stdAc::state_t *state, const decode_type_t vendor, const int16_t model, const bool power, const stdAc::opmode_t mode, const float degrees, const bool celsius, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet, const bool turbo, const bool econo, const bool light, const bool filter, const bool clean, const bool beep, const int16_t sleep, const int16_t clock)

| Initialise the given state with the supplied settings. More...
static void | initState (stdAc::state_t *state)
| Initialise the given state with the supplied settings. More...
static bool | cmpStates (const stdAc::state_t a, const stdAc::state_t b)
| Compare two AirCon states. More...
static bool | strToBool (const char *str, const bool def=false)
| Convert the supplied str into the appropriate boolean value. More...
static int16_t | strToModel (const char *str, const int16_t def=-1)
| Convert the supplied str into the appropriate enum. More...
static stdAc::opmode_t | strToOpmode (const char *str, const stdAc::opmode_t def=stdAc::opmode_t::kAuto)
| Convert the supplied str into the appropriate enum. More...
static stdAc::fanspeed_t | strToFanspeed (const char *str, const stdAc::fanspeed_t def=stdAc::fanspeed_t::kAuto)
| Convert the supplied str into the appropriate enum. More...
static stdAc::swingv_t | strToSwingV (const char *str, const stdAc::swingv_t def=stdAc::swingv_t::kOff)
| Convert the supplied str into the appropriate enum. More...
static stdAc::swingh_t | strToSwingH (const char *str, const stdAc::swingh_t def=stdAc::swingh_t::kOff)
| Convert the supplied str into the appropriate enum. More...
static String | boolToString (const bool value)
| Convert the supplied boolean into the appropriate String. More...
static String | opmodeToString (const stdAc::opmode_t mode)
| Convert the supplied operation mode into the appropriate String. More...
static String | fanspeedToString (const stdAc::fanspeed_t speed)
| Convert the supplied fan speed enum into the appropriate String. More...
static String | swingvToString (const stdAc::swingv_t swingv)
| Convert the supplied enum into the appropriate String. More...
static String | swinghToString (const stdAc::swingh_t swingh)
| Convert the supplied enum into the appropriate String. More...

## Public Attributes

stdAc::state_t | next
| The state we want the device to be in after we send. More...

## Private Member Functions

void | airwell (IRAirwellAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan)
| Send an Airwell A/C message with the supplied settings. More...
void | amcor (IRAmcorAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan)
| Send an Amcor A/C message with the supplied settings. More...
void | argo (IRArgoAC *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool turbo, const int16_t sleep=-1)
| Send an Argo A/C message with the supplied settings. More...
void | carrier64 (IRCarrierAc64 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const int16_t sleep=-1)
| Send a Carrier 64-bit A/C message with the supplied settings. More...
void | coolix (IRCoolixAC *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool turbo, const bool light, const bool clean, const int16_t sleep=-1)
| Send a Coolix A/C message with the supplied settings. More...
void | corona (IRCoronaAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool econo)
| Send a Corona A/C message with the supplied settings. More...
void | daikin (IRDaikinESP *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet, const bool turbo, const bool econo, const bool clean)
| Send a Daikin A/C message with the supplied settings. More...
void | daikin128 (IRDaikin128 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool quiet, const bool turbo, const bool light, const bool econo, const int16_t sleep=-1, const int16_t clock=-1)
| Send a Daikin 128-bit A/C message with the supplied settings. More...
void | daikin152 (IRDaikin152 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool quiet, const bool turbo, const bool econo)
| Send a Daikin 152-bit A/C message with the supplied settings. More...
void | daikin160 (IRDaikin160 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv)
| Send a Daikin 160-bit A/C message with the supplied settings. More...
void | daikin176 (IRDaikin176 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingh_t swingh)
| Send a Daikin 176-bit A/C message with the supplied settings. More...
void | daikin2 (IRDaikin2 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet, const bool turbo, const bool light, const bool econo, const bool filter, const bool clean, const bool beep, const int16_t sleep=-1, const int16_t clock=-1)
| Send a Daikin2 A/C message with the supplied settings. More...
void | daikin216 (IRDaikin216 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet, const bool turbo)
| Send a Daikin 216-bit A/C message with the supplied settings. More...
void | daikin64 (IRDaikin64 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool quiet, const bool turbo, const int16_t sleep=-1, const int16_t clock=-1)
| Send a Daikin 64-bit A/C message with the supplied settings. More...
void | delonghiac (IRDelonghiAc *ac, const bool on, const stdAc::opmode_t mode, const bool celsius, const float degrees, const stdAc::fanspeed_t fan, const bool turbo, const int16_t sleep=-1)
| Send a Delonghi A/C message with the supplied settings. More...
void | electra (IRElectraAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool turbo, const bool lighttoggle, const bool clean)
| Send an Electra A/C message with the supplied settings. More...
void | fujitsu (IRFujitsuAC *ac, const fujitsu_ac_remote_model_t model, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet, const bool turbo, const bool econo, const bool filter, const bool clean, const int16_t sleep=-1)
| Send a Fujitsu A/C message with the supplied settings. More...
void | goodweather (IRGoodweatherAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool turbo, const bool light, const int16_t sleep=-1)
| Send a Goodweather A/C message with the supplied settings. More...
void | gree (IRGreeAC *ac, const gree_ac_remote_model_t model, const bool on, const stdAc::opmode_t mode, const bool celsius, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool turbo, const bool light, const bool clean, const int16_t sleep=-1)
| Send a Gree A/C message with the supplied settings. More...
void | haier (IRHaierAC *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool filter, const int16_t sleep=-1, const int16_t clock=-1)
| Send a Haier A/C message with the supplied settings. More...
void | haierYrwo2 (IRHaierACYRW02 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool turbo, const bool filter, const int16_t sleep=-1)
| Send a Haier YRWO2 A/C message with the supplied settings. More...
void | hitachi (IRHitachiAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh)
| Send a Hitachi A/C message with the supplied settings. More...
void | hitachi1 (IRHitachiAc1 *ac, const hitachi_ac1_remote_model_t model, const bool on, const bool power_toggle, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool swing_toggle, const int16_t sleep=-1)
| Send a Hitachi1 A/C message with the supplied settings. More...
void | hitachi344 (IRHitachiAc344 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh)
| Send a Hitachi 344-bit A/C message with the supplied settings. More...
void | hitachi424 (IRHitachiAc424 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv)
| Send a Hitachi 424-bit A/C message with the supplied settings. More...
void | kelvinator (IRKelvinatorAC *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet, const bool turbo, const bool light, const bool filter, const bool clean)
| Send a Kelvinator A/C message with the supplied settings. More...
void | lg (IRLgAc *ac, const lg_ac_remote_model_t model, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan)
| Send a LG A/C message with the supplied settings. More...
void | midea (IRMideaAC *ac, const bool on, const stdAc::opmode_t mode, const bool celsius, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool turbo, const bool econo, const bool light, const int16_t sleep=-1)
| Send a Midea A/C message with the supplied settings. More...
void | mitsubishi (IRMitsubishiAC *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet, const int16_t clock=-1)
| Send a Mitsubishi A/C message with the supplied settings. More...
void | mitsubishi112 (IRMitsubishi112 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet)
| Send a Mitsubishi 112-bit A/C message with the supplied settings. More...
void | mitsubishi136 (IRMitsubishi136 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool quiet)
| Send a Mitsubishi 136-bit A/C message with the supplied settings. More...
void | mitsubishiHeavy88 (IRMitsubishiHeavy88Ac *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool turbo, const bool econo, const bool clean)
| Send a Mitsubishi Heavy 88-bit A/C message with the supplied settings. More...
void | mitsubishiHeavy152 (IRMitsubishiHeavy152Ac *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet, const bool turbo, const bool econo, const bool filter, const bool clean, const int16_t sleep=-1)
| Send a Mitsubishi Heavy 152-bit A/C message with the supplied settings. More...
void | neoclima (IRNeoclimaAc *ac, const bool on, const stdAc::opmode_t mode, const bool celsius, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool turbo, const bool econo, const bool light, const bool filter, const int16_t sleep=-1)
| Send a Neoclima A/C message with the supplied settings. More...
void | panasonic (IRPanasonicAc *ac, const panasonic_ac_remote_model_t model, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet, const bool turbo, const bool filter, const int16_t clock=-1)
| Send a Panasonic A/C message with the supplied settings. More...
void | samsung (IRSamsungAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool quiet, const bool turbo, const bool light, const bool filter, const bool clean, const bool beep, const bool prevpower=true, const bool forcepower=true)
| Send a Samsung A/C message with the supplied settings. More...
void | sanyo (IRSanyoAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool beep, const int16_t sleep=-1)
| Send a Toshiba A/C message with the supplied settings. More...
void | sharp (IRSharpAc *ac, const sharp_ac_remote_model_t model, const bool on, const bool prev_power, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool turbo, const bool light, const bool filter, const bool clean)
| Send a Sharp A/C message with the supplied settings. More...
void | tcl112 (IRTcl112Ac *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool turbo, const bool light, const bool econo, const bool filter)
| Send a TCL 112-bit A/C message with the supplied settings. More...
void | technibel (IRTechnibelAc *ac, const bool on, const stdAc::opmode_t mode, const bool celsius, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const int16_t sleep=-1)
| Send a Technibel A/C message with the supplied settings. More...
void | teco (IRTecoAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool light, const int16_t sleep=-1)
| Send a Teco A/C message with the supplied settings. More...
void | toshiba (IRToshibaAC *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool turbo, const bool econo)
| Send a Toshiba A/C message with the supplied settings. More...
void | trotec (IRTrotecESP *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const int16_t sleep=-1)
| Send a Trotec A/C message with the supplied settings. More...
void | vestel (IRVestelAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool turbo, const bool filter, const int16_t sleep=-1, const int16_t clock=-1, const bool sendNormal=true)
| Send a Vestel A/C message with the supplied settings. More...
void | voltas (IRVoltas *ac, const voltas_ac_remote_model_t model, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool turbo, const bool econo, const bool light, const int16_t sleep=-1)
| Send a Voltas A/C message with the supplied settings. More...
void | whirlpool (IRWhirlpoolAc *ac, const whirlpool_ac_remote_model_t model, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool turbo, const bool light, const int16_t sleep=-1, const int16_t clock=-1)
| Send a Whirlpool A/C message with the supplied settings. More...
void | transcold (IRTranscoldAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh)
| Send a Transcold A/C message with the supplied settings. More...

## Static Private Member Functions

static stdAc::state_t | cleanState (const stdAc::state_t state)
| Create a new state base on the provided state that has been suitably fixed. More...
static stdAc::state_t | handleToggles (const stdAc::state_t desired, const stdAc::state_t *prev=NULL)
| Create a new state base on desired & previous states but handle any state changes for options that need to be toggled. More...

## Private Attributes

uint16_t | _pin
| The GPIO to use to transmit messages from. More...
bool | _inverted
| IR LED is lit when GPIO is LOW (true) or HIGH (false)? More...
bool | _modulation
| Is frequency modulation to be used? More...
stdAc::state_t | _prev
| The state we expect the device to currently be in. More...

## Detailed Description

A universal/common/generic interface for controling supported A/Cs.

## Constructor & Destructor Documentation

## IRac()

IRac::IRac | ( | const uint16_t | pin,
|  | const bool | inverted = `false`,
|  | const bool | use_modulation = `true`
| ) |  |

explicit

Class constructor.

Parameters

  [in] | pin | Gpio pin to use when transmitting IR messages.
  [in] | inverted | true, gpio output defaults to high. false, to low.
  [in] | use_modulation | true means use frequency modulation. false, don't.

## Member Function Documentation

## airwell()

void IRac::airwell | ( | IRAirwellAc * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan
| ) |  |

private

Send an Airwell A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRAirwellAc object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.

## amcor()

void IRac::amcor | ( | IRAmcorAc * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan
| ) |  |

private

Send an Amcor A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRAmcorAc object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.

## argo()

void IRac::argo | ( | IRArgoAC * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const bool | turbo,
|  | const int16_t | sleep = `-1`
| ) |  |

private

Send an Argo A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRArgoAC object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | sleep | Nr. of minutes for sleep mode.

Note
  -1 is Off, >= 0 is on.

## boolToString()

String IRac::boolToString | ( | const bool | value | ) |

static

Convert the supplied boolean into the appropriate String.

Parameters

  [in] | value | The boolean value to be converted.

Returns
  The equivalent String for the locale.

## carrier64()

void IRac::carrier64 | ( | IRCarrierAc64 * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const int16_t | sleep = `-1`
| ) |  |

private

Send a Carrier 64-bit A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRCarrierAc64 object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | sleep | Nr. of minutes for sleep mode.

Note
  -1 is Off, >= 0 is on.

## cleanState()

stdAc::state_t IRac::cleanState | ( | const stdAc::state_t | state | ) |

staticprivate

Create a new state base on the provided state that has been suitably fixed.

Note
  This is for use with Home Assistant, which requires mode to be off if the power is off.

Parameters

  [in] | state | The state_t structure describing the desired a/c state.

Returns
  A stdAc::state_t with the needed settings.

## cmpStates()

bool IRac::cmpStates | ( | const stdAc::state_t | a,
|  | const stdAc::state_t | b
| ) |  |

static

Compare two AirCon states.

Note
  The comparison excludes the clock.

Parameters

  a | A state_t to be compared.
  b | A state_t to be compared.

Returns
  True if they differ, False if they don't.

## coolix()

void IRac::coolix | ( | IRCoolixAC * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | turbo,
|  | const bool | light,
|  | const bool | clean,
|  | const int16_t | sleep = `-1`
| ) |  |

private

Send a Coolix A/C message with the supplied settings.

Note
  May result in multiple messages being sent.

Parameters

  [in,out] | ac | A Ptr to an IRCoolixAC object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | light | Turn on the LED/Display mode.
  [in] | clean | Turn on the self-cleaning mode. e.g. Mould, dry filters etc
  [in] | sleep | Nr. of minutes for sleep mode.

Note
  -1 is Off, >= 0 is on.

## corona()

void IRac::corona | ( | IRCoronaAc * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const bool | econo
| ) |  |

private

Send a Corona A/C message with the supplied settings.

Note
  May result in multiple messages being sent.

Parameters

  [in,out] | ac | A Ptr to an IRCoronaAc object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | econo | Run the device in economical mode.

## daikin()

void IRac::daikin | ( | IRDaikinESP * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | quiet,
|  | const bool | turbo,
|  | const bool | econo,
|  | const bool | clean
| ) |  |

private

Send a Daikin A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRDaikinESP object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | quiet | Run the device in quiet/silent mode.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | econo | Run the device in economical mode.
  [in] | clean | Turn on the self-cleaning mode. e.g. Mould, dry filters etc

## daikin128()

void IRac::daikin128 | ( | IRDaikin128 * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const bool | quiet,
|  | const bool | turbo,
|  | const bool | light,
|  | const bool | econo,
|  | const int16_t | sleep = `-1`,
|  | const int16_t | clock = `-1`
| ) |  |

private

Send a Daikin 128-bit A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRDaikin128 object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | quiet | Run the device in quiet/silent mode.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | light | Turn on the LED/Display mode.
  [in] | econo | Run the device in economical mode.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.
  [in] | clock | The time in Nr. of mins since midnight. < 0 is ignore.

## daikin152()

void IRac::daikin152 | ( | IRDaikin152 * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const bool | quiet,
|  | const bool | turbo,
|  | const bool | econo
| ) |  |

private

Send a Daikin 152-bit A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRDaikin152 object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | quiet | Run the device in quiet/silent mode.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | econo | Run the device in economical mode.

## daikin160()

void IRac::daikin160 | ( | IRDaikin160 * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv
| ) |  |

private

Send a Daikin 160-bit A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRDaikin160 object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.

## daikin176()

void IRac::daikin176 | ( | IRDaikin176 * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingh_t | swingh
| ) |  |

private

Send a Daikin 176-bit A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRDaikin176 object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingh | The horizontal swing setting.

## daikin2()

void IRac::daikin2 | ( | IRDaikin2 * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | quiet,
|  | const bool | turbo,
|  | const bool | light,
|  | const bool | econo,
|  | const bool | filter,
|  | const bool | clean,
|  | const bool | beep,
|  | const int16_t | sleep = `-1`,
|  | const int16_t | clock = `-1`
| ) |  |

private

Send a Daikin2 A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRDaikin2 object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | quiet | Run the device in quiet/silent mode.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | light | Turn on the LED/Display mode.
  [in] | econo | Run the device in economical mode.
  [in] | filter | Turn on the (ion/pollen/etc) filter mode.
  [in] | clean | Turn on the self-cleaning mode. e.g. Mould, dry filters etc
  [in] | beep | Enable/Disable beeps when receiving IR messages.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.
  [in] | clock | The time in Nr. of mins since midnight. < 0 is ignore.

## daikin216()

void IRac::daikin216 | ( | IRDaikin216 * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | quiet,
|  | const bool | turbo
| ) |  |

private

Send a Daikin 216-bit A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRDaikin216 object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | quiet | Run the device in quiet/silent mode.
  [in] | turbo | Run the device in turbo/powerful mode.

## daikin64()

void IRac::daikin64 | ( | IRDaikin64 * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const bool | quiet,
|  | const bool | turbo,
|  | const int16_t | sleep = `-1`,
|  | const int16_t | clock = `-1`
| ) |  |

private

Send a Daikin 64-bit A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRDaikin64 object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | quiet | Run the device in quiet/silent mode.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.
  [in] | clock | The time in Nr. of mins since midnight. < 0 is ignore.

## delonghiac()

void IRac::delonghiac | ( | IRDelonghiAc * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const bool | celsius,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const bool | turbo,
|  | const int16_t | sleep = `-1`
| ) |  |

private

Send a Delonghi A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRDelonghiAc object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | celsius | Temperature units. True is Celsius, False is Fahrenheit.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.

## electra()

void IRac::electra | ( | IRElectraAc * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | turbo,
|  | const bool | lighttoggle,
|  | const bool | clean
| ) |  |

private

Send an Electra A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRElectraAc object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | lighttoggle | Should we toggle the LED/Display?
  [in] | clean | Turn on the self-cleaning mode. e.g. Mould, dry filters etc

## fanspeedToString()

String IRac::fanspeedToString | ( | const stdAc::fanspeed_t | speed | ) |

static

Convert the supplied fan speed enum into the appropriate String.

Parameters

  [in] | speed | The enum to be converted.

Returns
  The equivalent String for the locale.

## fujitsu()

void IRac::fujitsu | ( | IRFujitsuAC * | ac,
|  | const fujitsu_ac_remote_model_t | model,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | quiet,
|  | const bool | turbo,
|  | const bool | econo,
|  | const bool | filter,
|  | const bool | clean,
|  | const int16_t | sleep = `-1`
| ) |  |

private

Send a Fujitsu A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRFujitsuAC object to use.
  [in] | model | The A/C model to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | quiet | Run the device in quiet/silent mode.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | econo | Run the device in economical mode.
  [in] | filter | Turn on the (ion/pollen/etc) filter mode.
  [in] | clean | Turn on the self-cleaning mode. e.g. Mould, dry filters etc
  [in] | sleep | Nr. of minutes for sleep mode. <= 0 is Off, > 0 is on.

## getState()

stdAc::state_t IRac::getState | ( | void |  | ) |

Get the current internal A/C climate state.

Returns
  A Ptr to a state containing the current (to be sent) settings.

## getStatePrev()

stdAc::state_t IRac::getStatePrev | ( | void |  | ) |

Get the previous internal A/C climate state that should have already been sent to the device. i.e. What the A/C unit should already be set to.

Returns
  A Ptr to a state containing the previously sent settings.

## goodweather()

void IRac::goodweather | ( | IRGoodweatherAc * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const bool | turbo,
|  | const bool | light,
|  | const int16_t | sleep = `-1`
| ) |  |

private

Send a Goodweather A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRGoodweatherAc object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | light | Turn on the LED/Display mode.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.

## gree()

void IRac::gree | ( | IRGreeAC * | ac,
|  | const gree_ac_remote_model_t | model,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const bool | celsius,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const bool | turbo,
|  | const bool | light,
|  | const bool | clean,
|  | const int16_t | sleep = `-1`
| ) |  |

private

Send a Gree A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRGreeAC object to use.
  [in] | model | The A/C model to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | celsius | Temperature units. True is Celsius, False is Fahrenheit.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | light | Turn on the LED/Display mode.
  [in] | clean | Turn on the self-cleaning mode. e.g. Mould, dry filters etc
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.

## haier()

void IRac::haier | ( | IRHaierAC * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const bool | filter,
|  | const int16_t | sleep = `-1`,
|  | const int16_t | clock = `-1`
| ) |  |

private

Send a Haier A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRGreeAC object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | filter | Turn on the (ion/pollen/etc) filter mode.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.
  [in] | clock | The time in Nr. of mins since midnight. < 0 is ignore.

## haierYrwo2()

void IRac::haierYrwo2 | ( | IRHaierACYRW02 * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const bool | turbo,
|  | const bool | filter,
|  | const int16_t | sleep = `-1`
| ) |  |

private

Send a Haier YRWO2 A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRHaierACYRW02 object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | filter | Turn on the (ion/pollen/etc) filter mode.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.

## handleToggles()

stdAc::state_t IRac::handleToggles | ( | const stdAc::state_t | desired,
|  | const stdAc::state_t * | prev = `NULL`
| ) |  |

staticprivate

Create a new state base on desired & previous states but handle any state changes for options that need to be toggled.

Parameters

  [in] | desired | The state_t structure describing the desired a/c state.
  [in] | prev | A Ptr to the previous state_t structure.

Returns
  A stdAc::state_t with the needed settings.

## hasStateChanged()

bool IRac::hasStateChanged | ( | void |  | ) |

Check if the internal state has changed from what was previously sent.

Note
  The comparison excludes the clock.

Returns
  True if it has changed, False if not.

## hitachi()

void IRac::hitachi | ( | IRHitachiAc * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh
| ) |  |

private

Send a Hitachi A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRHitachiAc object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.

## hitachi1()

void IRac::hitachi1 | ( | IRHitachiAc1 * | ac,
|  | const hitachi_ac1_remote_model_t | model,
|  | const bool | on,
|  | const bool | power_toggle,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | swing_toggle,
|  | const int16_t | sleep = `-1`
| ) |  |

private

Send a Hitachi1 A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRHitachiAc1 object to use.
  [in] | model | The A/C model to use.
  [in] | on | The power setting.
  [in] | power_toggle | The power toggle setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | swing_toggle | The swing_toggle setting.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.

Note
  The sleep mode used is the "Sleep 2" setting.

## hitachi344()

void IRac::hitachi344 | ( | IRHitachiAc344 * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh
| ) |  |

private

Send a Hitachi 344-bit A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRHitachiAc344 object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.

## hitachi424()

void IRac::hitachi424 | ( | IRHitachiAc424 * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv
| ) |  |

private

Send a Hitachi 424-bit A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRHitachiAc424 object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.

## initState() [1/2]

void IRac::initState | ( | stdAc::state_t * | state | ) |

static

Initialise the given state with the supplied settings.

Parameters

  [out] | state | A Ptr to where the settings will be stored.

Note
  Sets all the parameters to reasonable base/automatic defaults.

## initState() [2/2]

void IRac::initState | ( | stdAc::state_t * | state,
|  | const decode_type_t | vendor,
|  | const int16_t | model,
|  | const bool | power,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const bool | celsius,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | quiet,
|  | const bool | turbo,
|  | const bool | econo,
|  | const bool | light,
|  | const bool | filter,
|  | const bool | clean,
|  | const bool | beep,
|  | const int16_t | sleep,
|  | const int16_t | clock
| ) |  |

static

Initialise the given state with the supplied settings.

Parameters

  [out] | state | A Ptr to where the settings will be stored.
  [in] | vendor | The vendor/protocol type.
  [in] | model | The A/C model if applicable.
  [in] | power | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | celsius | Temperature units. True is Celsius, False is Fahrenheit.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | quiet | Run the device in quiet/silent mode.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | econo | Run the device in economical mode.
  [in] | light | Turn on the LED/Display mode.
  [in] | filter | Turn on the (ion/pollen/etc) filter mode.
  [in] | clean | Turn on the self-cleaning mode. e.g. Mould, dry filters etc
  [in] | beep | Enable/Disable beeps when receiving IR messages.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on. Some devices it is the nr. of mins to run for. Others it may be the time to enter/exit sleep mode. i.e. Time in Nr. of mins since midnight.
  [in] | clock | The time in Nr. of mins since midnight. < 0 is ignore.

## isProtocolSupported()

bool IRac::isProtocolSupported | ( | const decode_type_t | protocol | ) |

static

Is the given protocol supported by the IRac class?

Parameters

  [in] | protocol | The vendor/protocol type.

Returns
  true if the protocol is supported by this class, otherwise false.

## kelvinator()

void IRac::kelvinator | ( | IRKelvinatorAC * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | quiet,
|  | const bool | turbo,
|  | const bool | light,
|  | const bool | filter,
|  | const bool | clean
| ) |  |

private

Send a Kelvinator A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRKelvinatorAC object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | quiet | Run the device in quiet/silent mode.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | light | Turn on the LED/Display mode.
  [in] | filter | Turn on the (ion/pollen/etc) filter mode.
  [in] | clean | Turn on the self-cleaning mode. e.g. XFan, dry filters etc

## lg()

void IRac::lg | ( | IRLgAc * | ac,
|  | const lg_ac_remote_model_t | model,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan
| ) |  |

private

Send a LG A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRLgAc object to use.
  [in] | model | The A/C model to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.

## markAsSent()

void IRac::markAsSent | ( | void |  | ) |

Update the previous state to the current one.

## midea()

void IRac::midea | ( | IRMideaAC * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const bool | celsius,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const bool | turbo,
|  | const bool | econo,
|  | const bool | light,
|  | const int16_t | sleep = `-1`
| ) |  |

private

Send a Midea A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRMideaAC object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | celsius | Temperature units. True is Celsius, False is Fahrenheit.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | turbo | Toggle the device's turbo/powerful mode.
  [in] | econo | Toggle the device's economical mode.
  [in] | light | Toggle the LED/Display mode.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.

Note
  On Danby A/C units, swingv controls the Ion Filter instead.

## mitsubishi()

void IRac::mitsubishi | ( | IRMitsubishiAC * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | quiet,
|  | const int16_t | clock = `-1`
| ) |  |

private

Send a Mitsubishi A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRMitsubishiAC object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | quiet | Run the device in quiet/silent mode.
  [in] | clock | The time in Nr. of mins since midnight. < 0 is ignore.

Note
  Clock can only be set in 10 minute increments. i.e. % 10.

## mitsubishi112()

void IRac::mitsubishi112 | ( | IRMitsubishi112 * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | quiet
| ) |  |

private

Send a Mitsubishi 112-bit A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRMitsubishi112 object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | quiet | Run the device in quiet/silent mode.

## mitsubishi136()

void IRac::mitsubishi136 | ( | IRMitsubishi136 * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const bool | quiet
| ) |  |

private

Send a Mitsubishi 136-bit A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRMitsubishi136 object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | quiet | Run the device in quiet/silent mode.

## mitsubishiHeavy152()

void IRac::mitsubishiHeavy152 | ( | IRMitsubishiHeavy152Ac * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | quiet,
|  | const bool | turbo,
|  | const bool | econo,
|  | const bool | filter,
|  | const bool | clean,
|  | const int16_t | sleep = `-1`
| ) |  |

private

Send a Mitsubishi Heavy 152-bit A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRMitsubishiHeavy152Ac object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | quiet | Run the device in quiet/silent mode.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | econo | Run the device in economical mode.
  [in] | filter | Turn on the (ion/pollen/etc) filter mode.
  [in] | clean | Turn on the self-cleaning mode. e.g. Mould, dry filters etc
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.

## mitsubishiHeavy88()

void IRac::mitsubishiHeavy88 | ( | IRMitsubishiHeavy88Ac * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | turbo,
|  | const bool | econo,
|  | const bool | clean
| ) |  |

private

Send a Mitsubishi Heavy 88-bit A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRMitsubishiHeavy88Ac object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | econo | Run the device in economical mode.
  [in] | clean | Turn on the self-cleaning mode. e.g. Mould, dry filters etc

## neoclima()

void IRac::neoclima | ( | IRNeoclimaAc * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const bool | celsius,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | turbo,
|  | const bool | econo,
|  | const bool | light,
|  | const bool | filter,
|  | const int16_t | sleep = `-1`
| ) |  |

private

Send a Neoclima A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRNeoclimaAc object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | celsius | Temperature units. True is Celsius, False is Fahrenheit.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | econo | Run the device in economical mode.
  [in] | light | Turn on the LED/Display mode.
  [in] | filter | Turn on the (ion/pollen/etc) filter mode.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.

## opmodeToString()

String IRac::opmodeToString | ( | const stdAc::opmode_t | mode | ) |

static

Convert the supplied operation mode into the appropriate String.

Parameters

  [in] | mode | The enum to be converted.

Returns
  The equivalent String for the locale.

## panasonic()

void IRac::panasonic | ( | IRPanasonicAc * | ac,
|  | const panasonic_ac_remote_model_t | model,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | quiet,
|  | const bool | turbo,
|  | const bool | filter,
|  | const int16_t | clock = `-1`
| ) |  |

private

Send a Panasonic A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRPanasonicAc object to use.
  [in] | model | The A/C model to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | quiet | Run the device in quiet/silent mode.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | filter | Turn on the (ion/pollen/etc) filter mode.
  [in] | clock | The time in Nr. of mins since midnight. < 0 is ignore.

## samsung()

void IRac::samsung | ( | IRSamsungAc * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const bool | quiet,
|  | const bool | turbo,
|  | const bool | light,
|  | const bool | filter,
|  | const bool | clean,
|  | const bool | beep,
|  | const bool | prevpower = `true`,
|  | const bool | forcepower = `true`
| ) |  |

private

Send a Samsung A/C message with the supplied settings.

Note
  Multiple IR messages may be generated & sent.

Parameters

  [in,out] | ac | A Ptr to an IRSamsungAc object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | quiet | Run the device in quiet/silent mode.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | light | Turn on the LED/Display mode.
  [in] | filter | Turn on the (ion/pollen/etc) filter mode.
  [in] | clean | Turn on the self-cleaning mode. e.g. Mould, dry filters etc
  [in] | beep | Enable/Disable beeps when receiving IR messages.
  [in] | prevpower | The power setting from the previous A/C state.
  [in] | forcepower | Do we force send the special power message?

## sanyo()

void IRac::sanyo | ( | IRSanyoAc * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const bool | beep,
|  | const int16_t | sleep = `-1`
| ) |  |

private

Send a Toshiba A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRSanyoAc object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | beep | Enable/Disable beeps when receiving IR messages.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.

## sendAc() [1/3]

bool IRac::sendAc | ( | const decode_type_t | vendor,
|  | const int16_t | model,
|  | const bool | power,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const bool | celsius,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | quiet,
|  | const bool | turbo,
|  | const bool | econo,
|  | const bool | light,
|  | const bool | filter,
|  | const bool | clean,
|  | const bool | beep,
|  | const int16_t | sleep = `-1`,
|  | const int16_t | clock = `-1`
| ) |  |

Send A/C message for a given device using common A/C settings.

Parameters

  [in] | vendor | The vendor/protocol type.
  [in] | model | The A/C model if applicable.
  [in] | power | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | celsius | Temperature units. True is Celsius, False is Fahrenheit.
  [in] | fan | The speed setting for the fan.

Note
  The following are all "if supported" by the underlying A/C classes.

Parameters

  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | quiet | Run the device in quiet/silent mode.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | econo | Run the device in economical mode.
  [in] | light | Turn on the LED/Display mode.
  [in] | filter | Turn on the (ion/pollen/etc) filter mode.
  [in] | clean | Turn on the self-cleaning mode. e.g. Mould, dry filters etc
  [in] | beep | Enable/Disable beeps when receiving IR messages.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on. Some devices it is the nr. of mins to run for. Others it may be the time to enter/exit sleep mode. i.e. Time in Nr. of mins since midnight.
  [in] | clock | The time in Nr. of mins since midnight. < 0 is ignore.

Returns
  True, if accepted/converted/attempted etc. False, if unsupported.

## sendAc() [2/3]

bool IRac::sendAc | ( | const stdAc::state_t | desired,
|  | const stdAc::state_t * | prev = `NULL`
| ) |  |

Send A/C message for a given device using state_t structures.

Parameters

  [in] | desired | The state_t structure describing the desired new ac state
  [in] | prev | A Ptr to the state_t structure containing the previous state

Returns
  True, if accepted/converted/attempted etc. False, if unsupported.

## sendAc() [3/3]

bool IRac::sendAc | ( | void |  | ) |

Send an A/C message based soley on our internal state.

Returns
  True, if accepted/converted/attempted. False, if unsupported.

## sharp()

void IRac::sharp | ( | IRSharpAc * | ac,
|  | const sharp_ac_remote_model_t | model,
|  | const bool | on,
|  | const bool | prev_power,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const bool | turbo,
|  | const bool | light,
|  | const bool | filter,
|  | const bool | clean
| ) |  |

private

Send a Sharp A/C message with the supplied settings.

Note
  Multiple IR messages may be generated & sent.

Parameters

  [in,out] | ac | A Ptr to an IRSharpAc object to use.
  [in] | model | The A/C model to use.
  [in] | on | The power setting.
  [in] | prev_power | The power setting from the previous A/C state.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | light | Turn on the LED/Display mode.
  [in] | filter | Turn on the (ion/pollen/etc) filter mode.
  [in] | clean | Turn on the self-cleaning mode. e.g. Mould, dry filters etc

## strToBool()

bool IRac::strToBool | ( | const char * | str,
|  | const bool | def = `false`
| ) |  |

static

Convert the supplied str into the appropriate boolean value.

Parameters

  [in] | str | A Ptr to a C-style string to be converted.
  [in] | def | The boolean value to return if no conversion was possible.

Returns
  The equivalent boolean value.

## strToFanspeed()

stdAc::fanspeed_t IRac::strToFanspeed | ( | const char * | str,
|  | const stdAc::fanspeed_t | def = `stdAc::fanspeed_t::kAuto`
| ) |  |

static

Convert the supplied str into the appropriate enum.

Parameters

  [in] | str | A Ptr to a C-style string to be converted.
  [in] | def | The enum to return if no conversion was possible.

Returns
  The equivalent enum.

## strToModel()

int16_t IRac::strToModel | ( | const char * | str,
|  | const int16_t | def = `-1`
| ) |  |

static

Convert the supplied str into the appropriate enum.

Note
  Assumes str is the model code or an integer >= 1.

Parameters

  [in] | str | A Ptr to a C-style string to be converted.
  [in] | def | The enum to return if no conversion was possible.

Returns
  The equivalent enum.

## strToOpmode()

stdAc::opmode_t IRac::strToOpmode | ( | const char * | str,
|  | const stdAc::opmode_t | def = `stdAc::opmode_t::kAuto`
| ) |  |

static

Convert the supplied str into the appropriate enum.

Parameters

  [in] | str | A Ptr to a C-style string to be converted.
  [in] | def | The enum to return if no conversion was possible.

Returns
  The equivalent enum.

## strToSwingH()

stdAc::swingh_t IRac::strToSwingH | ( | const char * | str,
|  | const stdAc::swingh_t | def = `stdAc::swingh_t::kOff`
| ) |  |

static

Convert the supplied str into the appropriate enum.

Parameters

  [in] | str | A Ptr to a C-style string to be converted.
  [in] | def | The enum to return if no conversion was possible.

Returns
  The equivalent enum.

## strToSwingV()

stdAc::swingv_t IRac::strToSwingV | ( | const char * | str,
|  | const stdAc::swingv_t | def = `stdAc::swingv_t::kOff`
| ) |  |

static

Convert the supplied str into the appropriate enum.

Parameters

  [in] | str | A Ptr to a C-style string to be converted.
  [in] | def | The enum to return if no conversion was possible.

Returns
  The equivalent enum.

## swinghToString()

String IRac::swinghToString | ( | const stdAc::swingh_t | swingh | ) |

static

Convert the supplied enum into the appropriate String.

Parameters

  [in] | swingh | The enum to be converted.

Returns
  The equivalent String for the locale.

## swingvToString()

String IRac::swingvToString | ( | const stdAc::swingv_t | swingv | ) |

static

Convert the supplied enum into the appropriate String.

Parameters

  [in] | swingv | The enum to be converted.

Returns
  The equivalent String for the locale.

## tcl112()

void IRac::tcl112 | ( | IRTcl112Ac * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | turbo,
|  | const bool | light,
|  | const bool | econo,
|  | const bool | filter
| ) |  |

private

Send a TCL 112-bit A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRTcl112Ac object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | light | Turn on the LED/Display mode.
  [in] | econo | Run the device in economical mode.
  [in] | filter | Turn on the (ion/pollen/etc) filter mode.

## technibel()

void IRac::technibel | ( | IRTechnibelAc * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const bool | celsius,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const int16_t | sleep = `-1`
| ) |  |

private

Send a Technibel A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRTechnibelAc object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | celsius | Temperature units. True is Celsius, False is Fahrenheit.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.

## teco()

void IRac::teco | ( | IRTecoAc * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const bool | light,
|  | const int16_t | sleep = `-1`
| ) |  |

private

Send a Teco A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRTecoAc object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | light | Turn on the LED/Display mode.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.

## toshiba()

void IRac::toshiba | ( | IRToshibaAC * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const bool | turbo,
|  | const bool | econo
| ) |  |

private

Send a Toshiba A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRToshibaAC object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | econo | Run the device in economical mode.

## transcold()

void IRac::transcold | ( | IRTranscoldAc * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh
| ) |  |

private

Send a Transcold A/C message with the supplied settings.

Note
  May result in multiple messages being sent.

Parameters

  [in,out] | ac | A Ptr to an IRTranscoldAc object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.

Note
  -1 is Off, >= 0 is on.

## trotec()

void IRac::trotec | ( | IRTrotecESP * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const int16_t | sleep = `-1`
| ) |  |

private

Send a Trotec A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRTrotecESP object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.

## vestel()

void IRac::vestel | ( | IRVestelAc * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const bool | turbo,
|  | const bool | filter,
|  | const int16_t | sleep = `-1`,
|  | const int16_t | clock = `-1`,
|  | const bool | sendNormal = `true`
| ) |  |

private

Send a Vestel A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRVestelAc object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | filter | Turn on the (ion/pollen/etc) filter mode.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.
  [in] | clock | The time in Nr. of mins since midnight. < 0 is ignore.
  [in] | sendNormal | Do we send a Normal settings message at all? i.e In addition to the clock/time/timer message

## voltas()

void IRac::voltas | ( | IRVoltas * | ac,
|  | const voltas_ac_remote_model_t | model,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | turbo,
|  | const bool | econo,
|  | const bool | light,
|  | const int16_t | sleep = `-1`
| ) |  |

private

Send a Voltas A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRVoltas object to use.
  [in] | model | The A/C model to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | econo | Run the device in economical mode.
  [in] | light | Turn on the LED/Display mode.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.

## whirlpool()

void IRac::whirlpool | ( | IRWhirlpoolAc * | ac,
|  | const whirlpool_ac_remote_model_t | model,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const bool | turbo,
|  | const bool | light,
|  | const int16_t | sleep = `-1`,
|  | const int16_t | clock = `-1`
| ) |  |

private

Send a Whirlpool A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRWhirlpoolAc object to use.
  [in] | model | The A/C model to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | light | Turn on the LED/Display mode.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.
  [in] | clock | The time in Nr. of mins since midnight. < 0 is ignore.

## Member Data Documentation

## _inverted

bool IRac::_inverted

private

IR LED is lit when GPIO is LOW (true) or HIGH (false)?

## _modulation

bool IRac::_modulation

private

Is frequency modulation to be used?

## _pin

uint16_t IRac::_pin

private

The GPIO to use to transmit messages from.

## _prev

stdAc::state_t IRac::_prev

private

The state we expect the device to currently be in.

## next

stdAc::state_t IRac::next

The state we want the device to be in after we send.

The documentation for this class was generated from the following files:

- src/IRac.h
- src/IRac.cpp