# IRremoteESP8266: CoronaProtocol Union Reference

CoronaProtocol Union Reference

Native representation of a Corona A/C message. More...

`#include <ir_Corona.h>`

Collaboration diagram for CoronaProtocol:
[legend]

## Public Attributes

uint8_t | raw [kCoronaAcStateLength]
| The state of the IR remote. More...
CoronaSection | sections [kCoronaAcSections]
struct {
uint8_t __pad0__:8
uint8_t __pad1__:8
uint8_t __pad2__:8
uint8_t Fan:2
uint8_t __pad3__:1
uint8_t Econo:1
uint8_t __pad4__:1
uint8_t __pad5__:1
uint8_t SwingVToggle:1
uint8_t __pad6__:1
uint8_t __pad7__:8
uint8_t Temp:4
uint8_t Power:1
uint8_t PowerButton:1
uint8_t Mode:2
}; |

## Detailed Description

Native representation of a Corona A/C message.

## Member Data Documentation

## @11

struct { ... }

## __pad0__

uint8_t CoronaProtocol::__pad0__

## __pad1__

uint8_t CoronaProtocol::__pad1__

## __pad2__

uint8_t CoronaProtocol::__pad2__

## __pad3__

uint8_t CoronaProtocol::__pad3__

## __pad4__

uint8_t CoronaProtocol::__pad4__

## __pad5__

uint8_t CoronaProtocol::__pad5__

## __pad6__

uint8_t CoronaProtocol::__pad6__

## __pad7__

uint8_t CoronaProtocol::__pad7__

## Econo

uint8_t CoronaProtocol::Econo

## Fan

uint8_t CoronaProtocol::Fan

## Mode

uint8_t CoronaProtocol::Mode

## Power

uint8_t CoronaProtocol::Power

## PowerButton

uint8_t CoronaProtocol::PowerButton

## raw

uint8_t CoronaProtocol::raw[kCoronaAcStateLength]

The state of the IR remote.

## sections

CoronaSection CoronaProtocol::sections[kCoronaAcSections]

## SwingVToggle

uint8_t CoronaProtocol::SwingVToggle

## Temp

uint8_t CoronaProtocol::Temp

The documentation for this union was generated from the following file:

- src/ir_Corona.h