# IRremoteESP8266: Daikin216Protocol Union Reference

Daikin216Protocol Union Reference

Native representation of a Daikin216 A/C message. More...

`#include <ir_Daikin.h>`

## Public Attributes

uint8_t | raw [kDaikin216StateLength]
| The state of the IR remote. More...
struct {
uint8_t pad0 [7]
uint8_t Sum1:8
uint8_t pad1 [5]
uint8_t Power:1
uint8_t __pad0__:3
uint8_t Mode:3
uint8_t __pad1__:1
uint8_t __pad2__:1
uint8_t Temp:6
uint8_t __pad3__:1
uint8_t __pad4__:8
uint8_t SwingV:4
uint8_t Fan:4
uint8_t SwingH:4
uint8_t __pad5__:4
uint8_t pad2 [3]
uint8_t Powerful:1
uint8_t __pad6__:0
uint8_t pad3 [4]
uint8_t Sum2:8
}; |

## Detailed Description

Native representation of a Daikin216 A/C message.

## Member Data Documentation

## @19

struct { ... }

## __pad0__

uint8_t Daikin216Protocol::__pad0__

## __pad1__

uint8_t Daikin216Protocol::__pad1__

## __pad2__

uint8_t Daikin216Protocol::__pad2__

## __pad3__

uint8_t Daikin216Protocol::__pad3__

## __pad4__

uint8_t Daikin216Protocol::__pad4__

## __pad5__

uint8_t Daikin216Protocol::__pad5__

## __pad6__

uint8_t Daikin216Protocol::__pad6__

## Fan

uint8_t Daikin216Protocol::Fan

## Mode

uint8_t Daikin216Protocol::Mode

## pad0

uint8_t Daikin216Protocol::pad0[7]

## pad1

uint8_t Daikin216Protocol::pad1[5]

## pad2

uint8_t Daikin216Protocol::pad2[3]

## pad3

uint8_t Daikin216Protocol::pad3[4]

## Power

uint8_t Daikin216Protocol::Power

## Powerful

uint8_t Daikin216Protocol::Powerful

## raw

uint8_t Daikin216Protocol::raw[kDaikin216StateLength]

The state of the IR remote.

## Sum1

uint8_t Daikin216Protocol::Sum1

## Sum2

uint8_t Daikin216Protocol::Sum2

## SwingH

uint8_t Daikin216Protocol::SwingH

## SwingV

uint8_t Daikin216Protocol::SwingV

## Temp

uint8_t Daikin216Protocol::Temp

The documentation for this union was generated from the following file:

- src/ir_Daikin.h