# IRremoteESP8266: Mitsubishi88Protocol Union Reference

Mitsubishi88Protocol Union Reference

Native representation of a Mitsubishi Heavy 88-bit A/C message. More...

`#include <ir_MitsubishiHeavy.h>`

## Public Attributes

uint8_t | raw [kMitsubishiHeavy88StateLength]
| State in code form. More...
struct {
uint8_t Sig [5]
uint8_t __pad0__:1
uint8_t SwingV5:1
uint8_t SwingH1:2
uint8_t __pad1__:1
uint8_t Clean:1
uint8_t SwingH2:2
uint8_t __pad2__:8
uint8_t __pad3__:3
uint8_t SwingV7:2
uint8_t Fan:3
uint8_t __pad4__:8
uint8_t Mode:3
uint8_t Power:1
uint8_t Temp:4
}; |

## Detailed Description

Native representation of a Mitsubishi Heavy 88-bit A/C message.

## Member Data Documentation

## @64

struct { ... }

## __pad0__

uint8_t Mitsubishi88Protocol::__pad0__

## __pad1__

uint8_t Mitsubishi88Protocol::__pad1__

## __pad2__

uint8_t Mitsubishi88Protocol::__pad2__

## __pad3__

uint8_t Mitsubishi88Protocol::__pad3__

## __pad4__

uint8_t Mitsubishi88Protocol::__pad4__

## Clean

uint8_t Mitsubishi88Protocol::Clean

## Fan

uint8_t Mitsubishi88Protocol::Fan

## Mode

uint8_t Mitsubishi88Protocol::Mode

## Power

uint8_t Mitsubishi88Protocol::Power

## raw

uint8_t Mitsubishi88Protocol::raw[kMitsubishiHeavy88StateLength]

State in code form.

## Sig

uint8_t Mitsubishi88Protocol::Sig[5]

## SwingH1

uint8_t Mitsubishi88Protocol::SwingH1

## SwingH2

uint8_t Mitsubishi88Protocol::SwingH2

## SwingV5

uint8_t Mitsubishi88Protocol::SwingV5

## SwingV7

uint8_t Mitsubishi88Protocol::SwingV7

## Temp

uint8_t Mitsubishi88Protocol::Temp

The documentation for this union was generated from the following file:

- src/ir_MitsubishiHeavy.h