# IRremoteESP8266: Member List

IRDaikin2 Member List

This is the complete list of members for IRDaikin2, including all inherited members.

_ | IRDaikin2 | private
_irsend | IRDaikin2 | private
begin(void) | IRDaikin2 |
calibrate(void) | IRDaikin2 | inline
checksum(void) | IRDaikin2 | private
clearOnTimerFlag(void) | IRDaikin2 | private
clearSleepTimerFlag(void) | IRDaikin2 | private
convertFan(const stdAc::fanspeed_t speed) | IRDaikin2 | static
convertMode(const stdAc::opmode_t mode) | IRDaikin2 | static
convertSwingH(const stdAc::swingh_t position) | IRDaikin2 | static
convertSwingV(const stdAc::swingv_t position) | IRDaikin2 | static
disableOffTimer(void) | IRDaikin2 |
disableOnTimer(void) | IRDaikin2 |
disableSleepTimer(void) | IRDaikin2 |
enableOffTimer(const uint16_t endtime) | IRDaikin2 |
enableOnTimer(const uint16_t starttime) | IRDaikin2 |
enableSleepTimer(const uint16_t sleeptime) | IRDaikin2 |
getBeep(void) const | IRDaikin2 |
getClean(void) const | IRDaikin2 |
getCurrentTime(void) const | IRDaikin2 |
getEcono(void) const | IRDaikin2 |
getEye(void) const | IRDaikin2 |
getEyeAuto(void) const | IRDaikin2 |
getFan(void) const | IRDaikin2 |
getFreshAir(void) const | IRDaikin2 |
getFreshAirHigh(void) const | IRDaikin2 |
getLight(void) const | IRDaikin2 |
getMode(void) const | IRDaikin2 |
getMold(void) const | IRDaikin2 |
getOffTime(void) const | IRDaikin2 |
getOffTimerEnabled(void) const | IRDaikin2 |
getOnTime(void) const | IRDaikin2 |
getOnTimerEnabled(void) const | IRDaikin2 |
getPower(void) const | IRDaikin2 |
getPowerful(void) const | IRDaikin2 |
getPurify(void) const | IRDaikin2 |
getQuiet(void) const | IRDaikin2 |
getRaw(void) | IRDaikin2 |
getSleepTime(void) const | IRDaikin2 |
getSleepTimerEnabled(void) const | IRDaikin2 |
getSwingHorizontal(void) const | IRDaikin2 |
getSwingVertical(void) const | IRDaikin2 |
getTemp(void) const | IRDaikin2 |
IRDaikin2(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRDaikin2 | explicit
off(void) | IRDaikin2 |
on(void) | IRDaikin2 |
send(const uint16_t repeat=kDaikin2DefaultRepeat) | IRDaikin2 |
setBeep(const uint8_t beep) | IRDaikin2 |
setClean(const bool on) | IRDaikin2 |
setCurrentTime(const uint16_t time) | IRDaikin2 |
setEcono(const bool on) | IRDaikin2 |
setEye(const bool on) | IRDaikin2 |
setEyeAuto(const bool on) | IRDaikin2 |
setFan(const uint8_t fan) | IRDaikin2 |
setFreshAir(const bool on) | IRDaikin2 |
setFreshAirHigh(const bool on) | IRDaikin2 |
setLight(const uint8_t light) | IRDaikin2 |
setMode(const uint8_t mode) | IRDaikin2 |
setMold(const bool on) | IRDaikin2 |
setPower(const bool state) | IRDaikin2 |
setPowerful(const bool on) | IRDaikin2 |
setPurify(const bool on) | IRDaikin2 |
setQuiet(const bool on) | IRDaikin2 |
setRaw(const uint8_t new_code[]) | IRDaikin2 |
setSwingHorizontal(const uint8_t position) | IRDaikin2 |
setSwingVertical(const uint8_t position) | IRDaikin2 |
setTemp(const uint8_t temp) | IRDaikin2 |
stateReset(void) | IRDaikin2 | private
toCommon(void) const | IRDaikin2 |
toCommonSwingH(const uint8_t setting) | IRDaikin2 | static
toCommonSwingV(const uint8_t setting) | IRDaikin2 | static
toString(void) const | IRDaikin2 |
validChecksum(uint8_t state[], const uint16_t length=kDaikin2StateLength) | IRDaikin2 | static