# IRremoteESP8266: Daikin176Protocol Union Reference

Daikin176Protocol Union Reference

Native representation of a Daikin176 A/C message. More...

`#include <ir_Daikin.h>`

## Public Attributes

uint8_t | raw [kDaikin176StateLength]
| The state of the IR remote. More...
struct {
uint8_t pad0 [6]
uint8_t Sum1:8
uint8_t pad1 [5]
uint8_t __pad0__:4
uint8_t AltMode:3
uint8_t __pad1__:1
uint8_t ModeButton:8
uint8_t Power:1
uint8_t __pad2__:3
uint8_t Mode:3
uint8_t __pad3__:1
uint8_t pad2 [2]
uint8_t __pad4__:1
uint8_t Temp:6
uint8_t __pad5__:1
uint8_t SwingH:4
uint8_t Fan:4
uint8_t pad3 [2]
uint8_t Sum2:8
}; |

## Detailed Description

Native representation of a Daikin176 A/C message.

## Member Data Documentation

## @23

struct { ... }

## __pad0__

uint8_t Daikin176Protocol::__pad0__

## __pad1__

uint8_t Daikin176Protocol::__pad1__

## __pad2__

uint8_t Daikin176Protocol::__pad2__

## __pad3__

uint8_t Daikin176Protocol::__pad3__

## __pad4__

uint8_t Daikin176Protocol::__pad4__

## __pad5__

uint8_t Daikin176Protocol::__pad5__

## AltMode

uint8_t Daikin176Protocol::AltMode

## Fan

uint8_t Daikin176Protocol::Fan

## Mode

uint8_t Daikin176Protocol::Mode

## ModeButton

uint8_t Daikin176Protocol::ModeButton

## pad0

uint8_t Daikin176Protocol::pad0[6]

## pad1

uint8_t Daikin176Protocol::pad1[5]

## pad2

uint8_t Daikin176Protocol::pad2[2]

## pad3

uint8_t Daikin176Protocol::pad3[2]

## Power

uint8_t Daikin176Protocol::Power

## raw

uint8_t Daikin176Protocol::raw[kDaikin176StateLength]

The state of the IR remote.

## Sum1

uint8_t Daikin176Protocol::Sum1

## Sum2

uint8_t Daikin176Protocol::Sum2

## SwingH

uint8_t Daikin176Protocol::SwingH

## Temp

uint8_t Daikin176Protocol::Temp

The documentation for this union was generated from the following file:

- src/ir_Daikin.h