# IRremoteESP8266: Member List

IRSamsungAc Member List

This is the complete list of members for IRSamsungAc, including all inherited members.

_forcepower | IRSamsungAc | private
_irsend | IRSamsungAc | private
_lastsentpowerstate | IRSamsungAc | private
begin(void) | IRSamsungAc |
calcChecksum(const uint8_t state[], const uint16_t length=kSamsungAcStateLength) | IRSamsungAc | static
calibrate(void) | IRSamsungAc | inline
checksum(const uint16_t length=kSamsungAcStateLength) | IRSamsungAc | private
convertFan(const stdAc::fanspeed_t speed) | IRSamsungAc |
convertMode(const stdAc::opmode_t mode) | IRSamsungAc |
getBeep(void) | IRSamsungAc |
getBreeze(void) | IRSamsungAc |
getClean(void) | IRSamsungAc |
getDisplay(void) | IRSamsungAc |
getFan(void) | IRSamsungAc |
getIon(void) | IRSamsungAc |
getMode(void) | IRSamsungAc |
getPower(void) | IRSamsungAc |
getPowerful(void) | IRSamsungAc |
getQuiet(void) | IRSamsungAc |
getRaw(void) | IRSamsungAc |
getSwing(void) | IRSamsungAc |
getTemp(void) | IRSamsungAc |
IRSamsungAc(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRSamsungAc | explicit
off(void) | IRSamsungAc |
on(void) | IRSamsungAc |
remote_state | IRSamsungAc | private
send(const uint16_t repeat=kSamsungAcDefaultRepeat, const bool calcchecksum=true) | IRSamsungAc |
sendExtended(const uint16_t repeat=kSamsungAcDefaultRepeat, const bool calcchecksum=true) | IRSamsungAc |
sendOff(const uint16_t repeat=kSamsungAcDefaultRepeat) | IRSamsungAc |
sendOn(const uint16_t repeat=kSamsungAcDefaultRepeat) | IRSamsungAc |
setBeep(const bool on) | IRSamsungAc |
setBreeze(const bool on) | IRSamsungAc |
setClean(const bool on) | IRSamsungAc |
setDisplay(const bool on) | IRSamsungAc |
setFan(const uint8_t speed) | IRSamsungAc |
setIon(const bool on) | IRSamsungAc |
setMode(const uint8_t mode) | IRSamsungAc |
setPower(const bool on) | IRSamsungAc |
setPowerful(const bool on) | IRSamsungAc |
setQuiet(const bool on) | IRSamsungAc |
setRaw(const uint8_t new_code[], const uint16_t length=kSamsungAcStateLength) | IRSamsungAc |
setSwing(const bool on) | IRSamsungAc |
setTemp(const uint8_t temp) | IRSamsungAc |
stateReset(const bool forcepower=true, const bool initialPower=true) | IRSamsungAc |
toCommon(void) | IRSamsungAc |
toCommonFanSpeed(const uint8_t speed) | IRSamsungAc | static
toCommonMode(const uint8_t mode) | IRSamsungAc | static
toString(void) | IRSamsungAc |
validChecksum(const uint8_t state[], const uint16_t length=kSamsungAcStateLength) | IRSamsungAc | static