# IRremoteESP8266: Hitachi424Protocol Union Reference

Hitachi424Protocol Union Reference

Native representation of a Hitachi 53-byte/424-bit A/C message. More...

`#include <ir_Hitachi.h>`

## Public Attributes

uint8_t | raw [kHitachiAc424StateLength]
| The state in native code. More...
struct {
uint8_t pad0 [11]
uint8_t Button:8
uint8_t __pad0__:8
uint8_t __pad1__:2
uint8_t Temp:6
uint8_t pad1 [11]
uint8_t Mode:4
uint8_t Fan:4
uint8_t __pad2__:8
uint8_t Power:8
uint8_t pad2 [7]
uint8_t SwingH:3
uint8_t __pad3__:5
uint8_t __pad4__:8
uint8_t __pad5__:5
uint8_t SwingV:1
uint8_t __pad6__:2
}; |

## Detailed Description

Native representation of a Hitachi 53-byte/424-bit A/C message.

## Member Data Documentation

## @45

struct { ... }

## __pad0__

uint8_t Hitachi424Protocol::__pad0__

## __pad1__

uint8_t Hitachi424Protocol::__pad1__

## __pad2__

uint8_t Hitachi424Protocol::__pad2__

## __pad3__

uint8_t Hitachi424Protocol::__pad3__

## __pad4__

uint8_t Hitachi424Protocol::__pad4__

## __pad5__

uint8_t Hitachi424Protocol::__pad5__

## __pad6__

uint8_t Hitachi424Protocol::__pad6__

## Button

uint8_t Hitachi424Protocol::Button

## Fan

uint8_t Hitachi424Protocol::Fan

## Mode

uint8_t Hitachi424Protocol::Mode

## pad0

uint8_t Hitachi424Protocol::pad0[11]

## pad1

uint8_t Hitachi424Protocol::pad1[11]

## pad2

uint8_t Hitachi424Protocol::pad2[7]

## Power

uint8_t Hitachi424Protocol::Power

## raw

uint8_t Hitachi424Protocol::raw[kHitachiAc424StateLength]

The state in native code.

## SwingH

uint8_t Hitachi424Protocol::SwingH

## SwingV

uint8_t Hitachi424Protocol::SwingV

## Temp

uint8_t Hitachi424Protocol::Temp

The documentation for this union was generated from the following file:

- src/ir_Hitachi.h