# IRremoteESP8266: Member List

IRCarrierAc64 Member List

This is the complete list of members for IRCarrierAc64, including all inherited members.

_ | IRCarrierAc64 | private
_cancelOffTimer(void) | IRCarrierAc64 | private
_cancelOnTimer(void) | IRCarrierAc64 | private
_irsend | IRCarrierAc64 | private
begin() | IRCarrierAc64 |
calcChecksum(const uint64_t state) | IRCarrierAc64 | static
calibrate(void) | IRCarrierAc64 | inline
checksum(void) | IRCarrierAc64 | private
convertFan(const stdAc::fanspeed_t speed) | IRCarrierAc64 | static
convertMode(const stdAc::opmode_t mode) | IRCarrierAc64 | static
getFan(void) const | IRCarrierAc64 |
getMode(void) const | IRCarrierAc64 |
getOffTimer(void) const | IRCarrierAc64 |
getOnTimer(void) const | IRCarrierAc64 |
getPower(void) const | IRCarrierAc64 |
getRaw(void) | IRCarrierAc64 |
getSleep(void) const | IRCarrierAc64 |
getSwingV(void) const | IRCarrierAc64 |
getTemp(void) const | IRCarrierAc64 |
IRCarrierAc64(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRCarrierAc64 | explicit
off(void) | IRCarrierAc64 |
on(void) | IRCarrierAc64 |
send(const uint16_t repeat=kCarrierAc64MinRepeat) | IRCarrierAc64 |
setFan(const uint8_t speed) | IRCarrierAc64 |
setMode(const uint8_t mode) | IRCarrierAc64 |
setOffTimer(const uint16_t nr_of_mins) | IRCarrierAc64 |
setOnTimer(const uint16_t nr_of_mins) | IRCarrierAc64 |
setPower(const bool on) | IRCarrierAc64 |
setRaw(const uint64_t state) | IRCarrierAc64 |
setSleep(const bool on) | IRCarrierAc64 |
setSwingV(const bool on) | IRCarrierAc64 |
setTemp(const uint8_t temp) | IRCarrierAc64 |
stateReset() | IRCarrierAc64 |
toCommon(void) const | IRCarrierAc64 |
toCommonFanSpeed(const uint8_t speed) | IRCarrierAc64 | static
toCommonMode(const uint8_t mode) | IRCarrierAc64 | static
toString(void) const | IRCarrierAc64 |
validChecksum(const uint64_t state) | IRCarrierAc64 | static