# IRremoteESP8266: IRMitsubishiHeavy152Ac Class Reference

IRMitsubishiHeavy152Ac Class Reference

Class for handling detailed Mitsubishi Heavy 152-bit A/C messages. More...

`#include <ir_MitsubishiHeavy.h>`

Collaboration diagram for IRMitsubishiHeavy152Ac:
[legend]

## Public Member Functions

| IRMitsubishiHeavy152Ac (const uint16_t pin, const bool inverted=false, const bool use_modulation=true)
| Class constructor. More...
void | stateReset (void)
| Reset the state of the remote to a known good state/sequence. More...
void | send (const uint16_t repeat=kMitsubishiHeavy152MinRepeat)
| Send the current internal state as an IR message. More...
int8_t | calibrate (void)
| Run the calibration to calculate uSec timing offsets for this platform. More...
void | begin (void)
| Set up hardware to be able to send a message. More...
void | on (void)
| Set the requested power state of the A/C to on. More...
void | off (void)
| Set the requested power state of the A/C to off. More...
void | setPower (const bool on)
| Change the power setting. More...
bool | getPower (void) const
| Get the value of the current power setting. More...
void | setTemp (const uint8_t temp)
| Set the temperature. More...
uint8_t | getTemp (void) const
| Get the current temperature setting. More...
void | setFan (const uint8_t fan)
| Set the speed of the fan. More...
uint8_t | getFan (void) const
| Get the current fan speed setting. More...
void | setMode (const uint8_t mode)
| Set the operating mode of the A/C. More...
uint8_t | getMode (void) const
| Get the operating mode setting of the A/C. More...
void | setSwingVertical (const uint8_t pos)
| Set the Vertical Swing mode of the A/C. More...
uint8_t | getSwingVertical (void) const
| Get the Vertical Swing mode of the A/C. More...
void | setSwingHorizontal (const uint8_t pos)
| Set the Horizontal Swing mode of the A/C. More...
uint8_t | getSwingHorizontal (void) const
| Get the Horizontal Swing mode of the A/C. More...
void | setNight (const bool on)
| Set the Night (Sleep) mode of the A/C. More...
bool | getNight (void) const
| Get the Night (Sleep) mode of the A/C. More...
void | set3D (const bool on)
| Set the 3D mode of the A/C. More...
bool | get3D (void) const
| Get the 3D mode of the A/C. More...
void | setSilent (const bool on)
| Set the Silent (Quiet) mode of the A/C. More...
bool | getSilent (void) const
| Get the Silent (Quiet) mode of the A/C. More...
void | setFilter (const bool on)
| Set the Filter mode of the A/C. More...
bool | getFilter (void) const
| Get the Filter mode of the A/C. More...
void | setClean (const bool on)
| Set the Clean mode of the A/C. More...
bool | getClean (void) const
| Get the Clean mode of the A/C. More...
void | setTurbo (const bool on)
| Set the Turbo mode of the A/C. More...
bool | getTurbo (void) const
| Get the Turbo mode of the A/C. More...
void | setEcono (const bool on)
| Set the Economical mode of the A/C. More...
bool | getEcono (void) const
| Get the Economical mode of the A/C. More...
uint8_t * | getRaw (void)
| Get a PTR to the internal state/code for this protocol. More...
void | setRaw (const uint8_t *data)
| Set the internal state from a valid code for this protocol. More...
stdAc::state_t | toCommon (void) const
| Convert the current internal state into its stdAc::state_t equivalent. More...
String | toString (void) const
| Convert the internal state into a human readable string. More...

## Static Public Member Functions

static bool | checkZmsSig (const uint8_t *state)
| Verify the given state has a ZM-S signature. More...
static bool | validChecksum (const uint8_t *state, const uint16_t length=kMitsubishiHeavy152StateLength)
| Verify the checksum is valid for a given state. More...
static uint8_t | convertMode (const stdAc::opmode_t mode)
| Convert a stdAc::opmode_t enum into its native mode. More...
static uint8_t | convertFan (const stdAc::fanspeed_t speed)
| Convert a stdAc::fanspeed_t enum into it's native speed. More...
static uint8_t | convertSwingV (const stdAc::swingv_t position)
| Convert a stdAc::swingv_t enum into it's native setting. More...
static uint8_t | convertSwingH (const stdAc::swingh_t position)
| Convert a stdAc::swingh_t enum into it's native setting. More...
static stdAc::opmode_t | toCommonMode (const uint8_t mode)
| Convert a native mode into its stdAc equivalent. More...
static stdAc::fanspeed_t | toCommonFanSpeed (const uint8_t speed)
| Convert a native fan speed into its stdAc equivalent. More...
static stdAc::swingv_t | toCommonSwingV (const uint8_t pos)
| Convert a native vertical swing postion to it's common equivalent. More...
static stdAc::swingh_t | toCommonSwingH (const uint8_t pos)
| Convert a native horizontal swing postion to it's common equivalent. More...

## Private Member Functions

void | checksum (void)
| Calculate the checksum for the current internal state of the remote. Note: Technically it has no checksum, but does have inverted byte pairs. More...

## Private Attributes

IRsend | _irsend
| Instance of the IR send class. More...
Mitsubishi152Protocol | _

## Detailed Description

Class for handling detailed Mitsubishi Heavy 152-bit A/C messages.

## Constructor & Destructor Documentation

## IRMitsubishiHeavy152Ac()

IRMitsubishiHeavy152Ac::IRMitsubishiHeavy152Ac | ( | const uint16_t | pin,
|  | const bool | inverted = `false`,
|  | const bool | use_modulation = `true`
| ) |  |

explicit

Class constructor.

Parameters

  [in] | pin | GPIO to be used when sending.
  [in] | inverted | Is the output signal to be inverted?
  [in] | use_modulation | Is frequency modulation to be used?

## Member Function Documentation

## begin()

void IRMitsubishiHeavy152Ac::begin | ( | void |  | ) |

Set up hardware to be able to send a message.

## calibrate()

int8_t IRMitsubishiHeavy152Ac::calibrate | ( | void |  | ) |

inline

Run the calibration to calculate uSec timing offsets for this platform.

Returns
  The uSec timing offset needed per modulation of the IR Led.

Note
  This will produce a 65ms IR signal pulse at 38kHz. Only ever needs to be run once per object instantiation, if at all.

## checksum()

void IRMitsubishiHeavy152Ac::checksum | ( | void |  | ) |

private

Calculate the checksum for the current internal state of the remote. Note: Technically it has no checksum, but does have inverted byte pairs.

## checkZmsSig()

bool IRMitsubishiHeavy152Ac::checkZmsSig | ( | const uint8_t * | state | ) |

static

Verify the given state has a ZM-S signature.

Parameters

  [in] | state | A ptr to a state to be checked.

Returns
  true, the check passed. Otherwise, false.

## convertFan()

uint8_t IRMitsubishiHeavy152Ac::convertFan | ( | const stdAc::fanspeed_t | speed | ) |

static

Convert a stdAc::fanspeed_t enum into it's native speed.

Parameters

  [in] | speed | The enum to be converted.

Returns
  The native equivalent of the enum.

## convertMode()

uint8_t IRMitsubishiHeavy152Ac::convertMode | ( | const stdAc::opmode_t | mode | ) |

static

Convert a stdAc::opmode_t enum into its native mode.

Parameters

  [in] | mode | The enum to be converted.

Returns
  The native equivalent of the enum.

## convertSwingH()

uint8_t IRMitsubishiHeavy152Ac::convertSwingH | ( | const stdAc::swingh_t | position | ) |

static

Convert a stdAc::swingh_t enum into it's native setting.

Parameters

  [in] | position | The enum to be converted.

Returns
  The native equivalent of the enum.

## convertSwingV()

uint8_t IRMitsubishiHeavy152Ac::convertSwingV | ( | const stdAc::swingv_t | position | ) |

static

Convert a stdAc::swingv_t enum into it's native setting.

Parameters

  [in] | position | The enum to be converted.

Returns
  The native equivalent of the enum.

## get3D()

bool IRMitsubishiHeavy152Ac::get3D | ( | void |  | ) | const

Get the 3D mode of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## getClean()

bool IRMitsubishiHeavy152Ac::getClean | ( | void |  | ) | const

Get the Clean mode of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## getEcono()

bool IRMitsubishiHeavy152Ac::getEcono | ( | void |  | ) | const

Get the Economical mode of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## getFan()

uint8_t IRMitsubishiHeavy152Ac::getFan | ( | void |  | ) | const

Get the current fan speed setting.

Returns
  The current fan speed/mode.

## getFilter()

bool IRMitsubishiHeavy152Ac::getFilter | ( | void |  | ) | const

Get the Filter mode of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## getMode()

uint8_t IRMitsubishiHeavy152Ac::getMode | ( | void |  | ) | const

Get the operating mode setting of the A/C.

Returns
  The current operating mode setting.

## getNight()

bool IRMitsubishiHeavy152Ac::getNight | ( | void |  | ) | const

Get the Night (Sleep) mode of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## getPower()

bool IRMitsubishiHeavy152Ac::getPower | ( | void |  | ) | const

Get the value of the current power setting.

Returns
  true, the setting is on. false, the setting is off.

## getRaw()

uint8_t * IRMitsubishiHeavy152Ac::getRaw | ( | void |  | ) |

Get a PTR to the internal state/code for this protocol.

Returns
  PTR to a code for this protocol based on the current internal state.

## getSilent()

bool IRMitsubishiHeavy152Ac::getSilent | ( | void |  | ) | const

Get the Silent (Quiet) mode of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## getSwingHorizontal()

uint8_t IRMitsubishiHeavy152Ac::getSwingHorizontal | ( | void |  | ) | const

Get the Horizontal Swing mode of the A/C.

Returns
  The native position/mode setting.

## getSwingVertical()

uint8_t IRMitsubishiHeavy152Ac::getSwingVertical | ( | void |  | ) | const

Get the Vertical Swing mode of the A/C.

Returns
  The native position/mode setting.

## getTemp()

uint8_t IRMitsubishiHeavy152Ac::getTemp | ( | void |  | ) | const

Get the current temperature setting.

Returns
  The current setting for temp. in degrees celsius.

## getTurbo()

bool IRMitsubishiHeavy152Ac::getTurbo | ( | void |  | ) | const

Get the Turbo mode of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## off()

void IRMitsubishiHeavy152Ac::off | ( | void |  | ) |

Set the requested power state of the A/C to off.

## on()

void IRMitsubishiHeavy152Ac::on | ( | void |  | ) |

Set the requested power state of the A/C to on.

## send()

void IRMitsubishiHeavy152Ac::send | ( | const uint16_t | repeat = `kMitsubishiHeavy152MinRepeat` | ) |

Send the current internal state as an IR message.

Parameters

  [in] | repeat | Nr. of times the message will be repeated.

## set3D()

void IRMitsubishiHeavy152Ac::set3D | ( | const bool | on | ) |

Set the 3D mode of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## setClean()

void IRMitsubishiHeavy152Ac::setClean | ( | const bool | on | ) |

Set the Clean mode of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## setEcono()

void IRMitsubishiHeavy152Ac::setEcono | ( | const bool | on | ) |

Set the Economical mode of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## setFan()

void IRMitsubishiHeavy152Ac::setFan | ( | const uint8_t | speed | ) |

Set the speed of the fan.

Parameters

  [in] | speed | The desired setting.

## setFilter()

void IRMitsubishiHeavy152Ac::setFilter | ( | const bool | on | ) |

Set the Filter mode of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## setMode()

void IRMitsubishiHeavy152Ac::setMode | ( | const uint8_t | mode | ) |

Set the operating mode of the A/C.

Parameters

  [in] | mode | The desired operating mode.

## setNight()

void IRMitsubishiHeavy152Ac::setNight | ( | const bool | on | ) |

Set the Night (Sleep) mode of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## setPower()

void IRMitsubishiHeavy152Ac::setPower | ( | const bool | on | ) |

Change the power setting.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## setRaw()

void IRMitsubishiHeavy152Ac::setRaw | ( | const uint8_t * | data | ) |

Set the internal state from a valid code for this protocol.

Parameters

  [in] | data | A valid code for this protocol.

## setSilent()

void IRMitsubishiHeavy152Ac::setSilent | ( | const bool | on | ) |

Set the Silent (Quiet) mode of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## setSwingHorizontal()

void IRMitsubishiHeavy152Ac::setSwingHorizontal | ( | const uint8_t | pos | ) |

Set the Horizontal Swing mode of the A/C.

Parameters

  [in] | pos | The position/mode to set the swing to.

## setSwingVertical()

void IRMitsubishiHeavy152Ac::setSwingVertical | ( | const uint8_t | pos | ) |

Set the Vertical Swing mode of the A/C.

Parameters

  [in] | pos | The position/mode to set the swing to.

## setTemp()

void IRMitsubishiHeavy152Ac::setTemp | ( | const uint8_t | temp | ) |

Set the temperature.

Parameters

  [in] | temp | The temperature in degrees celsius.

## setTurbo()

void IRMitsubishiHeavy152Ac::setTurbo | ( | const bool | on | ) |

Set the Turbo mode of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## stateReset()

void IRMitsubishiHeavy152Ac::stateReset | ( | void |  | ) |

Reset the state of the remote to a known good state/sequence.

## toCommon()

stdAc::state_t IRMitsubishiHeavy152Ac::toCommon | ( | void |  | ) | const

Convert the current internal state into its stdAc::state_t equivalent.

Returns
  The stdAc equivalent of the native settings.

## toCommonFanSpeed()

stdAc::fanspeed_t IRMitsubishiHeavy152Ac::toCommonFanSpeed | ( | const uint8_t | spd | ) |

static

Convert a native fan speed into its stdAc equivalent.

Parameters

  [in] | spd | The native setting to be converted.

Returns
  The stdAc equivalent of the native setting.

## toCommonMode()

stdAc::opmode_t IRMitsubishiHeavy152Ac::toCommonMode | ( | const uint8_t | mode | ) |

static

Convert a native mode into its stdAc equivalent.

Parameters

  [in] | mode | The native setting to be converted.

Returns
  The stdAc equivalent of the native setting.

## toCommonSwingH()

stdAc::swingh_t IRMitsubishiHeavy152Ac::toCommonSwingH | ( | const uint8_t | pos | ) |

static

Convert a native horizontal swing postion to it's common equivalent.

Parameters

  [in] | pos | A native position to convert.

Returns
  The common horizontal swing position.

## toCommonSwingV()

stdAc::swingv_t IRMitsubishiHeavy152Ac::toCommonSwingV | ( | const uint8_t | pos | ) |

static

Convert a native vertical swing postion to it's common equivalent.

Parameters

  [in] | pos | A native position to convert.

Returns
  The common vertical swing position.

## toString()

String IRMitsubishiHeavy152Ac::toString | ( | void |  | ) | const

Convert the internal state into a human readable string.

Returns
  A string containing the settings in human-readable form.

## validChecksum()

bool IRMitsubishiHeavy152Ac::validChecksum | ( | const uint8_t * | state,
|  | const uint16_t | length = `kMitsubishiHeavy152StateLength`
| ) |  |

static

Verify the checksum is valid for a given state.

Parameters

  [in] | state | The array to verify the checksum of.
  [in] | length | The length/size of the state array.

Returns
  true, if the state has a valid checksum. Otherwise, false. Note: Technically it has no checksum, but does have inverted byte pairs.

## Member Data Documentation

## _

Mitsubishi152Protocol IRMitsubishiHeavy152Ac::_

private

## _irsend

IRsend IRMitsubishiHeavy152Ac::_irsend

private

Instance of the IR send class.

The documentation for this class was generated from the following files:

- src/ir_MitsubishiHeavy.h
- src/ir_MitsubishiHeavy.cpp