# IRremoteESP8266: Member List

IRTcl112Ac Member List

This is the complete list of members for IRTcl112Ac, including all inherited members.

_irsend | IRTcl112Ac | private
begin(void) | IRTcl112Ac |
calcChecksum(uint8_t state[], const uint16_t length=kTcl112AcStateLength) | IRTcl112Ac | static
calibrate(void) | IRTcl112Ac | inline
checksum(const uint16_t length=kTcl112AcStateLength) | IRTcl112Ac | private
convertFan(const stdAc::fanspeed_t speed) | IRTcl112Ac |
convertMode(const stdAc::opmode_t mode) | IRTcl112Ac |
getEcono(void) | IRTcl112Ac |
getFan(void) | IRTcl112Ac |
getHealth(void) | IRTcl112Ac |
getLight(void) | IRTcl112Ac |
getMode(void) | IRTcl112Ac |
getPower(void) | IRTcl112Ac |
getRaw(void) | IRTcl112Ac |
getSwingHorizontal(void) | IRTcl112Ac |
getSwingVertical(void) | IRTcl112Ac |
getTemp(void) | IRTcl112Ac |
getTurbo(void) | IRTcl112Ac |
IRTcl112Ac(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRTcl112Ac | explicit
off(void) | IRTcl112Ac |
on(void) | IRTcl112Ac |
remote_state | IRTcl112Ac | private
send(const uint16_t repeat=kTcl112AcDefaultRepeat) | IRTcl112Ac |
setEcono(const bool on) | IRTcl112Ac |
setFan(const uint8_t speed) | IRTcl112Ac |
setHealth(const bool on) | IRTcl112Ac |
setLight(const bool on) | IRTcl112Ac |
setMode(const uint8_t mode) | IRTcl112Ac |
setPower(const bool on) | IRTcl112Ac |
setRaw(const uint8_t new_code[], const uint16_t length=kTcl112AcStateLength) | IRTcl112Ac |
setSwingHorizontal(const bool on) | IRTcl112Ac |
setSwingVertical(const bool on) | IRTcl112Ac |
setTemp(const float celsius) | IRTcl112Ac |
setTurbo(const bool on) | IRTcl112Ac |
stateReset(void) | IRTcl112Ac |
toCommon(void) | IRTcl112Ac |
toCommonFanSpeed(const uint8_t speed) | IRTcl112Ac | static
toCommonMode(const uint8_t mode) | IRTcl112Ac | static
toString(void) | IRTcl112Ac |
validChecksum(uint8_t state[], const uint16_t length=kTcl112AcStateLength) | IRTcl112Ac | static