# IRremoteESP8266: IRrecv Class Reference

IRrecv Class Reference

Class for receiving IR messages. More...

`#include <IRrecv.h>`

Collaboration diagram for IRrecv:
[legend]

## Public Member Functions

| IRrecv (const uint16_t recvpin, const uint16_t bufsize=kRawBuf, const uint8_t timeout=kTimeoutMs, const bool save_buffer=false, const uint8_t timer_num=kDefaultESP32Timer)
| Class constructor Args: More...
| IRrecv (const uint16_t recvpin, const uint16_t bufsize=kRawBuf, const uint8_t timeout=kTimeoutMs, const bool save_buffer=false)
| ~IRrecv (void)
| Class destructor Cleans up after the object is no longer needed. e.g. Frees up all memory used by the various buffers, and disables any timers or interrupts used. More...
void | setTolerance (const uint8_t percent=kTolerance)
| Set the base tolerance percentage for matching incoming IR messages. More...
uint8_t | getTolerance (void)
| Get the base tolerance percentage for matching incoming IR messages. More...
bool | decode (decode_results *results, irparams_t *save=NULL, uint8_t max_skip=0, uint16_t noise_floor=0)
| Decodes the received IR message. If the interrupt state is saved, we will immediately resume waiting for the next IR message to avoid missing messages. More...
void | enableIRIn (const bool pullup=false)
| Set up and (re)start the IR capture mechanism. More...
void | disableIRIn (void)
| Stop collection of any received IR data. Disable any timers and interrupts. More...
void | resume (void)
| Resume collection of received IR data. More...
uint16_t | getBufSize (void)
| Obtain the maximum number of entries possible in the capture buffer. i.e. It's size. More...
void | setUnknownThreshold (const uint16_t length)
| Set the minimum length we will consider for reporting UNKNOWN message types. More...
bool | match (const uint32_t measured, const uint32_t desired, const uint8_t tolerance=kUseDefTol, const uint16_t delta=0)
| Check if we match a pulse(measured) with the desired within +/-tolerance percent and/or +/- a fixed delta range. More...
bool | matchMark (const uint32_t measured, const uint32_t desired, const uint8_t tolerance=kUseDefTol, const int16_t excess=kMarkExcess)
| Check if we match a mark signal(measured) with the desired within +/-tolerance percent, after an expected is excess is added. More...
bool | matchSpace (const uint32_t measured, const uint32_t desired, const uint8_t tolerance=kUseDefTol, const int16_t excess=kMarkExcess)
| Check if we match a space signal(measured) with the desired within +/-tolerance percent, after an expected is excess is removed. More...

## Private Member Functions

uint8_t | _validTolerance (const uint8_t percentage)
| Convert the tolerance percentage into something valid. More...
void | copyIrParams (volatile irparams_t *src, irparams_t *dst)
| Make a copy of the interrupt state & buffer data. Needed because irparams is marked as volatile, thus memcpy() isn't allowed. Only call this when you know the interrupt handlers won't modify anything. i.e. In kStopState. More...
uint16_t | compare (const uint16_t oldval, const uint16_t newval)
| Compare two tick values. More...
uint32_t | ticksLow (const uint32_t usecs, const uint8_t tolerance=kUseDefTol, const uint16_t delta=0)
| Calculate the lower bound of the nr. of ticks. More...
uint32_t | ticksHigh (const uint32_t usecs, const uint8_t tolerance=kUseDefTol, const uint16_t delta=0)
| Calculate the upper bound of the nr. of ticks. More...
bool | matchAtLeast (const uint32_t measured, const uint32_t desired, const uint8_t tolerance=kUseDefTol, const uint16_t delta=0)
| Check if we match a pulse(measured) of at least desired within tolerance percent and/or a fixed delta margin. More...

uint16_t

_matchGeneric (volatile uint16_t *data_ptr, uint64_t *result_bits_ptr, uint8_t *result_ptr, const bool use_bits, const uint16_t remaining, const uint16_t required, const uint16_t hdrmark, const uint32_t hdrspace, const uint16_t onemark, const uint32_t onespace, const uint16_t zeromark, const uint32_t zerospace, const uint16_t footermark, const uint32_t footerspace, const bool atleast=false, const uint8_t tolerance=kUseDefTol, const int16_t excess=kMarkExcess, const bool MSBfirst=true)

| Match & decode a generic/typical IR message. The data is stored in result_bits_ptr or result_bytes_ptr depending on flag `use_bits`. More...
match_result_t | matchData (volatile uint16_t *data_ptr, const uint16_t nbits, const uint16_t onemark, const uint32_t onespace, const uint16_t zeromark, const uint32_t zerospace, const uint8_t tolerance=kUseDefTol, const int16_t excess=kMarkExcess, const bool MSBfirst=true)
| Match & decode the typical data section of an IR message. The data value is stored in the least significant bits reguardless of the bit ordering requested. More...
uint16_t | matchBytes (volatile uint16_t *data_ptr, uint8_t *result_ptr, const uint16_t remaining, const uint16_t nbytes, const uint16_t onemark, const uint32_t onespace, const uint16_t zeromark, const uint32_t zerospace, const uint8_t tolerance=kUseDefTol, const int16_t excess=kMarkExcess, const bool MSBfirst=true)
| Match & decode the typical data section of an IR message. The bytes are stored at result_ptr. The first byte in the result equates to the first byte encountered, and so on. More...

uint16_t

matchGeneric (volatile uint16_t *data_ptr, uint64_t *result_ptr, const uint16_t remaining, const uint16_t nbits, const uint16_t hdrmark, const uint32_t hdrspace, const uint16_t onemark, const uint32_t onespace, const uint16_t zeromark, const uint32_t zerospace, const uint16_t footermark, const uint32_t footerspace, const bool atleast=false, const uint8_t tolerance=kUseDefTol, const int16_t excess=kMarkExcess, const bool MSBfirst=true)

| Match & decode a generic/typical <= 64bit IR message. The data is stored at result_ptr. More...

uint16_t

matchGeneric (volatile uint16_t *data_ptr, uint8_t *result_ptr, const uint16_t remaining, const uint16_t nbits, const uint16_t hdrmark, const uint32_t hdrspace, const uint16_t onemark, const uint32_t onespace, const uint16_t zeromark, const uint32_t zerospace, const uint16_t footermark, const uint32_t footerspace, const bool atleast=false, const uint8_t tolerance=kUseDefTol, const int16_t excess=kMarkExcess, const bool MSBfirst=true)

| Match & decode a generic/typical > 64bit IR message. The bytes are stored at result_ptr. The first byte in the result equates to the first byte encountered, and so on. More...

uint16_t

matchGenericConstBitTime (volatile uint16_t *data_ptr, uint64_t *result_ptr, const uint16_t remaining, const uint16_t nbits, const uint16_t hdrmark, const uint32_t hdrspace, const uint16_t one, const uint32_t zero, const uint16_t footermark, const uint32_t footerspace, const bool atleast=false, const uint8_t tolerance=kUseDefTol, const int16_t excess=kMarkExcess, const bool MSBfirst=true)

| Match & decode a generic/typical constant bit time <= 64bit IR message. The data is stored at result_ptr. More...
uint16_t | matchManchesterData (volatile const uint16_t *data_ptr, uint64_t *result_ptr, const uint16_t remaining, const uint16_t nbits, const uint16_t half_period, const uint16_t starting_balance=0, const uint8_t tolerance=kUseDefTol, const int16_t excess=kMarkExcess, const bool MSBfirst=true, const bool GEThomas=true)
| Match & decode a Manchester Code data (<= 64bits. More...

uint16_t

matchManchester (volatile const uint16_t *data_ptr, uint64_t *result_ptr, const uint16_t remaining, const uint16_t nbits, const uint16_t hdrmark, const uint32_t hdrspace, const uint16_t clock_period, const uint16_t footermark, const uint32_t footerspace, const bool atleast=false, const uint8_t tolerance=kUseDefTol, const int16_t excess=kMarkExcess, const bool MSBfirst=true, const bool GEThomas=true)

| Match & decode a Manchester Code <= 64bit IR message. The data is stored at result_ptr. More...
void | crudeNoiseFilter (decode_results *results, const uint16_t floor=0)
| Remove or merge pulses in the capture buffer that are too short. More...
bool | decodeHash (decode_results *results)
| Decode any arbitrary IR message into a 32-bit code value. Instead of decoding using a standard encoding scheme (e.g. Sony, NEC, RC5), the code is hashed to a 32-bit value. More...
bool | decodeVoltas (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kVoltasBits, const bool strict=true)
| Decode the supplied Voltas message. Status: STABLE / Working on real device. More...
bool | decodeNEC (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kNECBits, const bool strict=true)
| Decode the supplied NEC (Renesas) message. Status: STABLE / Known good. More...
bool | decodeArgo (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kArgoBits, const bool strict=true)
| Decode the supplied Argo message. Status: BETA / Probably works. More...
bool | decodeSony (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kSonyMinBits, const bool strict=false)
| Decode the supplied Sony/SIRC message. Status: STABLE / Should be working. strict mode is ALPHA / Untested. More...
bool | decodeSanyoLC7461 (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kSanyoLC7461Bits, const bool strict=true)
| Decode the supplied SANYO LC7461 message. Status: BETA / Probably works. More...
bool | decodeSanyoAc (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kSanyoAcBits, const bool strict=true)
| Decode the supplied SanyoAc message. Status: STABLE / Reported as working. More...
bool | decodeMitsubishi (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kMitsubishiBits, const bool strict=true)
| Decode the supplied Mitsubishi 16-bit message. Status: STABLE / Working. More...
bool | decodeMitsubishi2 (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kMitsubishiBits, const bool strict=true)
| Decode the supplied second variation of a Mitsubishi 16-bit message. Status: STABLE / Working. More...
bool | decodeMitsubishiAC (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kMitsubishiACBits, const bool strict=false)
| Decode the supplied Mitsubish 144-bit A/C message. Status: BETA / Probably works. More...
bool | decodeMitsubishi136 (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kMitsubishi136Bits, const bool strict=true)
| Decode the supplied Mitsubishi 136-bit A/C message. (MITSUBISHI136) Status: STABLE / Reported as working. More...
bool | decodeMitsubishi112 (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kMitsubishi112Bits, const bool strict=true)
| Decode the supplied Mitsubishi/TCL 112-bit A/C message. (MITSUBISHI112, TCL112AC) Status: STABLE / Reported as working. More...
bool | decodeMitsubishiHeavy (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kMitsubishiHeavy152Bits, const bool strict=true)
| Decode the supplied Mitsubishi Heavy Industries A/C message. Status: BETA / Appears to be working. Needs testing against a real device. More...
int16_t | getRClevel (decode_results *results, uint16_t *offset, uint16_t *used, uint16_t bitTime, const uint8_t tolerance=kUseDefTol, const int16_t excess=kMarkExcess, const uint16_t delta=0, const uint8_t maxwidth=3)
| Gets one undecoded level at a time from the raw buffer. The RC5/6 decoding is easier if the data is broken into time intervals. E.g. if the buffer has MARK for 2 time intervals and SPACE for 1, successive calls to getRClevel will return MARK, MARK, SPACE. offset and used are updated to keep track of the current position. More...
bool | decodeRC5 (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kRC5XBits, const bool strict=true)
| Decode the supplied RC-5/RC5X message. Status: RC-5 (stable), RC-5X (alpha) More...
bool | decodeRC6 (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kRC6Mode0Bits, const bool strict=false)
| Decode the supplied RC6 message. Status: Stable. More...
bool | decodeRCMM (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kRCMMBits, const bool strict=false)
| Decode a Philips RC-MM packet (between 12 & 32 bits) if possible. Status: STABLE / Should be working. More...
bool | decodePanasonic (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kPanasonicBits, const bool strict=false, const uint32_t manufacturer=kPanasonicManufacturer)
| Decode the supplied Panasonic message. Status: STABLE / Should be working. More...
bool | decodeLG (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kLgBits, const bool strict=false)
| Decode the supplied LG message. Status: STABLE / Working. More...
bool | decodeInax (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kInaxBits, const bool strict=true)
| Decode the supplied Inax Toilet message. Status: Stable / Known working. More...
bool | decodeJVC (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kJvcBits, const bool strict=true)
| Decode the supplied JVC message. Status: Stable / Known working. More...
bool | decodeSAMSUNG (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kSamsungBits, const bool strict=true)
| Decode the supplied Samsung 32-bit message. Status: STABLE. More...
bool | decodeSamsung36 (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kSamsung36Bits, const bool strict=true)
| Decode the supplied Samsung36 message. Status: STABLE / Expected to work. More...
bool | decodeSamsungAC (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kSamsungAcBits, const bool strict=true)
| Decode the supplied Samsung A/C message. Status: Stable / Known to be working. More...
bool | decodeWhynter (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kWhynterBits, const bool strict=true)
| Decode the supplied Whynter message. Status: STABLE / Working. Strict mode is ALPHA. More...
bool | decodeCOOLIX (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kCoolixBits, const bool strict=true)
| Decode the supplied Coolix A/C message. Status: STABLE / Known Working. More...
bool | decodeDenon (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kDenonBits, const bool strict=true)
| Decode the supplied Delonghi A/C message. Status: STABLE / Should work fine. More...
bool | decodeDISH (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kDishBits, const bool strict=true)
| Decode the supplied DISH NETWORK message. Status: ALPHA (untested and unconfirmed.) More...
bool | decodeSharp (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kSharpBits, const bool strict=true, const bool expansion=true)
| Decode the supplied Sharp message. Status: STABLE / Working fine. More...
bool | decodeSharpAc (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kSharpAcBits, const bool strict=true)
| Decode the supplied Sharp A/C message. Status: STABLE / Known working. More...
bool | decodeAiwaRCT501 (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kAiwaRcT501Bits, const bool strict=true)
| Decode the supplied Aiwa RC T501 message. Status: BETA / Should work. More...
bool | decodeNikai (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kNikaiBits, const bool strict=true)
| Decode the supplied Nikai message. Status: STABLE / Working. More...
bool | decodeMagiQuest (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kMagiquestBits, const bool strict=true)
| Decode the supplied MagiQuest message. Status: Beta / Should work. More...
bool | decodeKelvinator (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kKelvinatorBits, const bool strict=true)
| Decode the supplied Kelvinator message. Status: STABLE / Known working. More...
bool | decodeDaikin (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kDaikinBits, const bool strict=true)
| Decode the supplied Daikin 280-bit message. (DAIKIN) Status: STABLE / Reported as working. More...
bool | decodeDaikin64 (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kDaikin64Bits, const bool strict=true)
| Decode the supplied Daikin 64-bit message. (DAIKIN64) Status: Beta / Probably Working. More...
bool | decodeDaikin128 (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kDaikin128Bits, const bool strict=true)
| Decode the supplied Daikin 128-bit message. (DAIKIN128) Status: STABLE / Known Working. More...
bool | decodeDaikin152 (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kDaikin152Bits, const bool strict=true)
| Decode the supplied Daikin 152-bit message. (DAIKIN152) Status: STABLE / Known Working. More...
bool | decodeDaikin160 (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kDaikin160Bits, const bool strict=true)
| Decode the supplied Daikin 160-bit message. (DAIKIN160) Status: STABLE / Confirmed working. More...
bool | decodeDaikin176 (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kDaikin176Bits, const bool strict=true)
| Decode the supplied Daikin 176-bit message. (DAIKIN176) Status: STABLE / Expected to work. More...
bool | decodeDaikin2 (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kDaikin2Bits, const bool strict=true)
| Decode the supplied Daikin 312-bit message. (DAIKIN2) Status: STABLE / Works as expected. More...
bool | decodeDaikin216 (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kDaikin216Bits, const bool strict=true)
| Decode the supplied Daikin 216-bit message. (DAIKIN216) Status: STABLE / Should be working. More...
bool | decodeToshibaAC (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kToshibaACBits, const bool strict=true)
| Decode the supplied Toshiba A/C message. Status: STABLE / Working. More...
bool | decodeTrotec (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kTrotecBits, const bool strict=true)
| Decode the supplied Trotec message. Status: STABLE / Works. Untested on real devices. More...
bool | decodeMidea (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kMideaBits, const bool strict=true)
| Decode the supplied Midea message. Status: Alpha / Needs testing against a real device. More...
bool | decodeMidea24 (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kMidea24Bits, const bool strict=true)
| Decode the supplied Midea24 message. Status: STABLE / Confirmed working on a real device. More...
bool | decodeFujitsuAC (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kFujitsuAcBits, const bool strict=false)
| Decode the supplied Fujitsu AC IR message if possible. Status: STABLE / Working. More...
bool | decodeLasertag (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kLasertagBits, const bool strict=true)
| Decode the supplied Lasertag message. Status: BETA / Appears to be working 90% of the time. More...
bool | decodeCarrierAC (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kCarrierAcBits, const bool strict=true)
| Decode the supplied Carrier HVAC message. More...
bool | decodeCarrierAC40 (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kCarrierAc40Bits, const bool strict=true)
| Decode the supplied Carrier 40-bit HVAC message. Carrier HVAC messages contain only 40 bits, but it is sent three(3) times. Status: STABLE / Tested against a real device. More...
bool | decodeCarrierAC64 (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kCarrierAc64Bits, const bool strict=true)
| Decode the supplied Carrier 64-bit HVAC message. Status: STABLE / Known to be working. More...
bool | decodeGoodweather (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kGoodweatherBits, const bool strict=true)
| Decode the supplied Goodweather message. Status: BETA / Probably works. More...
bool | decodeGree (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kGreeBits, const bool strict=true)
| Decode the supplied Gree HVAC message. Status: STABLE / Working. More...
bool | decodeHaierAC (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kHaierACBits, const bool strict=true)
| Decode the supplied Haier HSU07-HEA03 remote message. Status: STABLE / Known to be working. More...
bool | decodeHaierACYRW02 (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kHaierACYRW02Bits, const bool strict=true)
| Decode the supplied Haier YR-W02 remote A/C message. Status: BETA / Appears to be working. More...
bool | decodeHitachiAC (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kHitachiAcBits, const bool strict=true, const bool MSBfirst=true)
| Decode the supplied Hitachi A/C message. Status: STABLE / Expected to work. More...
bool | decodeHitachiAC1 (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kHitachiAc1Bits, const bool strict=true)
bool | decodeHitachiAc3 (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kHitachiAc3Bits, const bool strict=true)
| Decode the supplied Hitachi 15to27-byte/120to216-bit A/C message. Status: STABLE / Works fine. More...
bool | decodeHitachiAc424 (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kHitachiAc424Bits, const bool strict=true)
| Decode the supplied Hitachi 53-byte/424-bit A/C message. Status: STABLE / Reported as working. More...
bool | decodeGICable (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kGicableBits, const bool strict=true)
| Decode the supplied G.I. Cable message. Status: Alpha / Not tested against a real device. More...
bool | decodeWhirlpoolAC (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kWhirlpoolAcBits, const bool strict=true)
| Decode the supplied Whirlpool A/C message. Status: STABLE / Working as intended. More...
bool | decodeLutron (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kLutronBits, const bool strict=true)
| Decode the supplied Lutron message. Status: STABLE / Working. More...
bool | decodeElectraAC (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kElectraAcBits, const bool strict=true)
| Decode the supplied Electra A/C message. Status: STABLE / Known working. More...
bool | decodePanasonicAC (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kPanasonicAcBits, const bool strict=true)
| Decode the supplied Panasonic AC message. Status: STABLE / Works with real device(s). More...
bool | decodePanasonicAC32 (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kPanasonicAc32Bits, const bool strict=true)
| Decode the supplied Panasonic AC 32/16bit message. Status: STABLE / Confirmed working. More...
bool | decodePioneer (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kPioneerBits, const bool strict=true)
| Decode the supplied Pioneer message. Status: STABLE / Should be working. (Self decodes & real examples) More...
bool | decodeMWM (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=24, const bool strict=true)
| Decode the supplied MWM message. Status: Implemented. More...
bool | decodeVestelAc (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kVestelAcBits, const bool strict=true)
| Decode the supplied Vestel message. Status: Alpha / Needs testing against a real device. More...
bool | decodeTeco (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kTecoBits, const bool strict=false)
| Decode the supplied Teco message. Status: STABLE / Tested. More...
bool | decodeLegoPf (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kLegoPfBits, const bool strict=true)
| Decode the supplied LEGO Power Functions message. Status: STABLE / Appears to work. More...
bool | decodeNeoclima (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kNeoclimaBits, const bool strict=true)
| Decode the supplied Neoclima message. Status: STABLE / Known working. More...
bool | decodeAmcor (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kAmcorBits, const bool strict=true)
| Decode the supplied Amcor HVAC message. Status: STABLE / Reported as working. More...
bool | decodeEpson (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kEpsonBits, const bool strict=true)
| Decode the supplied Epson message. Status: Beta / Probably works. More...
bool | decodeSymphony (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kSymphonyBits, const bool strict=true)
| Decode the supplied Symphony packet/message. Status: STABLE / Should be working. More...
bool | decodeAirwell (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kAirwellBits, const bool strict=true)
| Decode the supplied Airwell "Manchester code" message. More...
bool | decodeDelonghiAc (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kDelonghiAcBits, const bool strict=true)
| Decode the supplied Delonghi A/C message. Status: STABLE / Expected to be working. More...
bool | decodeDoshisha (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kDoshishaBits, const bool strict=true)
| Decode the supplied Doshisha message. Status: STABLE / Works on real device. More...
bool | decodeMultibrackets (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kMultibracketsBits, const bool strict=true)
| Decode the Multibrackets message. Status: BETA / Appears to be working. More...
bool | decodeTechnibelAc (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kTechnibelAcBits, const bool strict=true)
| Status: STABLE / Reported as working on a real device. More...
bool | decodeCoronaAc (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kCoronaAcBitsShort, const bool strict=true)
| Decode the supplied CoronaAc message. Status: STABLE / Appears to be working. More...
bool | decodeZepeal (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kZepealBits, const bool strict=true)
| Decode the supplied Zepeal message. Status: STABLE / Works on real device. More...
bool | decodeMetz (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kMetzBits, const bool strict=true)
| Decode the supplied Metz message. Status: BETA / Probably works. More...
bool | decodeTranscold (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kTranscoldBits, const bool strict=true)
| Decode the supplied Transcold A/C message. Status: STABLE / Known Working. More...
bool | decodeMirage (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kMirageBits, const bool strict=true)
| Decode the supplied Mirage message. Status: STABLE / Reported as working. More...
bool | decodeElitescreens (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kEliteScreensBits, const bool strict=true)
| Decode the supplied Elite Screens message. Status: STABLE / Confirmed working. More...

## Private Attributes

irparams_t * | irparams_save
uint8_t | _tolerance
uint8_t | _timer_num
uint16_t | _unknown_threshold

## Detailed Description

Class for receiving IR messages.

## Constructor & Destructor Documentation

## IRrecv() [1/2]

IRrecv::IRrecv | ( | const uint16_t | recvpin,
|  | const uint16_t | bufsize = `kRawBuf`,
|  | const uint8_t | timeout = `kTimeoutMs`,
|  | const bool | save_buffer = `false`,
|  | const uint8_t | timer_num = `kDefaultESP32Timer`
| ) |  |

explicit

Class constructor Args:

Parameters

  [in] | recvpin | The GPIO pin the IR receiver module's data pin is connected to.
  [in] | bufsize | Nr. of entries to have in the capture buffer. (Default: kRawBuf)
  [in] | timeout | Nr. of milli-Seconds of no signal before we stop capturing data. (Default: kTimeoutMs)
  [in] | save_buffer | Use a second (save) buffer to decode from. (Default: false)
  [in] | timer_num | Nr. of the ESP32 timer to use (0 to 3) (ESP32 Only)

## IRrecv() [2/2]

IRrecv::IRrecv | ( | const uint16_t | recvpin,
|  | const uint16_t | bufsize = `kRawBuf`,
|  | const uint8_t | timeout = `kTimeoutMs`,
|  | const bool | save_buffer = `false`
| ) |  |

explicit

## ~IRrecv()

IRrecv::~IRrecv | ( | void |  | ) |

Class destructor Cleans up after the object is no longer needed. e.g. Frees up all memory used by the various buffers, and disables any timers or interrupts used.

## Member Function Documentation

## _matchGeneric()

uint16_t IRrecv::_matchGeneric | ( | volatile uint16_t * | data_ptr,
|  | uint64_t * | result_bits_ptr,
|  | uint8_t * | result_bytes_ptr,
|  | const bool | use_bits,
|  | const uint16_t | remaining,
|  | const uint16_t | nbits,
|  | const uint16_t | hdrmark,
|  | const uint32_t | hdrspace,
|  | const uint16_t | onemark,
|  | const uint32_t | onespace,
|  | const uint16_t | zeromark,
|  | const uint32_t | zerospace,
|  | const uint16_t | footermark,
|  | const uint32_t | footerspace,
|  | const bool | atleast = `false`,
|  | const uint8_t | tolerance = `kUseDefTol`,
|  | const int16_t | excess = `kMarkExcess`,
|  | const bool | MSBfirst = `true`
| ) |  |

private

Match & decode a generic/typical IR message. The data is stored in result_bits_ptr or result_bytes_ptr depending on flag `use_bits`.

Note
  Values of 0 for hdrmark, hdrspace, footermark, or footerspace mean skip that requirement.

Parameters

  [in] | data_ptr | A pointer to where we are at in the capture buffer.
  [out] | result_bits_ptr | A pointer to where to start storing the bits we decoded.
  [out] | result_bytes_ptr | A pointer to where to start storing the bytes we decoded.
  [in] | use_bits | A flag indicating if we are to decode bits or bytes.
  [in] | remaining | The size of the capture buffer remaining.
  [in] | nbits | Nr. of data bits we expect.
  [in] | hdrmark | Nr. of uSeconds for the expected header mark signal.
  [in] | hdrspace | Nr. of uSeconds for the expected header space signal.
  [in] | onemark | Nr. of uSeconds in an expected mark signal for a '1' bit.
  [in] | onespace | Nr. of uSecs in an expected space signal for a '1' bit.
  [in] | zeromark | Nr. of uSecs in an expected mark signal for a '0' bit.
  [in] | zerospace | Nr. of uSecs in an expected space signal for a '0' bit.
  [in] | footermark | Nr. of uSeconds for the expected footer mark signal.
  [in] | footerspace | Nr. of uSeconds for the expected footer space/gap signal.
  [in] | atleast | Is the match on the footerspace a matchAtLeast or matchSpace?
  [in] | tolerance | Percentage error margin to allow. (Default: kUseDefTol)
  [in] | excess | Nr. of uSeconds. (Def: kMarkExcess)
  [in] | MSBfirst | Bit order to save the data in. (Def: true) true is Most Significant Bit First Order, false is Least Significant First

Returns
  If successful, how many buffer entries were used. Otherwise 0.

## _validTolerance()

uint8_t IRrecv::_validTolerance | ( | const uint8_t | percentage | ) |

private

Convert the tolerance percentage into something valid.

Parameters

  [in] | percentage | An integer percentage.

## compare()

uint16_t IRrecv::compare | ( | const uint16_t | oldval,
|  | const uint16_t | newval
| ) |  |

private

Compare two tick values.

Parameters

  [in] | oldval | Nr. of ticks.
  [in] | newval | Nr. of ticks.

Returns
  0 if newval is shorter, 1 if it is equal, & 2 if it is longer.

Note
  Use a tolerance of 20%

## copyIrParams()

void IRrecv::copyIrParams | ( | volatile irparams_t * | src,
|  | irparams_t * | dst
| ) |  |

private

Make a copy of the interrupt state & buffer data. Needed because irparams is marked as volatile, thus memcpy() isn't allowed. Only call this when you know the interrupt handlers won't modify anything. i.e. In kStopState.

Parameters

  [in] | src | Pointer to an irparams_t structure to copy from.
  [out] | dst | Pointer to an irparams_t structure to copy to.

## crudeNoiseFilter()

void IRrecv::crudeNoiseFilter | ( | decode_results * | results,
|  | const uint16_t | floor = `0`
| ) |  |

private

Remove or merge pulses in the capture buffer that are too short.

Parameters

  [in,out] | results | Ptr to the decode_results we are going to filter.
  [in] | floor | Only allow values in the buffer large than this. (in microSeconds)

## decode()

bool IRrecv::decode | ( | decode_results * | results,
|  | irparams_t * | save = `NULL`,
|  | uint8_t | max_skip = `0`,
|  | uint16_t | noise_floor = `0`
| ) |  |

Decodes the received IR message. If the interrupt state is saved, we will immediately resume waiting for the next IR message to avoid missing messages.

Note
  There is a trade-off here. Saving the state means less time lost until we can receiving the next message vs. using more RAM. Choose appropriately.

Parameters

  [out] | results | A PTR to where the decoded IR message will be stored.
  [out] | save | A PTR to an irparams_t instance in which to save the interrupt's memory/state. NULL means don't save it.
  [in] | max_skip | Maximum Nr. of pulses at the begining of a capture we can skip when attempting to find a protocol we can successfully decode. This parameter can dramatically improve detection of protocols when there is light IR interference just before an incoming IR message, however, it comes at a steep performace price. (Default is 0. No skipping.)

Warning
  Increasing the `max_skip` value will dramatically (linearly) increase the cpu time & usage to decode protocols. e.g. 0 -> 1 will be a 2x increase in cpu usage/time. 0 -> 2 will be a 3x increase etc. If you are going to do this, consider disabling protocol decoding for protocols you are not expecting.

Parameters

  [in] | noise_floor | Pulses below this size (in usecs) will be removed or merged prior to any decoding. This is to try to remove noise/poor readings & slightly increase the chances of a successful decode but at the cost of data fidelity & integrity. (Defaults to 0 usecs. i.e. Don't filter; which is safe!)

Warning
  DANGER: Here Be Dragons! If you set the `noise_floor` value too high, it WILL break decoding of some protocols. You have been warned! Any non-zero value has the potential to cook the captured raw data i.e. The raw data is going to lie to you. It may obscure hardware, circuit, & environment issues thus making it impossible to support you accurately or confidently. Values of <= 50 usecs will probably be safe. 51 - 100 usecs might be okay. 100 - 150 usecs is "Danger, Will Robinson!". 150 - 200 usecs expect broken protocols. At 200+ usecs, you have protocols you can't decode!!

Returns
  A boolean indicating if an IR message is ready or not.

## decodeAirwell()

bool IRrecv::decodeAirwell | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kAirwellBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Airwell "Manchester code" message.

Status: BETA / Appears to be working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode result.
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

See also
  https://github.com/crankyoldgit/IRremoteESP8266/issues/1069

## decodeAiwaRCT501()

bool IRrecv::decodeAiwaRCT501 | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kAiwaRcT501Bits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Aiwa RC T501 message. Status: BETA / Should work.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode result.
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

Note
  Aiwa RC T501 appears to be a 42 bit variant of the NEC1 protocol. However, we historically (original Arduino IRremote project) treats it as a 15 bit (data) protocol. So, we expect nbits to typically be 15, and we will remove the prefix and postfix from the raw data, and use that as the result.

See also
  http://www.sbprojects.com/knowledge/ir/nec.php
  https://github.com/crankyoldgit/IRremoteESP8266/issues/1069

## decodeAmcor()

bool IRrecv::decodeAmcor | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kAmcorBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Amcor HVAC message. Status: STABLE / Reported as working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode result.
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

## decodeArgo()

bool IRrecv::decodeArgo | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kArgoBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Argo message. Status: BETA / Probably works.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode result.
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

Note
  This decoder is based soley off sendArgo(). We have no actual captures to test this against. If you have one of these units, please let us know.

## decodeCarrierAC()

bool IRrecv::decodeCarrierAC | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kCarrierAcBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Carrier HVAC message.

Note
  Carrier HVAC messages contain only 32 bits, but it is sent three(3) times. i.e. normal + inverted + normal Status: BETA / Probably works.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode result.
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

## decodeCarrierAC40()

bool IRrecv::decodeCarrierAC40 | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kCarrierAc40Bits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Carrier 40-bit HVAC message. Carrier HVAC messages contain only 40 bits, but it is sent three(3) times. Status: STABLE / Tested against a real device.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode result.
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

## decodeCarrierAC64()

bool IRrecv::decodeCarrierAC64 | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kCarrierAc64Bits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Carrier 64-bit HVAC message. Status: STABLE / Known to be working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode result.
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

## decodeCOOLIX()

bool IRrecv::decodeCOOLIX | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kCoolixBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Coolix A/C message. Status: STABLE / Known Working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode result.
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

## decodeCoronaAc()

bool IRrecv::decodeCoronaAc | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kCoronaAcBitsShort`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied CoronaAc message. Status: STABLE / Appears to be working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store it
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

## decodeDaikin()

bool IRrecv::decodeDaikin | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kDaikinBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Daikin 280-bit message. (DAIKIN) Status: STABLE / Reported as working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode result.
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

See also
  https://github.com/mharizanov/Daikin-AC-remote-control-over-the-Internet/tree/master/IRremote

## decodeDaikin128()

bool IRrecv::decodeDaikin128 | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kDaikin128Bits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Daikin 128-bit message. (DAIKIN128) Status: STABLE / Known Working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode result.
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

See also
  https://github.com/crankyoldgit/IRremoteESP8266/issues/827

## decodeDaikin152()

bool IRrecv::decodeDaikin152 | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kDaikin152Bits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Daikin 152-bit message. (DAIKIN152) Status: STABLE / Known Working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode result.
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

See also
  https://github.com/crankyoldgit/IRremoteESP8266/issues/873

## decodeDaikin160()

bool IRrecv::decodeDaikin160 | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kDaikin160Bits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Daikin 160-bit message. (DAIKIN160) Status: STABLE / Confirmed working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode result.
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

See also
  https://github.com/crankyoldgit/IRremoteESP8266/issues/731

## decodeDaikin176()

bool IRrecv::decodeDaikin176 | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kDaikin176Bits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Daikin 176-bit message. (DAIKIN176) Status: STABLE / Expected to work.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode result.
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

## decodeDaikin2()

bool IRrecv::decodeDaikin2 | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kDaikin2Bits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Daikin 312-bit message. (DAIKIN2) Status: STABLE / Works as expected.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode result.
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

## decodeDaikin216()

bool IRrecv::decodeDaikin216 | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kDaikin216Bits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Daikin 216-bit message. (DAIKIN216) Status: STABLE / Should be working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode result.
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

See also
  https://github.com/crankyoldgit/IRremoteESP8266/issues/689
  https://github.com/danny-source/Arduino_DY_IRDaikin

## decodeDaikin64()

bool IRrecv::decodeDaikin64 | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kDaikin64Bits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Daikin 64-bit message. (DAIKIN64) Status: Beta / Probably Working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode result.
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

See also
  https://github.com/crankyoldgit/IRremoteESP8266/issues/1064

## decodeDelonghiAc()

bool IRrecv::decodeDelonghiAc | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kDelonghiAcBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Delonghi A/C message. Status: STABLE / Expected to be working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode result.
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

See also
  https://github.com/crankyoldgit/IRremoteESP8266/issues/1096

## decodeDenon()

bool IRrecv::decodeDenon | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kDenonBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Delonghi A/C message. Status: STABLE / Should work fine.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode result.
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

See also
  https://github.com/z3t0/Arduino-IRremote/blob/master/ir_Denon.cpp

## decodeDISH()

bool IRrecv::decodeDISH | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kDishBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied DISH NETWORK message. Status: ALPHA (untested and unconfirmed.)

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode result.
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

Note
  Dishplayer is a different protocol. Typically a DISH device needs to get a command a total of at least 4 times to accept it.

See also
  http://www.hifi-remote.com/wiki/index.php?title=Dish
  http://lirc.sourceforge.net/remotes/echostar/301_501_3100_5100_58xx_59xx
  https://github.com/marcosamarinho/IRremoteESP8266/blob/master/ir_Dish.cpp

## decodeDoshisha()

bool IRrecv::decodeDoshisha | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kDoshishaBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Doshisha message. Status: STABLE / Works on real device.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode result.
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

## decodeElectraAC()

bool IRrecv::decodeElectraAC | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kElectraAcBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Electra A/C message. Status: STABLE / Known working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode result.
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

## decodeElitescreens()

bool IRrecv::decodeElitescreens | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kEliteScreensBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Elite Screens message. Status: STABLE / Confirmed working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode result.
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

## decodeEpson()

bool IRrecv::decodeEpson | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kEpsonBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Epson message. Status: Beta / Probably works.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode result.
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

Note
  Experimental data indicates there are at least three messages (first + 2 repeats). We only require the first + a single repeat to match. This helps us distinguish it from NEC messages which are near identical.

## decodeFujitsuAC()

bool IRrecv::decodeFujitsuAC | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kFujitsuAcBits`,
|  | const bool | strict = `false`
| ) |  |

private

Decode the supplied Fujitsu AC IR message if possible. Status: STABLE / Working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode result.
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

## decodeGICable()

bool IRrecv::decodeGICable | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kGicableBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied G.I. Cable message. Status: Alpha / Not tested against a real device.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode result.
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

## decodeGoodweather()

bool IRrecv::decodeGoodweather | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kGoodweatherBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Goodweather message. Status: BETA / Probably works.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode result.
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

## decodeGree()

bool IRrecv::decodeGree | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kGreeBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Gree HVAC message. Status: STABLE / Working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode result.
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

## decodeHaierAC()

bool IRrecv::decodeHaierAC | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kHaierACBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Haier HSU07-HEA03 remote message. Status: STABLE / Known to be working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode result.
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

## decodeHaierACYRW02()

bool IRrecv::decodeHaierACYRW02 | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kHaierACYRW02Bits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Haier YR-W02 remote A/C message. Status: BETA / Appears to be working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode result.
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

## decodeHash()

bool IRrecv::decodeHash | ( | decode_results * | results | ) |

private

Decode any arbitrary IR message into a 32-bit code value. Instead of decoding using a standard encoding scheme (e.g. Sony, NEC, RC5), the code is hashed to a 32-bit value.

The algorithm: look at the sequence of MARK signals, and see if each one is shorter (0), the same length (1), or longer (2) than the previous. Do the same with the SPACE signals. Hash the resulting sequence of 0's, 1's, and 2's to a 32-bit value. This will give a unique value for each different code (probably), for most code systems.

See also
  http://arcfn.com/2010/01/using-arbitrary-remotes-with-arduino.html

Note
  This isn't a "real" decoding, just an arbitrary value. Hopefully this code is unique for each button.

## decodeHitachiAC()

bool IRrecv::decodeHitachiAC | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kHitachiAcBits`,
|  | const bool | strict = `true`,
|  | const bool | MSBfirst = `true`
| ) |  |

private

Decode the supplied Hitachi A/C message. Status: STABLE / Expected to work.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect. Typically kHitachiAcBits, kHitachiAc1Bits, kHitachiAc2Bits, kHitachiAc344Bits
  [in] | strict | Flag indicating if we should perform strict matching.
  [in] | MSBfirst | Is the data per byte stored in MSB First (true) or LSB First order(false)?

Returns
  True if it can decode it, false if it can't.

See also
  https://github.com/crankyoldgit/IRremoteESP8266/issues/417
  https://github.com/crankyoldgit/IRremoteESP8266/issues/453
  https://github.com/crankyoldgit/IRremoteESP8266/issues/1134

## decodeHitachiAC1()

bool IRrecv::decodeHitachiAC1 | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kHitachiAc1Bits`,
|  | const bool | strict = `true`
| ) |  |

private

## decodeHitachiAc3()

bool IRrecv::decodeHitachiAc3 | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kHitachiAc3Bits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Hitachi 15to27-byte/120to216-bit A/C message. Status: STABLE / Works fine.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  True if it can decode it, false if it can't.

Note
  This protocol is almost exactly the same as HitachiAC424 except this variant has subtle timing differences and multiple lengths. There are five(5) typical lengths: kHitachiAc3MinStateLength (Cancel Timer), kHitachiAc3MinStateLength + 2 (Change Temp), kHitachiAc3StateLength - 6 (Change Mode), kHitachiAc3StateLength - 4 (Normal), & kHitachiAc3StateLength (Set Timer)

See also
  https://github.com/crankyoldgit/IRremoteESP8266/issues/1060

## decodeHitachiAc424()

bool IRrecv::decodeHitachiAc424 | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kHitachiAc424Bits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Hitachi 53-byte/424-bit A/C message. Status: STABLE / Reported as working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  True if it can decode it, false if it can't.

Note
  This protocol is almost exactly the same as HitachiAC2 except this variant has a leader section as well, and subtle timing differences. It is also in LSBF order (per byte), rather than MSBF order.

See also
  https://github.com/crankyoldgit/IRremoteESP8266/issues/973
  (Japanese Manual) https://kadenfan.hitachi.co.jp/support/raj/item/docs/ras_aj22h_a_tori.pdf

## decodeInax()

bool IRrecv::decodeInax | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kInaxBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Inax Toilet message. Status: Stable / Known working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  True if it can decode it, false if it can't.

See also
  https://github.com/crankyoldgit/IRremoteESP8266/issues/706

## decodeJVC()

bool IRrecv::decodeJVC | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kJvcBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied JVC message. Status: Stable / Known working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  True if it can decode it, false if it can't.

Note
  JVC repeat codes don't have a header.

See also
  http://www.sbprojects.com/knowledge/ir/jvc.php

## decodeKelvinator()

bool IRrecv::decodeKelvinator | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kKelvinatorBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Kelvinator message. Status: STABLE / Known working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode result.
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

## decodeLasertag()

bool IRrecv::decodeLasertag | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kLasertagBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Lasertag message. Status: BETA / Appears to be working 90% of the time.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  True if it can decode it, false if it can't.

Note
  This protocol is pretty much just raw Manchester encoding.

See also
  http://www.sbprojects.com/knowledge/ir/rc5.php
  https://en.wikipedia.org/wiki/RC-5
  https://en.wikipedia.org/wiki/Manchester_code

Todo:
  Convert to using `matchManchester()` if we can.

## decodeLegoPf()

bool IRrecv::decodeLegoPf | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kLegoPfBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied LEGO Power Functions message. Status: STABLE / Appears to work.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  True if it can decode it, false if it can't.

## decodeLG()

bool IRrecv::decodeLG | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kLgBits`,
|  | const bool | strict = `false`
| ) |  |

private

Decode the supplied LG message. Status: STABLE / Working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect. Typically kLgBits or kLg32Bits.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  True if it can decode it, false if it can't.

Note
  LG protocol has a repeat code which is 4 items long. Even though the protocol has 28/32 bits of data, only 24/28 bits are distinct. In transmission order, the 28/32 bits are constructed as follows: 8/12 bits of address + 16 bits of command + 4 bits of checksum.
  LG 32bit protocol appears near identical to the Samsung protocol. They possibly differ on how they repeat and initial HDR mark.

See also
  https://funembedded.wordpress.com/2014/11/08/ir-remote-control-for-lg-conditioner-using-stm32f302-mcu-on-mbed-platform/

## decodeLutron()

bool IRrecv::decodeLutron | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kLutronBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Lutron message. Status: STABLE / Working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  True if it can decode it, false if it can't.

## decodeMagiQuest()

bool IRrecv::decodeMagiQuest | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kMagiquestBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied MagiQuest message. Status: Beta / Should work.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  True if it can decode it, false if it can't.

Note
  MagiQuest protocol appears to be a header of 8 'zero' bits, followed by 32 bits of "wand ID" and finally 16 bits of "magnitude". Even though we describe this protocol as 56 bits, it really only has 48 bits of data that matter. In transmission order, 8 zeros + 32 wand_id + 16 magnitude.

See also
  https://github.com/kitlaan/Arduino-IRremote/blob/master/ir_Magiquest.cpp

## decodeMetz()

bool IRrecv::decodeMetz | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kMetzBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Metz message. Status: BETA / Probably works.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

## decodeMidea()

bool IRrecv::decodeMidea | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kMideaBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Midea message. Status: Alpha / Needs testing against a real device.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect. Typically kHitachiAcBits, kHitachiAc1Bits, kHitachiAc2Bits, kHitachiAc344Bits
  [in] | strict | Flag indicating if we should perform strict matching.

## decodeMidea24()

bool IRrecv::decodeMidea24 | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kMidea24Bits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Midea24 message. Status: STABLE / Confirmed working on a real device.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode result.
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

Note
  This protocol is basically a 48-bit version of the NEC protocol with alternate bytes inverted, thus only 24 bits of real data.

Warning
  Can't be used beyond 32 bits.

## decodeMirage()

bool IRrecv::decodeMirage | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kMirageBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Mirage message. Status: STABLE / Reported as working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

## decodeMitsubishi()

bool IRrecv::decodeMitsubishi | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kMitsubishiBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Mitsubishi 16-bit message. Status: STABLE / Working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  True if it can decode it, false if it can't.

Note
  This protocol appears to have no header.

See also
  GlobalCache's Control Tower's Mitsubishi TV data.

## decodeMitsubishi112()

bool IRrecv::decodeMitsubishi112 | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kMitsubishi112Bits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Mitsubishi/TCL 112-bit A/C message. (MITSUBISHI112, TCL112AC) Status: STABLE / Reported as working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Note
  Note Mitsubishi112 & Tcl112Ac are basically the same protocol. The only significant difference I can see is Mitsubishi112 has a slightly longer header mark. We will use that to determine which variant it should be. The other differences require full decoding and only only with certain settings. There are some other timing differences too, but the tolerances will overlap.

See also
  https://github.com/crankyoldgit/IRremoteESP8266/issues/619
  https://github.com/crankyoldgit/IRremoteESP8266/issues/947

## decodeMitsubishi136()

bool IRrecv::decodeMitsubishi136 | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kMitsubishi136Bits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Mitsubishi 136-bit A/C message. (MITSUBISHI136) Status: STABLE / Reported as working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

See also
  https://github.com/crankyoldgit/IRremoteESP8266/issues/888

## decodeMitsubishi2()

bool IRrecv::decodeMitsubishi2 | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kMitsubishiBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied second variation of a Mitsubishi 16-bit message. Status: STABLE / Working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  True if it can decode it, false if it can't.

See also
  https://github.com/crankyoldgit/IRremoteESP8266/issues/441

## decodeMitsubishiAC()

bool IRrecv::decodeMitsubishiAC | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kMitsubishiACBits`,
|  | const bool | strict = `false`
| ) |  |

private

Decode the supplied Mitsubish 144-bit A/C message. Status: BETA / Probably works.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

See also
  https://www.analysir.com/blog/2015/01/06/reverse-engineering-mitsubishi-ac-infrared-protocol/

## decodeMitsubishiHeavy()

bool IRrecv::decodeMitsubishiHeavy | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kMitsubishiHeavy152Bits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Mitsubishi Heavy Industries A/C message. Status: BETA / Appears to be working. Needs testing against a real device.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect. Typically kMitsubishiHeavy88Bits or kMitsubishiHeavy152Bits (def).
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  True if it can decode it, false if it can't.

## decodeMultibrackets()

bool IRrecv::decodeMultibrackets | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kMultibracketsBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the Multibrackets message. Status: BETA / Appears to be working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  True if it can decode it, false if it can't.

## decodeMWM()

bool IRrecv::decodeMWM | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `24`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied MWM message. Status: Implemented.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  True if it can decode it, false if it can't.

Note
  This protocol is 2400 bps serial, 1 start bit (mark), 1 stop bit (space), no parity

## decodeNEC()

bool IRrecv::decodeNEC | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kNECBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied NEC (Renesas) message. Status: STABLE / Known good.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  True if it can decode it, false if it can't.

Note
  NEC protocol has three variants/forms. Normal: an 8 bit address & an 8 bit command in 32 bit data form. i.e. address + inverted(address) + command + inverted(command) Extended: a 16 bit address & an 8 bit command in 32 bit data form. i.e. address + command + inverted(command) Repeat: a 0-bit code. i.e. No data bits. Just the header + footer.

See also
  http://www.sbprojects.com/knowledge/ir/nec.php

## decodeNeoclima()

bool IRrecv::decodeNeoclima | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kNeoclimaBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Neoclima message. Status: STABLE / Known working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  True if it can decode it, false if it can't.

## decodeNikai()

bool IRrecv::decodeNikai | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kNikaiBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Nikai message. Status: STABLE / Working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

## decodePanasonic()

bool IRrecv::decodePanasonic | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kPanasonicBits`,
|  | const bool | strict = `false`,
|  | const uint32_t | manufacturer = `kPanasonicManufacturer`
| ) |  |

private

Decode the supplied Panasonic message. Status: STABLE / Should be working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | manufacturer | A 16-bit manufacturer code. e.g. 0x4004 is Panasonic
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  True if it can decode it, false if it can't.

Warning
  Results to be used with `sendPanasonic64()`, not `sendPanasonic()`.

Note
  Panasonic 48-bit protocol is a modified version of Kaseikyo.

See also
  http://www.remotecentral.com/cgi-bin/mboard/rc-pronto/thread.cgi?2615
  http://www.hifi-remote.com/wiki/index.php?title=Panasonic

## decodePanasonicAC()

bool IRrecv::decodePanasonicAC | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kPanasonicAcBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Panasonic AC message. Status: STABLE / Works with real device(s).

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  True if it can decode it, false if it can't.

## decodePanasonicAC32()

bool IRrecv::decodePanasonicAC32 | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kPanasonicAc32Bits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Panasonic AC 32/16bit message. Status: STABLE / Confirmed working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode result.
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect. Typically: kPanasonicAc32Bits or kPanasonicAc32Bits/2
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

See also
  https://github.com/crankyoldgit/IRremoteESP8266/issues/1307

Note
  Protocol has two known configurations: (long) Two sections of identical 32 bit data block pairs. ie. (32+32)+(32+32)=128 or (short) A single section of 3 x identical 32 bit data blocks i.e. (32+32+32)=96 Each data block also has a pair of 8 bits repeated identical bits. e.g. (8+8)+(8+8)=32

So each long version really only has 32 unique bits, and the short version really only has 16 unique bits.

## decodePioneer()

bool IRrecv::decodePioneer | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kPioneerBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Pioneer message. Status: STABLE / Should be working. (Self decodes & real examples)

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  True if it can decode it, false if it can't.

## decodeRC5()

bool IRrecv::decodeRC5 | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kRC5XBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied RC-5/RC5X message. Status: RC-5 (stable), RC-5X (alpha)

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  True if it can decode it, false if it can't.

Note
  The 'toggle' bit is included as the 6th (MSB) address bit, the MSB of data, & in the count of bits decoded.

Todo:
  Serious testing of the RC-5X and strict aspects needs to be done.

## decodeRC6()

bool IRrecv::decodeRC6 | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kRC6Mode0Bits`,
|  | const bool | strict = `false`
| ) |  |

private

Decode the supplied RC6 message. Status: Stable.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  True if it can decode it, false if it can't.

Todo:
  Testing of the strict compliance aspects.

## decodeRCMM()

bool IRrecv::decodeRCMM | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kRCMMBits`,
|  | const bool | strict = `false`
| ) |  |

private

Decode a Philips RC-MM packet (between 12 & 32 bits) if possible. Status: STABLE / Should be working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  True if it can decode it, false if it can't.

## decodeSAMSUNG()

bool IRrecv::decodeSAMSUNG | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kSamsungBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Samsung 32-bit message. Status: STABLE.

Note
  Samsung messages whilst 32 bits in size, only contain 16 bits of distinct data. e.g. In transmition order: customer_byte + customer_byte(same) + address_byte + invert(address_byte)

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  True if it can decode it, false if it can't.

Note
  LG 32bit protocol appears near identical to the Samsung protocol. They differ on their compliance criteria and how they repeat.

See also
  http://elektrolab.wz.cz/katalog/samsung_protocol.pdf

## decodeSamsung36()

bool IRrecv::decodeSamsung36 | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kSamsung36Bits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Samsung36 message. Status: STABLE / Expected to work.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  True if it can decode it, false if it can't.

See also
  https://github.com/crankyoldgit/IRremoteESP8266/issues/621

## decodeSamsungAC()

bool IRrecv::decodeSamsungAC | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kSamsungAcBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Samsung A/C message. Status: Stable / Known to be working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  True if it can decode it, false if it can't.

See also
  https://github.com/crankyoldgit/IRremoteESP8266/issues/505

## decodeSanyoAc()

bool IRrecv::decodeSanyoAc | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kSanyoAcBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied SanyoAc message. Status: STABLE / Reported as working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

See also
  https://github.com/crankyoldgit/IRremoteESP8266/issues/1211

## decodeSanyoLC7461()

bool IRrecv::decodeSanyoLC7461 | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kSanyoLC7461Bits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied SANYO LC7461 message. Status: BETA / Probably works.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  True if it can decode it, false if it can't.

Note
  Based on @marcosamarinho's work. This protocol uses the NEC protocol. However, data is formatted as : address(13 bits), !address, command (8 bits), !command. According with LIRC, this protocol is used on Sanyo, Aiwa and Chinon Information for this protocol is available at the Sanyo LC7461 datasheet.

See also
  http://slydiman.narod.ru/scr/kb/sanyo.htm
  https://github.com/marcosamarinho/IRremoteESP8266/blob/master/ir_Sanyo.cpp
  http://pdf.datasheetcatalog.com/datasheet/sanyo/LC7461.pdf

## decodeSharp()

bool IRrecv::decodeSharp | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kSharpBits`,
|  | const bool | strict = `true`,
|  | const bool | expansion = `true`
| ) |  |

private

Decode the supplied Sharp message. Status: STABLE / Working fine.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.
  [in] | expansion | Should we expect the expansion bit to be set. Default is true.

Returns
  True if it can decode it, false if it can't.

Note
  This procedure returns a value suitable for use in `sendSharpRaw()`.

Todo:
  Need to ensure capture of the inverted message as it can be missed due to the interrupt timeout used to detect an end of message. Several compliance checks are disabled until that is resolved.

## decodeSharpAc()

bool IRrecv::decodeSharpAc | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kSharpAcBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Sharp A/C message. Status: STABLE / Known working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  True if it can decode it, false if it can't.

See also
  https://github.com/crankyoldgit/IRremoteESP8266/issues/638
  https://github.com/ToniA/arduino-heatpumpir/blob/master/SharpHeatpumpIR.cpp

## decodeSony()

bool IRrecv::decodeSony | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kSonyMinBits`,
|  | const bool | strict = `false`
| ) |  |

private

Decode the supplied Sony/SIRC message. Status: STABLE / Should be working. strict mode is ALPHA / Untested.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  True if it can decode it, false if it can't.

Note
  SONY protocol, SIRC (Serial Infra-Red Control) can be 12, 15, or 20 bits long.

## decodeSymphony()

bool IRrecv::decodeSymphony | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kSymphonyBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Symphony packet/message. Status: STABLE / Should be working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  True if it can decode it, false if it can't.

## decodeTechnibelAc()

bool IRrecv::decodeTechnibelAc | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kTechnibelAcBits`,
|  | const bool | strict = `true`
| ) |  |

private

Status: STABLE / Reported as working on a real device.

Parameters

  [in,out] | results | Ptr to data to decode & where to store the decode
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect (kTechnibelAcBits).
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

## decodeTeco()

bool IRrecv::decodeTeco | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kTecoBits`,
|  | const bool | strict = `false`
| ) |  |

private

Decode the supplied Teco message. Status: STABLE / Tested.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  True if it can decode it, false if it can't.

## decodeToshibaAC()

bool IRrecv::decodeToshibaAC | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kToshibaACBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Toshiba A/C message. Status: STABLE / Working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  True if it can decode it, false if it can't.

## decodeTranscold()

bool IRrecv::decodeTranscold | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kTranscoldBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Transcold A/C message. Status: STABLE / Known Working.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode result.
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

## decodeTrotec()

bool IRrecv::decodeTrotec | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kTrotecBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Trotec message. Status: STABLE / Works. Untested on real devices.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  True if it can decode it, false if it can't.

## decodeVestelAc()

bool IRrecv::decodeVestelAc | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kVestelAcBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Vestel message. Status: Alpha / Needs testing against a real device.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  True if it can decode it, false if it can't.

## decodeVoltas()

bool IRrecv::decodeVoltas | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kVoltasBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Voltas message. Status: STABLE / Working on real device.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

## decodeWhirlpoolAC()

bool IRrecv::decodeWhirlpoolAC | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kWhirlpoolAcBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Whirlpool A/C message. Status: STABLE / Working as intended.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  True if it can decode it, false if it can't.

## decodeWhynter()

bool IRrecv::decodeWhynter | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kWhynterBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Whynter message. Status: STABLE / Working. Strict mode is ALPHA.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the result
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  True if it can decode it, false if it can't.

See also
  https://github.com/z3t0/Arduino-IRremote/blob/master/ir_Whynter.cpp

## decodeZepeal()

bool IRrecv::decodeZepeal | ( | decode_results * | results,
|  | uint16_t | offset = `kStartOffset`,
|  | const uint16_t | nbits = `kZepealBits`,
|  | const bool | strict = `true`
| ) |  |

private

Decode the supplied Zepeal message. Status: STABLE / Works on real device.

Parameters

  [in,out] | results | Ptr to the data to decode & where to store the decode result.
  [in] | offset | The starting index to use when attempting to decode the raw data. Typically/Defaults to kStartOffset.
  [in] | nbits | The number of data bits to expect. Typically kZepealBits.
  [in] | strict | Flag indicating if we should perform strict matching.

Returns
  A boolean. True if it can decode it, false if it can't.

## disableIRIn()

void IRrecv::disableIRIn | ( | void |  | ) |

Stop collection of any received IR data. Disable any timers and interrupts.

## enableIRIn()

void IRrecv::enableIRIn | ( | const bool | pullup = `false` | ) |

Set up and (re)start the IR capture mechanism.

Parameters

  [in] | pullup | A flag indicating should the GPIO use the internal pullup resistor. (Default: `false`. i.e. No.)

## getBufSize()

uint16_t IRrecv::getBufSize | ( | void |  | ) |

Obtain the maximum number of entries possible in the capture buffer. i.e. It's size.

Returns
  The size of the buffer that is in use by the object.

## getRClevel()

int16_t IRrecv::getRClevel | ( | decode_results * | results,
|  | uint16_t * | offset,
|  | uint16_t * | used,
|  | uint16_t | bitTime,
|  | const uint8_t | tolerance = `kUseDefTol`,
|  | const int16_t | excess = `kMarkExcess`,
|  | const uint16_t | delta = `0`,
|  | const uint8_t | maxwidth = `3`
| ) |  |

private

Gets one undecoded level at a time from the raw buffer. The RC5/6 decoding is easier if the data is broken into time intervals. E.g. if the buffer has MARK for 2 time intervals and SPACE for 1, successive calls to getRClevel will return MARK, MARK, SPACE. offset and used are updated to keep track of the current position.

Parameters

  [in,out] | results | Ptr to the data to decode and where to store the decode result.
  [in,out] | offset | Ptr to the currect offset to the rawbuf.
  [in,out] | used | Ptr to the current used counter.
  [in] | bitTime | Time interval of single bit in microseconds.
  [in] | tolerance | Percent tolerance to be used in matching.
  [in] | excess | Extra useconds to add to Marks & removed from Spaces.
  [in] | delta | A non-scaling (+/-) error margin (in useconds).
  [in] | maxwidth | Maximum number of successive levels to find in a single level (default is 3)

Returns
  MARK, SPACE, or -1 for error. (The measured time interval is not a multiple of t1.)

See also
  https://en.wikipedia.org/wiki/Manchester_code

## getTolerance()

uint8_t IRrecv::getTolerance | ( | void |  | ) |

Get the base tolerance percentage for matching incoming IR messages.

Returns
  A integer percentage.

## match()

bool IRrecv::match | ( | const uint32_t | measured,
|  | const uint32_t | desired,
|  | const uint8_t | tolerance = `kUseDefTol`,
|  | const uint16_t | delta = `0`
| ) |  |

Check if we match a pulse(measured) with the desired within +/-tolerance percent and/or +/- a fixed delta range.

Parameters

  [in] | measured | The recorded period of the signal pulse.
  [in] | desired | The expected period (in usecs) we are matching against.
  [in] | tolerance | A percentage expressed as an integer. e.g. 10 is 10%.
  [in] | delta | A non-scaling (+/-) error margin (in useconds).

Returns
  A Boolean. true if it matches, false if it doesn't.

## matchAtLeast()

bool IRrecv::matchAtLeast | ( | const uint32_t | measured,
|  | const uint32_t | desired,
|  | const uint8_t | tolerance = `kUseDefTol`,
|  | const uint16_t | delta = `0`
| ) |  |

private

Check if we match a pulse(measured) of at least desired within tolerance percent and/or a fixed delta margin.

Parameters

  [in] | measured | The recorded period of the signal pulse.
  [in] | desired | The expected period (in usecs) we are matching against.
  [in] | tolerance | A percentage expressed as an integer. e.g. 10 is 10%.
  [in] | delta | A non-scaling amount to reduce usecs by.

Returns
  A Boolean. true if it matches, false if it doesn't.

## matchBytes()

uint16_t IRrecv::matchBytes | ( | volatile uint16_t * | data_ptr,
|  | uint8_t * | result_ptr,
|  | const uint16_t | remaining,
|  | const uint16_t | nbytes,
|  | const uint16_t | onemark,
|  | const uint32_t | onespace,
|  | const uint16_t | zeromark,
|  | const uint32_t | zerospace,
|  | const uint8_t | tolerance = `kUseDefTol`,
|  | const int16_t | excess = `kMarkExcess`,
|  | const bool | MSBfirst = `true`
| ) |  |

private

Match & decode the typical data section of an IR message. The bytes are stored at result_ptr. The first byte in the result equates to the first byte encountered, and so on.

Parameters

  [in] | data_ptr | A pointer to where we are at in the capture buffer.
  [out] | result_ptr | A ptr to where to start storing the bytes we decoded.
  [in] | remaining | The size of the capture buffer remaining.
  [in] | nbytes | Nr. of data bytes we expect.
  [in] | onemark | Nr. of uSeconds in an expected mark signal for a '1' bit.
  [in] | onespace | Nr. of uSecs in an expected space signal for a '1' bit.
  [in] | zeromark | Nr. of uSecs in an expected mark signal for a '0' bit.
  [in] | zerospace | Nr. of uSecs in an expected space signal for a '0' bit.
  [in] | tolerance | Percentage error margin to allow. (Default: kUseDefTol)
  [in] | excess | Nr. of uSeconds. (Def: kMarkExcess)
  [in] | MSBfirst | Bit order to save the data in. (Def: true) true is Most Significant Bit First Order, false is Least Significant First

Returns
  If successful, how many buffer entries were used. Otherwise 0.

## matchData()

match_result_t IRrecv::matchData | ( | volatile uint16_t * | data_ptr,
|  | const uint16_t | nbits,
|  | const uint16_t | onemark,
|  | const uint32_t | onespace,
|  | const uint16_t | zeromark,
|  | const uint32_t | zerospace,
|  | const uint8_t | tolerance = `kUseDefTol`,
|  | const int16_t | excess = `kMarkExcess`,
|  | const bool | MSBfirst = `true`
| ) |  |

private

Match & decode the typical data section of an IR message. The data value is stored in the least significant bits reguardless of the bit ordering requested.

Parameters

  [in] | data_ptr | A pointer to where we are at in the capture buffer.
  [in] | nbits | Nr. of data bits we expect.
  [in] | onemark | Nr. of uSeconds in an expected mark signal for a '1' bit.
  [in] | onespace | Nr. of uSecs in an expected space signal for a '1' bit.
  [in] | zeromark | Nr. of uSecs in an expected mark signal for a '0' bit.
  [in] | zerospace | Nr. of uSecs in an expected space signal for a '0' bit.
  [in] | tolerance | Percentage error margin to allow. (Default: kUseDefTol)
  [in] | excess | Nr. of uSeconds. (Def: kMarkExcess)
  [in] | MSBfirst | Bit order to save the data in. (Def: true) true is Most Significant Bit First Order, false is Least Significant First

Returns
  A match_result_t structure containing the success (or not), the data value, and how many buffer entries were used.

## matchGeneric() [1/2]

uint16_t IRrecv::matchGeneric | ( | volatile uint16_t * | data_ptr,
|  | uint64_t * | result_ptr,
|  | const uint16_t | remaining,
|  | const uint16_t | nbits,
|  | const uint16_t | hdrmark,
|  | const uint32_t | hdrspace,
|  | const uint16_t | onemark,
|  | const uint32_t | onespace,
|  | const uint16_t | zeromark,
|  | const uint32_t | zerospace,
|  | const uint16_t | footermark,
|  | const uint32_t | footerspace,
|  | const bool | atleast = `false`,
|  | const uint8_t | tolerance = `kUseDefTol`,
|  | const int16_t | excess = `kMarkExcess`,
|  | const bool | MSBfirst = `true`
| ) |  |

private

Match & decode a generic/typical <= 64bit IR message. The data is stored at result_ptr.

Note
  Values of 0 for hdrmark, hdrspace, footermark, or footerspace mean skip that requirement.

Parameters

  [in] | data_ptr | A pointer to where we are at in the capture buffer.
  [out] | result_ptr | A ptr to where to start storing the bits we decoded.
  [in] | remaining | The size of the capture buffer remaining.
  [in] | nbits | Nr. of data bits we expect.
  [in] | hdrmark | Nr. of uSeconds for the expected header mark signal.
  [in] | hdrspace | Nr. of uSeconds for the expected header space signal.
  [in] | onemark | Nr. of uSeconds in an expected mark signal for a '1' bit.
  [in] | onespace | Nr. of uSecs in an expected space signal for a '1' bit.
  [in] | zeromark | Nr. of uSecs in an expected mark signal for a '0' bit.
  [in] | zerospace | Nr. of uSecs in an expected space signal for a '0' bit.
  [in] | footermark | Nr. of uSeconds for the expected footer mark signal.
  [in] | footerspace | Nr. of uSeconds for the expected footer space/gap signal.
  [in] | atleast | Is the match on the footerspace a matchAtLeast or matchSpace?
  [in] | tolerance | Percentage error margin to allow. (Default: kUseDefTol)
  [in] | excess | Nr. of uSeconds. (Def: kMarkExcess)
  [in] | MSBfirst | Bit order to save the data in. (Def: true) true is Most Significant Bit First Order, false is Least Significant First

Returns
  If successful, how many buffer entries were used. Otherwise 0.

## matchGeneric() [2/2]

uint16_t IRrecv::matchGeneric | ( | volatile uint16_t * | data_ptr,
|  | uint8_t * | result_ptr,
|  | const uint16_t | remaining,
|  | const uint16_t | nbits,
|  | const uint16_t | hdrmark,
|  | const uint32_t | hdrspace,
|  | const uint16_t | onemark,
|  | const uint32_t | onespace,
|  | const uint16_t | zeromark,
|  | const uint32_t | zerospace,
|  | const uint16_t | footermark,
|  | const uint32_t | footerspace,
|  | const bool | atleast = `false`,
|  | const uint8_t | tolerance = `kUseDefTol`,
|  | const int16_t | excess = `kMarkExcess`,
|  | const bool | MSBfirst = `true`
| ) |  |

private

Match & decode a generic/typical > 64bit IR message. The bytes are stored at result_ptr. The first byte in the result equates to the first byte encountered, and so on.

Note
  Values of 0 for hdrmark, hdrspace, footermark, or footerspace mean skip that requirement.

Parameters

  [in] | data_ptr | A pointer to where we are at in the capture buffer.
  [out] | result_ptr | A ptr to where to start storing the bytes we decoded.
  [in] | remaining | The size of the capture buffer remaining.
  [in] | nbits | Nr. of data bits we expect.
  [in] | hdrmark | Nr. of uSeconds for the expected header mark signal.
  [in] | hdrspace | Nr. of uSeconds for the expected header space signal.
  [in] | onemark | Nr. of uSeconds in an expected mark signal for a '1' bit.
  [in] | onespace | Nr. of uSecs in an expected space signal for a '1' bit.
  [in] | zeromark | Nr. of uSecs in an expected mark signal for a '0' bit.
  [in] | zerospace | Nr. of uSecs in an expected space signal for a '0' bit.
  [in] | footermark | Nr. of uSeconds for the expected footer mark signal.
  [in] | footerspace | Nr. of uSeconds for the expected footer space/gap signal.
  [in] | atleast | Is the match on the footerspace a matchAtLeast or matchSpace?
  [in] | tolerance | Percentage error margin to allow. (Default: kUseDefTol)
  [in] | excess | Nr. of uSeconds. (Def: kMarkExcess)
  [in] | MSBfirst | Bit order to save the data in. (Def: true) true is Most Significant Bit First Order, false is Least Significant First

Returns
  If successful, how many buffer entries were used. Otherwise 0.

## matchGenericConstBitTime()

uint16_t IRrecv::matchGenericConstBitTime | ( | volatile uint16_t * | data_ptr,
|  | uint64_t * | result_ptr,
|  | const uint16_t | remaining,
|  | const uint16_t | nbits,
|  | const uint16_t | hdrmark,
|  | const uint32_t | hdrspace,
|  | const uint16_t | one,
|  | const uint32_t | zero,
|  | const uint16_t | footermark,
|  | const uint32_t | footerspace,
|  | const bool | atleast = `false`,
|  | const uint8_t | tolerance = `kUseDefTol`,
|  | const int16_t | excess = `kMarkExcess`,
|  | const bool | MSBfirst = `true`
| ) |  |

private

Match & decode a generic/typical constant bit time <= 64bit IR message. The data is stored at result_ptr.

Note
  Values of 0 for hdrmark, hdrspace, footermark, or footerspace mean skip that requirement.

Parameters

  [in] | data_ptr | A pointer to where we are at in the capture buffer.

Note
  `data_ptr` is assumed to be pointing to a "Mark", not a "Space".

Parameters

  [out] | result_ptr | A ptr to where to start storing the bits we decoded.
  [in] | remaining | The size of the capture buffer remaining.
  [in] | nbits | Nr. of data bits we expect.
  [in] | hdrmark | Nr. of uSeconds for the expected header mark signal.
  [in] | hdrspace | Nr. of uSeconds for the expected header space signal.
  [in] | one | Nr. of uSeconds in an expected mark signal for a '1' bit.
  [in] | zero | Nr. of uSeconds in an expected mark signal for a '0' bit.
  [in] | footermark | Nr. of uSeconds for the expected footer mark signal.
  [in] | footerspace | Nr. of uSeconds for the expected footer space/gap signal.
  [in] | atleast | Is the match on the footerspace a matchAtLeast or matchSpace?
  [in] | tolerance | Percentage error margin to allow. (Default: kUseDefTol)
  [in] | excess | Nr. of uSeconds. (Def: kMarkExcess)
  [in] | MSBfirst | Bit order to save the data in. (Def: true) true is Most Significant Bit First Order, false is Least Significant First

Returns
  If successful, how many buffer entries were used. Otherwise 0.

Note
  Parameters one + zero add up to the total time for a bit. e.g. mark(one) + space(zero) is a `1`, mark(zero) + space(one) is a `0`.

## matchManchester()

uint16_t IRrecv::matchManchester | ( | volatile const uint16_t * | data_ptr,
|  | uint64_t * | result_ptr,
|  | const uint16_t | remaining,
|  | const uint16_t | nbits,
|  | const uint16_t | hdrmark,
|  | const uint32_t | hdrspace,
|  | const uint16_t | half_period,
|  | const uint16_t | footermark,
|  | const uint32_t | footerspace,
|  | const bool | atleast = `false`,
|  | const uint8_t | tolerance = `kUseDefTol`,
|  | const int16_t | excess = `kMarkExcess`,
|  | const bool | MSBfirst = `true`,
|  | const bool | GEThomas = `true`
| ) |  |

private

Match & decode a Manchester Code <= 64bit IR message. The data is stored at result_ptr.

Note
  Values of 0 for hdrmark, hdrspace, footermark, or footerspace mean skip that requirement.

Parameters

  [in] | data_ptr | A pointer to where we are at in the capture buffer.

Note
  `data_ptr` is assumed to be pointing to a "Mark", not a "Space".

Parameters

  [out] | result_ptr | A ptr to where to start storing the bits we decoded.
  [in] | remaining | The size of the capture buffer remaining.
  [in] | nbits | Nr. of data bits we expect.
  [in] | hdrmark | Nr. of uSeconds for the expected header mark signal.
  [in] | hdrspace | Nr. of uSeconds for the expected header space signal.
  [in] | half_period | Nr. of uSeconds for half the clock's period. i.e. 1/2 wavelength
  [in] | footermark | Nr. of uSeconds for the expected footer mark signal.
  [in] | footerspace | Nr. of uSeconds for the expected footer space/gap signal.
  [in] | atleast | Is the match on the footerspace a matchAtLeast or matchSpace?
  [in] | tolerance | Percentage error margin to allow. (Default: kUseDefTol)
  [in] | excess | Nr. of uSeconds. (Def: kMarkExcess)
  [in] | MSBfirst | Bit order to save the data in. (Def: true) true is Most Significant Bit First Order, false is Least Significant First
  [in] | GEThomas | Use G.E. Thomas (true) or IEEE 802.3 (false) convention?

Returns
  If successful, how many buffer entries were used. Otherwise 0.

See also
  https://en.wikipedia.org/wiki/Manchester_code
  http://ww1.microchip.com/downloads/en/AppNotes/Atmel-9164-Manchester-Coding-Basics_Application-Note.pdf

## matchManchesterData()

uint16_t IRrecv::matchManchesterData | ( | volatile const uint16_t * | data_ptr,
|  | uint64_t * | result_ptr,
|  | const uint16_t | remaining,
|  | const uint16_t | nbits,
|  | const uint16_t | half_period,
|  | const uint16_t | starting_balance = `0`,
|  | const uint8_t | tolerance = `kUseDefTol`,
|  | const int16_t | excess = `kMarkExcess`,
|  | const bool | MSBfirst = `true`,
|  | const bool | GEThomas = `true`
| ) |  |

private

Match & decode a Manchester Code data (<= 64bits.

Parameters

  [in] | data_ptr | A pointer to where we are at in the capture buffer.

Note
  `data_ptr` is assumed to be pointing to a "Mark", not a "Space".

Parameters

  [out] | result_ptr | A ptr to where to start storing the bits we decoded.
  [in] | remaining | The size of the capture buffer remaining.
  [in] | nbits | Nr. of data bits we expect.
  [in] | half_period | Nr. of uSeconds for half the clock's period. i.e. 1/2 wavelength
  [in] | tolerance | Percentage error margin to allow. (Default: kUseDefTol)
  [in] | starting_balance | Amount of uSeconds to assume exists prior to the current value pointed too.
  [in] | excess | Nr. of uSeconds. (Def: kMarkExcess)
  [in] | MSBfirst | Bit order to save the data in. (Def: true) true is Most Significant Bit First Order, false is Least Significant First
  [in] | GEThomas | Use G.E. Thomas (true) or IEEE 802.3 (false) convention?

Returns
  If successful, how many buffer entries were used. Otherwise 0.

See also
  https://en.wikipedia.org/wiki/Manchester_code
  http://ww1.microchip.com/downloads/en/AppNotes/Atmel-9164-Manchester-Coding-Basics_Application-Note.pdf

Todo:
  Clean up and optimise this. It is just "get it working code" atm.

## matchMark()

bool IRrecv::matchMark | ( | const uint32_t | measured,
|  | const uint32_t | desired,
|  | const uint8_t | tolerance = `kUseDefTol`,
|  | const int16_t | excess = `kMarkExcess`
| ) |  |

Check if we match a mark signal(measured) with the desired within +/-tolerance percent, after an expected is excess is added.

Parameters

  [in] | measured | The recorded period of the signal pulse.
  [in] | desired | The expected period (in usecs) we are matching against.
  [in] | tolerance | A percentage expressed as an integer. e.g. 10 is 10%.
  [in] | excess | A non-scaling amount to reduce usecs by.

Returns
  A Boolean. true if it matches, false if it doesn't.

## matchSpace()

bool IRrecv::matchSpace | ( | const uint32_t | measured,
|  | const uint32_t | desired,
|  | const uint8_t | tolerance = `kUseDefTol`,
|  | const int16_t | excess = `kMarkExcess`
| ) |  |

Check if we match a space signal(measured) with the desired within +/-tolerance percent, after an expected is excess is removed.

Parameters

  [in] | measured | The recorded period of the signal pulse.
  [in] | desired | The expected period (in usecs) we are matching against.
  [in] | tolerance | A percentage expressed as an integer. e.g. 10 is 10%.
  [in] | excess | A non-scaling amount to reduce usecs by.

Returns
  A Boolean. true if it matches, false if it doesn't.

## resume()

void IRrecv::resume | ( | void |  | ) |

Resume collection of received IR data.

Note
  This is required if `decode()` is successful and `save_buffer` was not set when the class was instanciated.

See also
  IRrecv class constructor

## setTolerance()

void IRrecv::setTolerance | ( | const uint8_t | percent = `kTolerance` | ) |

Set the base tolerance percentage for matching incoming IR messages.

Parameters

  [in] | percent | An integer percentage. (0-100)

## setUnknownThreshold()

void IRrecv::setUnknownThreshold | ( | const uint16_t | length | ) |

Set the minimum length we will consider for reporting UNKNOWN message types.

Parameters

  [in] | length | Min nr. of mark/space pulses required to be considered.

## ticksHigh()

uint32_t IRrecv::ticksHigh | ( | const uint32_t | usecs,
|  | const uint8_t | tolerance = `kUseDefTol`,
|  | const uint16_t | delta = `0`
| ) |  |

private

Calculate the upper bound of the nr. of ticks.

Parameters

  [in] | usecs | Nr. of uSeconds.
  [in] | tolerance | Percent as an integer. e.g. 10 is 10%
  [in] | delta | A non-scaling amount to increase usecs by.

Returns
  Nr. of ticks.

## ticksLow()

uint32_t IRrecv::ticksLow | ( | const uint32_t | usecs,
|  | const uint8_t | tolerance = `kUseDefTol`,
|  | const uint16_t | delta = `0`
| ) |  |

private

Calculate the lower bound of the nr. of ticks.

Parameters

  [in] | usecs | Nr. of uSeconds.
  [in] | tolerance | Percent as an integer. e.g. 10 is 10%
  [in] | delta | A non-scaling amount to reduce usecs by.

Returns
  Nr. of ticks.

## Member Data Documentation

## _timer_num

uint8_t IRrecv::_timer_num

private

## _tolerance

uint8_t IRrecv::_tolerance

private

## _unknown_threshold

uint16_t IRrecv::_unknown_threshold

private

## irparams_save

irparams_t* IRrecv::irparams_save

private

The documentation for this class was generated from the following files:

- src/IRrecv.h
- src/ir_Airwell.cpp
- src/ir_Aiwa.cpp
- src/ir_Amcor.cpp
- src/ir_Argo.cpp
- src/ir_Carrier.cpp
- src/ir_Coolix.cpp
- src/ir_Corona.cpp
- src/ir_Daikin.cpp
- src/ir_Delonghi.cpp
- src/ir_Denon.cpp
- src/ir_Dish.cpp
- src/ir_Doshisha.cpp
- src/ir_Electra.cpp
- src/ir_EliteScreens.cpp
- src/ir_Epson.cpp
- src/ir_Fujitsu.cpp
- src/ir_GICable.cpp
- src/ir_Goodweather.cpp
- src/ir_Gree.cpp
- src/ir_Haier.cpp
- src/ir_Hitachi.cpp
- src/ir_Inax.cpp
- src/ir_JVC.cpp
- src/ir_Kelvinator.cpp
- src/ir_Lasertag.cpp
- src/ir_Lego.cpp
- src/ir_LG.cpp
- src/ir_Lutron.cpp
- src/ir_Magiquest.cpp
- src/ir_Metz.cpp
- src/ir_Midea.cpp
- src/ir_Mirage.cpp
- src/ir_Mitsubishi.cpp
- src/ir_MitsubishiHeavy.cpp
- src/ir_Multibrackets.cpp
- src/ir_MWM.cpp
- src/ir_NEC.cpp
- src/ir_Neoclima.cpp
- src/ir_Nikai.cpp
- src/ir_Panasonic.cpp
- src/ir_Pioneer.cpp
- src/ir_RC5_RC6.cpp
- src/ir_RCMM.cpp
- src/ir_Samsung.cpp
- src/ir_Sanyo.cpp
- src/ir_Sharp.cpp
- src/ir_Sony.cpp
- src/ir_Symphony.cpp
- src/ir_Technibel.cpp
- src/ir_Teco.cpp
- src/ir_Toshiba.cpp
- src/ir_Transcold.cpp
- src/ir_Trotec.cpp
- src/ir_Vestel.cpp
- src/ir_Voltas.cpp
- src/ir_Whirlpool.cpp
- src/ir_Whynter.cpp
- src/ir_Zepeal.cpp
- src/IRrecv.cpp