# IRremoteESP8266: Member List

IRTechnibelAc Member List

This is the complete list of members for IRTechnibelAc, including all inherited members.

_irsend | IRTechnibelAc | private
_irsend | IRTechnibelAc | private
_saved_temp | IRTechnibelAc | private
_saved_temp_units | IRTechnibelAc | private
begin() | IRTechnibelAc |
calcChecksum(const uint64_t state) | IRTechnibelAc | static
calibrate(void) | IRTechnibelAc | inline
checksum(void) | IRTechnibelAc | private
convertFan(const stdAc::fanspeed_t speed) | IRTechnibelAc |
convertMode(const stdAc::opmode_t mode) | IRTechnibelAc |
convertSwing(const stdAc::swingv_t swing) | IRTechnibelAc |
getFan() | IRTechnibelAc |
getMode() | IRTechnibelAc |
getPower() | IRTechnibelAc |
getRaw() | IRTechnibelAc |
getSleep() | IRTechnibelAc |
getSwing() | IRTechnibelAc |
getTemp() | IRTechnibelAc |
getTempUnit(void) | IRTechnibelAc |
getTimer(void) | IRTechnibelAc |
getTimerEnabled(void) | IRTechnibelAc |
IRTechnibelAc(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRTechnibelAc | explicit
off() | IRTechnibelAc |
on() | IRTechnibelAc |
remote_state | IRTechnibelAc | private
send(const uint16_t repeat=kTechnibelAcDefaultRepeat) | IRTechnibelAc |
setFan(const uint8_t speed) | IRTechnibelAc |
setMode(const uint8_t mode) | IRTechnibelAc |
setPower(const bool on) | IRTechnibelAc |
setRaw(const uint64_t state) | IRTechnibelAc |
setSleep(const bool on) | IRTechnibelAc |
setSwing(const bool on) | IRTechnibelAc |
setTemp(const uint8_t temp, const bool fahrenheit=false) | IRTechnibelAc |
setTempUnit(const bool celsius) | IRTechnibelAc |
setTimer(const uint16_t nr_of_mins) | IRTechnibelAc |
setTimerEnabled(const bool on) | IRTechnibelAc |
stateReset() | IRTechnibelAc |
toCommon(void) | IRTechnibelAc |
toCommonFanSpeed(const uint8_t speed) | IRTechnibelAc | static
toCommonMode(const uint8_t mode) | IRTechnibelAc | static
toCommonSwing(const bool swing) | IRTechnibelAc |
toString() | IRTechnibelAc |
validChecksum(const uint64_t state) | IRTechnibelAc | static