# IRremoteESP8266: src/IRtimer.h Source File

IRtimer.h
Go to the documentation of this file.
// Copyright 2017 David Conran
#ifndef IRTIMER_H_
#define IRTIMER_H_
#define __STDC_LIMIT_MACROS
#include <stdint.h>
// Classes
class IRtimer {
public:
IRtimer();
void reset();
uint32_t elapsed();
#ifdef UNIT_TEST
static void add(uint32_t usecs);
#endif // UNIT_TEST
private:
uint32_t start;
};
class TimerMs {
public:
TimerMs();
void reset();
uint32_t elapsed();
#ifdef UNIT_TEST
static void add(uint32_t msecs);
#endif // UNIT_TEST
private:
uint32_t start;
};
#endif // IRTIMER_H_
TimerMs::start
uint32_t start
Time in mSeconds when the class was instantiated/reset.
Definition: IRtimer.h:38
IRtimer
This class offers a simple counter in micro-seconds since instantiated.
Definition: IRtimer.h:13
IRtimer::add
static void add(uint32_t usecs)
Add time to the timer to simulate elapsed time.
Definition: IRtimer.cpp:44
IRtimer::reset
void reset()
Resets the IRtimer object. I.e. The counter starts again from now.
Definition: IRtimer.cpp:18
IRtimer::IRtimer
IRtimer()
Class constructor.
Definition: IRtimer.cpp:15
IRtimer::elapsed
uint32_t elapsed()
Calculate how many microseconds have elapsed since the timer was started.
Definition: IRtimer.cpp:28
TimerMs::elapsed
uint32_t elapsed()
Calculate how many milliseconds have elapsed since the timer was started.
Definition: IRtimer.cpp:61
TimerMs::reset
void reset()
Resets the TimerMs object. I.e. The counter starts again from now.
Definition: IRtimer.cpp:51
TimerMs::TimerMs
TimerMs()
Class constructor.
Definition: IRtimer.cpp:48
IRtimer::start
uint32_t start
Time in uSeconds when the class was instantiated/reset.
Definition: IRtimer.h:23
TimerMs::add
static void add(uint32_t msecs)
Add time to the timer to simulate elapsed time.
Definition: IRtimer.cpp:77
TimerMs
This class offers a simple counter in milli-seconds since instantiated.
Definition: IRtimer.h:28