# IRremoteESP8266: HaierProtocol Union Reference

HaierProtocol Union Reference

Native representation of a Haier HSU07-HEA03 A/C message. More...

`#include <ir_Haier.h>`

## Public Attributes

uint8_t | remote_state [kHaierACStateLength]
| < The state in native IR code form More...
struct {
uint8_t Prefix
uint8_t Command:4
uint8_t Temp:4
uint8_t CurrHours:5
uint8_t unknown:1
uint8_t Swing:2
uint8_t CurrMins:6
uint8_t OffTimer:1
uint8_t OnTimer:1
uint8_t OffHours:5
uint8_t Health:1
uint8_t __pad0__:0
uint8_t OffMins:6
uint8_t Fan:2
uint8_t OnHours:5
uint8_t Mode:3
uint8_t OnMins:6
uint8_t Sleep:1
uint8_t __pad1__:0
uint8_t Sum
}; |

## Detailed Description

Native representation of a Haier HSU07-HEA03 A/C message.

## Member Data Documentation

## @39

struct { ... }

## __pad0__

uint8_t HaierProtocol::__pad0__

## __pad1__

uint8_t HaierProtocol::__pad1__

## Command

uint8_t HaierProtocol::Command

## CurrHours

uint8_t HaierProtocol::CurrHours

## CurrMins

uint8_t HaierProtocol::CurrMins

## Fan

uint8_t HaierProtocol::Fan

## Health

uint8_t HaierProtocol::Health

## Mode

uint8_t HaierProtocol::Mode

## OffHours

uint8_t HaierProtocol::OffHours

## OffMins

uint8_t HaierProtocol::OffMins

## OffTimer

uint8_t HaierProtocol::OffTimer

## OnHours

uint8_t HaierProtocol::OnHours

## OnMins

uint8_t HaierProtocol::OnMins

## OnTimer

uint8_t HaierProtocol::OnTimer

## Prefix

uint8_t HaierProtocol::Prefix

## remote_state

uint8_t HaierProtocol::remote_state[kHaierACStateLength]

< The state in native IR code form

## Sleep

uint8_t HaierProtocol::Sleep

## Sum

uint8_t HaierProtocol::Sum

## Swing

uint8_t HaierProtocol::Swing

## Temp

uint8_t HaierProtocol::Temp

## unknown

uint8_t HaierProtocol::unknown

The documentation for this union was generated from the following file:

- src/ir_Haier.h