# IRremoteESP8266: Daikin128Protocol Union Reference

Daikin128Protocol Union Reference

Native representation of a Daikin128 A/C message. More...

`#include <ir_Daikin.h>`

## Public Attributes

uint8_t | raw [kDaikin128StateLength]
| The state of the IR remote. More...
struct {
uint8_t __pad0__:8
uint8_t Mode:4
uint8_t Fan:4
uint8_t ClockMins:8
uint8_t ClockHours:8
uint8_t OnHours:6
uint8_t OnHalfHour:1
uint8_t OnTimer:1
uint8_t OffHours:6
uint8_t OffHalfHour:1
uint8_t OffTimer:1
uint8_t Temp:8
uint8_t SwingV:1
uint8_t Sleep:1
uint8_t __pad1__:1
uint8_t Power:1
uint8_t Sum1:4
uint8_t __pad2__:8
uint8_t Ceiling:1
uint8_t __pad3__:1
uint8_t Econo:1
uint8_t Wall:1
uint8_t __pad4__:4
uint8_t pad [5]
uint8_t Sum2:8
}; |

## Detailed Description

Native representation of a Daikin128 A/C message.

## Member Data Documentation

## @25

struct { ... }

## __pad0__

uint8_t Daikin128Protocol::__pad0__

## __pad1__

uint8_t Daikin128Protocol::__pad1__

## __pad2__

uint8_t Daikin128Protocol::__pad2__

## __pad3__

uint8_t Daikin128Protocol::__pad3__

## __pad4__

uint8_t Daikin128Protocol::__pad4__

## Ceiling

uint8_t Daikin128Protocol::Ceiling

## ClockHours

uint8_t Daikin128Protocol::ClockHours

## ClockMins

uint8_t Daikin128Protocol::ClockMins

## Econo

uint8_t Daikin128Protocol::Econo

## Fan

uint8_t Daikin128Protocol::Fan

## Mode

uint8_t Daikin128Protocol::Mode

## OffHalfHour

uint8_t Daikin128Protocol::OffHalfHour

## OffHours

uint8_t Daikin128Protocol::OffHours

## OffTimer

uint8_t Daikin128Protocol::OffTimer

## OnHalfHour

uint8_t Daikin128Protocol::OnHalfHour

## OnHours

uint8_t Daikin128Protocol::OnHours

## OnTimer

uint8_t Daikin128Protocol::OnTimer

## pad

uint8_t Daikin128Protocol::pad[5]

## Power

uint8_t Daikin128Protocol::Power

## raw

uint8_t Daikin128Protocol::raw[kDaikin128StateLength]

The state of the IR remote.

## Sleep

uint8_t Daikin128Protocol::Sleep

## Sum1

uint8_t Daikin128Protocol::Sum1

## Sum2

uint8_t Daikin128Protocol::Sum2

## SwingV

uint8_t Daikin128Protocol::SwingV

## Temp

uint8_t Daikin128Protocol::Temp

## Wall

uint8_t Daikin128Protocol::Wall

The documentation for this union was generated from the following file:

- src/ir_Daikin.h