# IRremoteESP8266: Daikin64Protocol Union Reference

Daikin64Protocol Union Reference

Native representation of a Daikin64 A/C message. More...

`#include <ir_Daikin.h>`

## Public Attributes

uint64_t | raw
| The state of the IR remote. More...
struct {
uint8_t __pad0__:8
uint8_t Mode:4
uint8_t Fan:4
uint8_t ClockMins:8
uint8_t ClockHours:8
uint8_t OnHours:6
uint8_t OnHalfHour:1
uint8_t OnTimer:1
uint8_t OffHours:6
uint8_t OffHalfHour:1
uint8_t OffTimer:1
uint8_t Temp:8
uint8_t SwingV:1
uint8_t Sleep:1
uint8_t __pad1__:1
uint8_t Power:1
uint8_t Sum:4
}; |

## Detailed Description

Native representation of a Daikin64 A/C message.

## Member Data Documentation

## @29

struct { ... }

## __pad0__

uint8_t Daikin64Protocol::__pad0__

## __pad1__

uint8_t Daikin64Protocol::__pad1__

## ClockHours

uint8_t Daikin64Protocol::ClockHours

## ClockMins

uint8_t Daikin64Protocol::ClockMins

## Fan

uint8_t Daikin64Protocol::Fan

## Mode

uint8_t Daikin64Protocol::Mode

## OffHalfHour

uint8_t Daikin64Protocol::OffHalfHour

## OffHours

uint8_t Daikin64Protocol::OffHours

## OffTimer

uint8_t Daikin64Protocol::OffTimer

## OnHalfHour

uint8_t Daikin64Protocol::OnHalfHour

## OnHours

uint8_t Daikin64Protocol::OnHours

## OnTimer

uint8_t Daikin64Protocol::OnTimer

## Power

uint8_t Daikin64Protocol::Power

## raw

uint64_t Daikin64Protocol::raw

The state of the IR remote.

## Sleep

uint8_t Daikin64Protocol::Sleep

## Sum

uint8_t Daikin64Protocol::Sum

## SwingV

uint8_t Daikin64Protocol::SwingV

## Temp

uint8_t Daikin64Protocol::Temp

The documentation for this union was generated from the following file:

- src/ir_Daikin.h